(export (version D)
  (design
    (source /home/user/ref/ads_frontend/cable_breakout/cable_breakout.sch)
    (date "Sun Jul  1 13:42:33 2018")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source cable_breakout.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value "Bergstak 20P female 3.7mm")
      (footprint footprints:bergstak_plug_2x20_male)
      (datasheet https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10144517.pdf)
      (fields
        (field (name "Mfg PN") 10144517-041802LF)
        (field (name Mfg) Amphenol)
        (field (name "Digikey PN") 609-5429-1-ND)
        (field (name "Digikey URL") https://www.digikey.com/product-detail/en/amphenol-fci/10144517-041802LF/609-5429-1-ND/8573002)
        (field (name Mating) "Amphenol 10144518-042802LF"))
      (libsource (lib conn) (part Conn_02x20_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B3484F9))
    (comp (ref J3)
      (value Conn_02x20_Odd_Even)
      (footprint footprints:bergstak_plug_2x20_male)
      (datasheet https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10144517.pdf)
      (fields
        (field (name "Mfg PN") 10144517-041802LF)
        (field (name Mfg) Amphenol)
        (field (name "Digikey PN") 609-5429-1-ND)
        (field (name "Digikey URL") https://www.digikey.com/product-detail/en/amphenol-fci/10144517-041802LF/609-5429-1-ND/8573002)
        (field (name Mating) "Amphenol 10144518-042802LF"))
      (libsource (lib conn) (part Conn_02x20_Odd_Even))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B348A9B))
    (comp (ref TP2)
      (value TEST)
      (footprint footprints:patch_pad)
      (libsource (lib device) (part TEST))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B36F726))
    (comp (ref TP1)
      (value TEST)
      (footprint footprints:patch_pad)
      (libsource (lib device) (part TEST))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B36F888))
    (comp (ref TP3)
      (value TEST)
      (footprint footprints:patch_pad)
      (libsource (lib device) (part TEST))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B36E052))
    (comp (ref TP4)
      (value TEST)
      (footprint footprints:patch_pad)
      (libsource (lib device) (part TEST))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B36E1C8))
    (comp (ref TP6)
      (value TEST)
      (footprint footprints:patch_pad)
      (libsource (lib device) (part TEST))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38C0FA))
    (comp (ref TP5)
      (value TEST)
      (footprint footprints:patch_pad)
      (libsource (lib device) (part TEST))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38C16F))
    (comp (ref JP4)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38C712))
    (comp (ref JP3)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38C8AB))
    (comp (ref JP1)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38C926))
    (comp (ref JP5)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38CDD6))
    (comp (ref JP6)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38D01D))
    (comp (ref JP7)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38D0B1))
    (comp (ref JP8)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38D0F6))
    (comp (ref JP9)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38D1CE))
    (comp (ref J2)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38DD78))
    (comp (ref J4)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38DE9E))
    (comp (ref J5)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38DEED))
    (comp (ref J6)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38DF3B))
    (comp (ref J7)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38DF8C))
    (comp (ref J8)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38DFE0))
    (comp (ref J9)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E037))
    (comp (ref J10)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E091))
    (comp (ref J11)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E546))
    (comp (ref J12)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E54C))
    (comp (ref J13)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E552))
    (comp (ref J14)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E558))
    (comp (ref J15)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E55E))
    (comp (ref J16)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E564))
    (comp (ref J17)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E56A))
    (comp (ref J18)
      (value Conn_Coaxial_Power)
      (footprint footprints:rg178_coax_solder_pad)
      (libsource (lib conn) (part Conn_Coaxial_Power))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38E570))
    (comp (ref JP2)
      (value Jumper_NC_Small)
      (footprint footprints:solder_jumper_2pin)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38C8ED))
    (comp (ref TP7)
      (value TEST)
      (footprint footprints:patch_pad)
      (libsource (lib device) (part TEST))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38CD35))
    (comp (ref TP8)
      (value TEST)
      (footprint footprints:patch_pad)
      (libsource (lib device) (part TEST))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B38DE8E)))
  (libparts
    (libpart (lib conn) (part Conn_02x20_Odd_Even)
      (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)")
      (docs ~)
      (footprints
        (fp Connector*:*2x??x*mm*)
        (fp Connector*:*2x???Pitch*)
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x20_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive))))
    (libpart (lib conn) (part Conn_Coaxial_Power)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (docs ~)
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_Coaxial_Power))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))))
    (libpart (lib device) (part Jumper_NC_Small)
      (description "Jumper, normally closed")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part TEST)
      (description "Testpoint, connection for test equipment")
      (fields
        (field (name Reference) TP)
        (field (name Value) TEST))
      (pins
        (pin (num 1) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib)))
  (nets
    (net (code 1) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3))
      (node (ref TP1) (pin 1)))
    (net (code 2) (name "Net-(J3-Pad39)")
      (node (ref J3) (pin 39))
      (node (ref TP3) (pin 1)))
    (net (code 3) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref TP2) (pin 1)))
    (net (code 4) (name "Net-(J3-Pad37)")
      (node (ref TP4) (pin 1))
      (node (ref J3) (pin 37)))
    (net (code 5) (name /NCOM)
      (node (ref JP2) (pin 2))
      (node (ref JP4) (pin 2))
      (node (ref JP7) (pin 2))
      (node (ref JP6) (pin 2))
      (node (ref JP5) (pin 1))
      (node (ref JP1) (pin 2))
      (node (ref JP3) (pin 2))
      (node (ref JP9) (pin 2))
      (node (ref JP8) (pin 2)))
    (net (code 6) (name /SCL_PT)
      (node (ref TP6) (pin 1))
      (node (ref J3) (pin 38)))
    (net (code 7) (name "Net-(J3-Pad35)")
      (node (ref J3) (pin 35)))
    (net (code 8) (name "Net-(J3-Pad36)")
      (node (ref J3) (pin 36)))
    (net (code 9) (name "Net-(J3-Pad34)")
      (node (ref J3) (pin 34)))
    (net (code 10) (name "Net-(J3-Pad33)")
      (node (ref J3) (pin 33)))
    (net (code 11) (name /2P)
      (node (ref J1) (pin 26))
      (node (ref J15) (pin 1)))
    (net (code 12) (name /1N)
      (node (ref JP6) (pin 1))
      (node (ref J18) (pin 1))
      (node (ref J1) (pin 30)))
    (net (code 13) (name /1P)
      (node (ref J17) (pin 1))
      (node (ref J1) (pin 32)))
    (net (code 14) (name VSSA)
      (node (ref J3) (pin 11))
      (node (ref J3) (pin 21))
      (node (ref J3) (pin 31))
      (node (ref J3) (pin 29))
      (node (ref J3) (pin 25))
      (node (ref J3) (pin 9))
      (node (ref TP8) (pin 1))
      (node (ref J3) (pin 17))
      (node (ref J3) (pin 1))
      (node (ref J3) (pin 15))
      (node (ref J1) (pin 33))
      (node (ref J1) (pin 23))
      (node (ref J1) (pin 13))
      (node (ref J3) (pin 27))
      (node (ref J1) (pin 31))
      (node (ref J1) (pin 21))
      (node (ref J1) (pin 11))
      (node (ref J1) (pin 9))
      (node (ref J3) (pin 5))
      (node (ref J3) (pin 19))
      (node (ref J1) (pin 39))
      (node (ref J1) (pin 29))
      (node (ref J1) (pin 19))
      (node (ref J1) (pin 27))
      (node (ref J1) (pin 17))
      (node (ref J3) (pin 23))
      (node (ref J1) (pin 25))
      (node (ref J1) (pin 15))
      (node (ref J3) (pin 13))
      (node (ref J3) (pin 7)))
    (net (code 15) (name VDD)
      (node (ref J1) (pin 6))
      (node (ref J1) (pin 5)))
    (net (code 16) (name GNDD)
      (node (ref J1) (pin 8))
      (node (ref J1) (pin 7)))
    (net (code 17) (name "Net-(J1-Pad37)")
      (node (ref TP7) (pin 1))
      (node (ref J1) (pin 37)))
    (net (code 18) (name /8P)
      (node (ref J2) (pin 1))
      (node (ref J3) (pin 12)))
    (net (code 19) (name /7P)
      (node (ref J5) (pin 1))
      (node (ref J3) (pin 18)))
    (net (code 20) (name /4N)
      (node (ref JP9) (pin 1))
      (node (ref J1) (pin 12))
      (node (ref J12) (pin 1)))
    (net (code 21) (name /8N)
      (node (ref J4) (pin 1))
      (node (ref JP1) (pin 1))
      (node (ref J3) (pin 10)))
    (net (code 22) (name /7N)
      (node (ref J6) (pin 1))
      (node (ref JP2) (pin 1))
      (node (ref J3) (pin 16)))
    (net (code 23) (name /6N)
      (node (ref JP3) (pin 1))
      (node (ref J3) (pin 22))
      (node (ref J8) (pin 1)))
    (net (code 24) (name /5N)
      (node (ref JP4) (pin 1))
      (node (ref J10) (pin 1))
      (node (ref J3) (pin 28)))
    (net (code 25) (name /5P)
      (node (ref J3) (pin 30))
      (node (ref J9) (pin 1)))
    (net (code 26) (name /4P)
      (node (ref J1) (pin 14))
      (node (ref J11) (pin 1)))
    (net (code 27) (name /3N)
      (node (ref JP8) (pin 1))
      (node (ref J14) (pin 1))
      (node (ref J1) (pin 18)))
    (net (code 28) (name /3P)
      (node (ref J13) (pin 1))
      (node (ref J1) (pin 20)))
    (net (code 29) (name /2N)
      (node (ref JP7) (pin 1))
      (node (ref J16) (pin 1))
      (node (ref J1) (pin 24)))
    (net (code 30) (name /6P)
      (node (ref J7) (pin 1))
      (node (ref J3) (pin 24)))
    (net (code 31) (name /BIAS)
      (node (ref J5) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref J16) (pin 2))
      (node (ref J6) (pin 2))
      (node (ref J11) (pin 2))
      (node (ref J10) (pin 2))
      (node (ref J7) (pin 2))
      (node (ref J9) (pin 2))
      (node (ref J8) (pin 2))
      (node (ref JP5) (pin 2))
      (node (ref J1) (pin 10))
      (node (ref J1) (pin 22))
      (node (ref J3) (pin 26))
      (node (ref J3) (pin 14))
      (node (ref J3) (pin 32))
      (node (ref J3) (pin 20))
      (node (ref J3) (pin 8))
      (node (ref J12) (pin 2))
      (node (ref J13) (pin 2))
      (node (ref J14) (pin 2))
      (node (ref J15) (pin 2))
      (node (ref J18) (pin 2))
      (node (ref J17) (pin 2))
      (node (ref J1) (pin 34))
      (node (ref J1) (pin 16))
      (node (ref J1) (pin 28)))
    (net (code 32) (name /SDA_PT)
      (node (ref TP5) (pin 1))
      (node (ref J3) (pin 40)))
    (net (code 33) (name "Net-(J3-Pad6)")
      (node (ref J3) (pin 6)))
    (net (code 34) (name "Net-(J1-Pad40)")
      (node (ref J1) (pin 40)))
    (net (code 35) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 36) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 37) (name "Net-(J3-Pad4)")
      (node (ref J3) (pin 4)))
    (net (code 38) (name "Net-(J3-Pad3)")
      (node (ref J3) (pin 3)))
    (net (code 39) (name "Net-(J3-Pad2)")
      (node (ref J3) (pin 2)))
    (net (code 40) (name "Net-(J1-Pad38)")
      (node (ref J1) (pin 38)))
    (net (code 41) (name "Net-(J1-Pad36)")
      (node (ref J1) (pin 36)))
    (net (code 42) (name "Net-(J1-Pad35)")
      (node (ref J1) (pin 35)))))