(module bergstak_plug_2x20_male (layer F.Cu) (tedit 5B389E24)
  (fp_text reference REF** (at 0.4 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value bergstak_plug_2x20_male (at -0.2 -8.6) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 8.5 -1) (end -8.5 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.5 1) (end 8.5 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.5 1) (end 8.5 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.5 -1) (end -8.5 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -10 2) (end -8.5 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -10 0) (end -10 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -9 0) (end -10 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -9 -2) (end -9 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.5 -2) (end -9 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 9 -2) (end 8.5 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 9 0) (end 9 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.5 0) (end 9 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 0) (end 9.5 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 0.5) (end 10 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 2) (end 10 0.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.5 2) (end 10 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -11 3) (end -11 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.5 3) (end -11 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.5 2) (end -8.5 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.5 2) (end -8.5 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.5 3) (end 8.5 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 11 3) (end 8.5 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 11 -3) (end 11 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.5 -3) (end 11 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.5 -2) (end 8.5 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.5 -2) (end 8.5 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -8.5 -3) (end -8.5 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -11 -3) (end -8.5 -3) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -7.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -7.594018 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -6.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -6.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -5.994018 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -5.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -5.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -4.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -4.394018 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -3.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -3.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -2.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -2.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -1.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -1.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -0.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -0.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 0.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 0.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 1.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 1.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 2.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 2.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 3.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 3.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 4.4 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 4.4 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 5.2 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at 5.2 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at 6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at 6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at 6.8 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 38 smd rect (at 6.8 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at 7.6 -2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad 40 smd rect (at 7.6 2.2 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at 10.1 0) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -10.1 0) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
)
