(module Würth_WR-WST_debug_490107670812_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 650B5558)
  (descr "Würth WR-WST series direct-to-board connector footprint, debug application tolerances, MPN 490107670812 https://www.we-online.com/components/products/datasheet/490107670812.pdf Generated with kicad-footprint-generator.")
  (tags "connector Würth WR-WST_debug vertical")
  (attr exclude_from_bom)
  (fp_text reference REF** (at 0 -10.07) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Würth_WR-WST_debug_490107670812_2x04_P2.54mm_Vertical (at 0 10.07) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.8 -8.875) (end -2.8 8.875) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 8.875) (end 2.8 8.875) (layer F.Fab) (width 0.1))
  (fp_line (start 2.8 8.875) (end 2.8 -8.875) (layer F.Fab) (width 0.1))
  (fp_line (start 2.8 -8.875) (end -2.8 -8.875) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 -5.195) (end -1.3 -4.445) (layer F.Fab) (width 0.1))
  (fp_line (start -1.3 -4.445) (end -2.8 -3.695) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 -8.875) (end -2.8 8.875) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 8.875) (end 2.8 8.875) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 8.875) (end 2.8 -8.875) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 -8.875) (end -2.8 -8.875) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.24 -7.815) (end -3.24 -9.315) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.24 -9.315) (end -1.74 -9.315) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 -7.795) (end -1.3 -7.045) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.3 -7.045) (end -2.8 -6.295) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 -7.795) (end 2.4 -7.795) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.4 -7.795) (end 2.4 -6.295) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.4 -6.295) (end 2.8 -6.295) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 5.895) (end -2.4 5.895) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.4 5.895) (end -2.4 7.395) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.4 7.395) (end -2.8 7.395) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 -9.375) (end -3.3 9.375) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.3 9.375) (end 3.3 9.375) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.3 9.375) (end 3.3 -9.375) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.3 -9.375) (end -3.3 -9.375) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at -1.27 -4.445) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.27 -3.175) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -1.27 -1.905) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 1.27 -0.635) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -1.27 0.635) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 1.27 1.905) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -1.27 3.175) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 1.27 4.445) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 1.27 -5.675) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -1.27 5.675) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  (fp_text user ${REFERENCE} (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
)
