(footprint "proto_3x3" (version 20230410) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "Dwgs.User") hide (tstamp 46bb6dc7-58f5-4f26-9ae9-75ed7489d6fd)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (fp_text value "proto_3x3" (at 0 1 unlocked) (layer "F.Fab") (tstamp 76661532-5791-42a8-b4da-4c1de8ab4132)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") (tstamp 4827b9a1-3c6b-4d65-933c-455a0e3d03cd)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 8375d10b-19b0-4e25-a5d0-fa7de82b2a57))
  (pad "1" thru_hole circle (at -2.54 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 063f7b41-f563-45a9-a038-17f9f111ae04))
  (pad "1" thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp e78a9d05-2562-4030-9ce2-1d3e7f576a1e))
  (pad "1" thru_hole circle (at 0 -2.54) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 77b07121-6d23-4e87-b583-412dce7c3a1f))
  (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 6cd283f6-0657-44b0-8c1a-8a5168d6e039))
  (pad "1" thru_hole circle (at 0 2.54) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 0b6b0558-2feb-4aa7-8407-9362acc4ed00))
  (pad "1" thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 714cc91f-43db-4ac4-983a-89ed1e1eb4c0))
  (pad "1" thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp fdc3f656-f95d-4f99-85c8-aaeb734a2848))
  (pad "1" thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp ef0fb373-9454-4a30-a257-b761ae5b2903))
)
