(footprint "led_tape_3528_2835" (version 20230913) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "Jr" (at 0 0.499999 0) (layer "F.SilkS") hide (tstamp 4093aa2f-3722-4c37-bced-fe5acff3bcf7)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Value" "bottom left" (at 0 -0.499999 0) (layer "F.Fab") hide (tstamp d0e35734-5823-495d-afd7-d6888dc03b27)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 30f47938-bfe8-41a3-8cc3-a1386ca2daf4)
    (effects (font (size 1.27 1.27)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp df1a507b-3df3-45ed-96a7-65c8443300d3)
    (effects (font (size 1.27 1.27)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 74b77890-d4fd-48ba-9045-58fc46cd4788)
    (effects (font (size 1.27 1.27)))
  )
  (attr through_hole)
  (fp_line (start -4 0) (end -4 29)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp aed19ae8-3fc0-468d-b321-0c6267836b24))
  (fp_line (start -4 0) (end 4 0)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp c155d873-1895-4b81-9bc9-fb1441059805))
  (fp_line (start -4 1.000001) (end 1 3.000001)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp 8960bc22-b9a3-4933-b841-be5ff656ee2b))
  (fp_line (start -4 2.000001) (end -1.5 3.000001)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp bb766257-16ac-4b2e-a8dd-c9af06b1a478))
  (fp_line (start -4 3.000001) (end 4 3.000001)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp e423540d-64dc-428a-bf52-71c98db81b6e))
  (fp_line (start 1 0.000001) (end 4 1.000001)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp 085d21a2-d3e2-4a32-8995-d05daac4d9d6))
  (fp_line (start 4 2.000001) (end -1.5 0.000001)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp 5b9e2953-2259-4aeb-b81d-0148660d9091))
  (fp_line (start 4 3.000001) (end -4 0)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp dc34f365-cf3e-49d6-ab3a-efe2b6a1b8ba))
  (fp_line (start 4 29) (end 4 0)
    (stroke (width 0.5) (type solid)) (layer "F.SilkS") (tstamp 6e73dfc9-2809-4850-9289-74bc83f4d89e))
  (fp_line (start -7 0) (end -7 3)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp d9fd38eb-0aef-40ca-a723-43d1b6c0aa0a))
  (fp_line (start -7 3) (end -5 3)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 2d936a0e-0d74-43d7-9b88-19929fa9c6d9))
  (fp_line (start -5 0) (end -7 0)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 9e846c8f-857f-45ab-926e-3ded8e99d358))
  (fp_line (start -5 3) (end -5 0)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 59293fc9-e48a-43ed-a2f0-7af561eb91d6))
  (fp_line (start -5 29) (end 5 29)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 6115e487-7bec-44ca-a080-6de0c3f4ba29))
  (fp_line (start -5 31.5) (end -5 29)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 609f168e-fd7e-42e8-9f57-7752e059abcd))
  (fp_line (start 5 3) (end 5 0)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 116e171b-194b-4cff-b280-b4797251ab88))
  (fp_line (start 5 3) (end 7 3)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp fec93335-7a67-4085-ae71-4a7184dc0a88))
  (fp_line (start 5 29) (end 5 31.5)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp c1953598-ca5c-4e4a-9d75-97c10032338d))
  (fp_line (start 5 31.5) (end -5 31.5)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 69fd8437-fa9a-4c0c-8718-4dad02b7c7bd))
  (fp_line (start 7 0) (end 5 0)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 8b5b2780-7771-42aa-ac6b-e2510133540f))
  (fp_line (start 7 0) (end 7 3)
    (stroke (width 0.12) (type solid)) (layer "Dwgs.User") (tstamp 539ccb8e-b877-4632-9499-fad83dc1f6ca))
  (pad "1" smd roundrect (at 2 19.4) (size 3 18) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.08333333333)
    (tstamp c9fd947b-eb73-4e20-8383-55b39c6482be)
  )
  (pad "2" smd roundrect (at -2 19.4) (size 3 18) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.08333333333)
    (tstamp 831bd7ee-192d-417f-8663-949b9d5bba96)
  )
)
