(footprint "milliohm_shunt_P10D2.5" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 38cf1763-5c47-41b0-b836-733f980b60bf)
  )
  (fp_text value "milliohm_shunt_P10D2.5" (at 0 5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 55e694ef-df43-4977-b9e4-86d34c032108)
  )
  (fp_text user "${REF}" (at 0 3.75 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b97f913d-c881-47cf-9c50-94d39caf90ca)
  )
  (fp_line (start -2.25 -1.75) (end 2.25 -1.75)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 1fe2f51b-223c-4c38-8822-99c821e85ef9))
  (fp_line (start -2 1) (end -0.75 1)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 616009a4-eae6-4606-8432-f7df1959bc2e))
  (fp_line (start -0.75 -1) (end 0.75 -1)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp c4beef9b-7ff5-4494-a88c-4d9b9aec1b88))
  (fp_line (start -0.75 1) (end -0.75 -1)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp edaf3bcc-463c-4ec3-af7e-e48cc1e14ea2))
  (fp_line (start 0.75 -1) (end 0.75 1)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 3108e88e-91c8-4a40-acb2-a10ce197bbda))
  (fp_line (start 0.75 1) (end 2 1)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp ea50f612-57a7-491f-b517-0dd275cc3c59))
  (fp_line (start 2.25 1.75) (end -2.25 1.75)
    (stroke (width 0.25) (type default)) (layer "F.SilkS") (tstamp 0a6fc625-c064-40bc-a06a-c6034d420bd1))
  (fp_rect (start -2.75 -2.25) (end -7.25 2.25)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp db788ad0-61a6-4e4f-a847-4de00c7faea1))
  (fp_rect (start 2.75 -2.25) (end 7.25 2.25)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 04aac230-2f9c-427e-9f85-823afe4e1965))
  (pad "1" thru_hole roundrect (at -5 0) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp b5fc41d3-3d86-4d3a-b344-e6dcec9d09f1))
  (pad "2" thru_hole roundrect (at 5 0) (size 4.5 4.5) (drill 2.7) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp caf3e255-b97d-4cf4-a435-6f71ea2b3336))
)
