(footprint "double_wire_pads" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp cf043f51-e415-43dc-9a1a-f1be56a11d98)
  )
  (fp_text value "double_wire_pads" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp db15ba4e-d2d9-45a1-8d68-26a6caa8a2ab)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7cca8717-8e6a-45c5-92f3-f50e60376275)
  )
  (pad "1" thru_hole rect (at -2.5 0 90) (size 8 3.5) (drill 2) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp a9430b68-d1fa-4341-b8d1-e783a3cb168d))
  (pad "2" thru_hole rect (at 2.5 0 90) (size 8 3.5) (drill 2) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp c60f0d20-a2b9-415e-b867-94b73ce8e55d))
)
