(footprint "terminal_chonky_JL5EDGRHC_2P" (version 20230410) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") (tstamp e6278b32-5dcb-4472-a6f8-72243221e0e7)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "terminal_chonky_JL5EDGRHC_2P" (at 0 1 unlocked) (layer "F.Fab") (tstamp 660a64a5-e775-4cf2-b1a3-32bd9c3151ca)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -8.89 -1.905) (end -8.89 27.345)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 44ceb615-13bf-4c5f-88fd-44b57f345de5))
  (fp_line (start -8.89 -1.905) (end 8.89 -1.905)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp da4f48ee-3e95-410f-8186-4991f51a96b0))
  (fp_line (start -8.89 24.765) (end 8.89 24.765)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b25af151-8799-4c6d-b59c-0c01db4ae3be))
  (fp_line (start -8.89 27.345) (end 8.89 27.345)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 7ef2b7a8-e343-4173-96f6-de1f003f8ed4))
  (fp_line (start -5.715 16.51) (end -6.35 24.765)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 22f67dd9-0546-470a-959d-c96f0e422126))
  (fp_line (start -3.175 16.51) (end -5.715 16.51)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c3b70f1e-cccb-423f-9cb4-675cd6cccc1f))
  (fp_line (start -2.54 24.765) (end -3.175 16.51)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp ed36b909-2821-4f6c-a63a-e674efff28cf))
  (fp_line (start 0 -1.905) (end 0 27.345)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 47551fe3-0fa7-4085-9f98-8c772bb493ce))
  (fp_line (start 3.175 16.51) (end 2.54 24.765)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b8969e49-5906-4c46-a206-d6cc527e843e))
  (fp_line (start 5.715 16.51) (end 3.175 16.51)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp dd03fb91-cd0f-478d-af1c-303c6f465191))
  (fp_line (start 6.35 24.765) (end 5.715 16.51)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d4fd486e-e17e-44dc-a7ee-eda83205c84a))
  (fp_line (start 8.89 -1.905) (end 8.89 27.345)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d419d677-e889-4fb3-b282-3721bb6edc79))
  (fp_rect (start -8.89 -1.905) (end 8.89 27.305)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 35a53d7e-08db-4c48-bb49-571e3ac1f05c))
  (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab") (tstamp 50585957-eb69-44bf-a92c-7081d51f56a7)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" thru_hole oval (at -3.81 0 90) (size 3.5 3) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp 462b4d3b-5bce-4de9-83f1-a364c67e5fa5))
  (pad "1" thru_hole oval (at -3.81 5.08 90) (size 3.5 3) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp 9ac30da5-3f02-4b52-8e18-195b355606ea))
  (pad "1" thru_hole oval (at -3.81 7.62 90) (size 3.5 3) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp bd2808d9-3b94-416d-a8d9-cfacfdfce461))
  (pad "2" thru_hole oval (at 3.81 -0.000865 90) (size 3.5 3) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp b75a8add-80ff-4ffc-8e26-48414960417c))
  (pad "2" thru_hole oval (at 3.81 5.079135 90) (size 3.5 3) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp 56c09a3a-1215-4699-9ba9-09e5a2aa1631))
  (pad "2" thru_hole oval (at 3.81 7.619135 90) (size 3.5 3) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp 52717eeb-ca3b-4b57-a347-3bdfa4f88c60))
)
