(module Würth_WR-WST_permanent_490107671812_2x09_P2.54mm_Vertical (layer F.Cu) (tedit 650B5558)
  (descr "Würth WR-WST series direct-to-board connector footprint, permanent application tolerances, MPN 490107671812 https://www.we-online.com/components/products/datasheet/490107671812.pdf Generated with kicad-footprint-generator.")
  (tags "connector Würth WR-WST_permanent vertical")
  (attr exclude_from_bom)
  (fp_text reference REF** (at 0 -16.42) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Würth_WR-WST_permanent_490107671812_2x09_P2.54mm_Vertical (at 0 16.42) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.8 -15.225) (end -2.8 15.225) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 15.225) (end 2.8 15.225) (layer F.Fab) (width 0.1))
  (fp_line (start 2.8 15.225) (end 2.8 -15.225) (layer F.Fab) (width 0.1))
  (fp_line (start 2.8 -15.225) (end -2.8 -15.225) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 -11.545) (end -1.3 -10.795) (layer F.Fab) (width 0.1))
  (fp_line (start -1.3 -10.795) (end -2.8 -10.045) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 -15.225) (end -2.8 15.225) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 15.225) (end 2.8 15.225) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 15.225) (end 2.8 -15.225) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 -15.225) (end -2.8 -15.225) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.24 -14.165) (end -3.24 -15.665) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.24 -15.665) (end -1.74 -15.665) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 -14.045) (end -1.3 -13.295) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.3 -13.295) (end -2.8 -12.545) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 -14.045) (end 2.4 -14.045) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.4 -14.045) (end 2.4 -12.545) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.4 -12.545) (end 2.8 -12.545) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 12.145) (end -2.4 12.145) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.4 12.145) (end -2.4 13.645) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.4 13.645) (end -2.8 13.645) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 -15.725) (end -3.3 15.725) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.3 15.725) (end 3.3 15.725) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.3 15.725) (end 3.3 -15.725) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.3 -15.725) (end -3.3 -15.725) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at -1.27 -10.795) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.27 -9.525) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -1.27 -8.255) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 1.27 -6.985) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -1.27 -5.715) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 1.27 -4.445) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -1.27 -3.175) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 1.27 -1.905) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at -1.27 -0.635) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 1.27 0.635) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at -1.27 1.905) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 1.27 3.175) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at -1.27 4.445) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 1.27 5.715) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at -1.27 6.985) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 1.27 8.255) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at -1.27 9.525) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 1.27 10.795) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 1.27 -12.125) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -1.27 12.125) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  (fp_text user ${REFERENCE} (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
)
