(footprint "inductor_chonky_18x18mm" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 73ca33e1-5cdc-40bd-889f-e806c545e1ee)
  )
  (fp_text value "inductor_chonky_18x18mm" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 93e12f10-7c29-42f0-a9c7-dcd2c166719d)
  )
  (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4f221382-2e49-450f-855c-f95e9f50bcc0)
  )
  (fp_line (start -9 -9) (end 9 -9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e842c36f-ff12-4eeb-9bec-f4386565137d))
  (fp_line (start -9 -3) (end -9 -9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 65c6198e-c26b-4ba0-91c1-a7da8c48da74))
  (fp_line (start -9 9) (end -9 3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp bb857c9d-2c2e-478f-b5b7-2d009fd24f24))
  (fp_line (start 9 -9) (end 9 -3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b9d9078c-98a7-4db1-b4c7-56e869e36146))
  (fp_line (start 9 3) (end 9 9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 1294cfc2-ed22-40a6-9768-e63186ed09a9))
  (fp_line (start 9 9) (end -9 9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 1e863e19-3b63-4cd9-bd8f-937332dc2039))
  (fp_arc (start -7 -3) (mid 0 -7.615773) (end 7 -3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp ae2f7385-7c21-492d-a4da-3bf14532d53d))
  (fp_arc (start 7 3) (mid 0 7.615773) (end -7 3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp eaf7db45-3ad6-4c0c-ad20-946a12934d25))
  (fp_rect (start -9 -9) (end 9 9)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp 677b58da-5dd7-4576-9a5d-93e9100f2be0))
  (fp_rect (start -9 -9) (end 9 9)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 55fc8439-34d9-4e39-b1e4-125742f0909c))
  (pad "1" smd rect (at -6.65 0) (size 6 6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 23bdb584-c11c-4750-ae06-717f39ef3a85))
  (pad "2" smd rect (at 6.65 0) (size 6 6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 0bd0d0a5-147c-4c2c-8927-c46ab9ec0c99))
)
