(module led_tape_3528_2835 (layer F.Cu) (tedit 5BF8B28A)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value led_tape_3528_2835 (at 0 -0.5) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.5 0) (end 0.5 0) (layer F.SilkS) (width 0.5))
  (fp_line (start 4 22) (end 4 0) (layer F.SilkS) (width 0.5))
  (fp_line (start -4 0) (end -4 22) (layer F.SilkS) (width 0.5))
  (fp_line (start -4 15) (end 4 15) (layer F.SilkS) (width 0.5))
  (fp_line (start 4 15) (end -4 12) (layer F.SilkS) (width 0.5))
  (fp_line (start -4 12) (end 4 12) (layer F.SilkS) (width 0.5))
  (fp_line (start 4 14) (end -1.5 12) (layer F.SilkS) (width 0.5))
  (fp_line (start 1 12) (end 4 13) (layer F.SilkS) (width 0.5))
  (fp_line (start -4 14) (end -1.5 15) (layer F.SilkS) (width 0.5))
  (fp_line (start -4 13) (end 1 15) (layer F.SilkS) (width 0.5))
  (pad 2 smd oval (at 2.25 0) (size 2.8 5) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd oval (at -2.25 0) (size 2.8 5) (layers F.Cu F.Paste F.Mask))
)
