(footprint "inductor_chonky_28x28" (version 20230410) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") (tstamp 67245126-7a71-4d4c-b5ea-9b571daf9bf9)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (fp_text value "inductor_chonky_28x28" (at 0 1 unlocked) (layer "F.Fab") (tstamp 709d799d-981f-4bc4-8d8b-626755592647)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_rect (start -14 -9.75) (end 14 9.75)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp a9e8633f-5c2f-4c80-95ba-75e8548ac351))
  (fp_poly
    (pts
      (xy -3.5 -10.5)
      (xy -3.5 -12.5)
      (xy 3.5 -12.5)
      (xy 3.5 -10.5)
      (xy 14.5 -10.5)
      (xy 14.5 10.5)
      (xy 9 10.5)
      (xy 9 18)
      (xy -9 18)
      (xy -9 10.5)
      (xy -14.5 10.5)
      (xy -14.5 -10.5)
    )
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 6a0a9738-448f-4c43-aea3-7ee2508d7d42))
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") (tstamp b66430a5-0069-4982-a80c-36eee1d734ea)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd rect (at -5.215 14.4) (size 6 6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp cdc20095-3528-404e-ba6c-8d1496b19235))
  (pad "2" smd rect (at 5.215 14.4) (size 6 6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6478105b-5fd7-4c74-b0f5-68bd948bc64b))
  (pad "MP" smd rect (at 0 -8.75) (size 6 6) (property pad_prop_heatsink) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 8967f083-8f34-42e9-b841-44b910d1a0a9))
)
