(module Würth_WR-WST_debug_490107670612_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 650B5558)
  (descr "Würth WR-WST series direct-to-board connector footprint, debug application tolerances, MPN 490107670612 https://www.we-online.com/components/products/datasheet/490107670612.pdf Generated with kicad-footprint-generator.")
  (tags "connector Würth WR-WST_debug vertical")
  (attr exclude_from_bom)
  (fp_text reference REF** (at 0 -8.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Würth_WR-WST_debug_490107670612_2x03_P2.54mm_Vertical (at 0 8.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.8 -7.605) (end -2.8 7.605) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 7.605) (end 2.8 7.605) (layer F.Fab) (width 0.1))
  (fp_line (start 2.8 7.605) (end 2.8 -7.605) (layer F.Fab) (width 0.1))
  (fp_line (start 2.8 -7.605) (end -2.8 -7.605) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 -3.925) (end -1.3 -3.175) (layer F.Fab) (width 0.1))
  (fp_line (start -1.3 -3.175) (end -2.8 -2.425) (layer F.Fab) (width 0.1))
  (fp_line (start -2.8 -7.605) (end -2.8 7.605) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 7.605) (end 2.8 7.605) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 7.605) (end 2.8 -7.605) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 -7.605) (end -2.8 -7.605) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.24 -6.545) (end -3.24 -8.045) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.24 -8.045) (end -1.74 -8.045) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 -6.525) (end -1.3 -5.775) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.3 -5.775) (end -2.8 -5.025) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.8 -6.525) (end 2.4 -6.525) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.4 -6.525) (end 2.4 -5.025) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.4 -5.025) (end 2.8 -5.025) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.8 4.625) (end -2.4 4.625) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.4 4.625) (end -2.4 6.125) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.4 6.125) (end -2.8 6.125) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.3 -8.105) (end -3.3 8.105) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.3 8.105) (end 3.3 8.105) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.3 8.105) (end 3.3 -8.105) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.3 -8.105) (end -3.3 -8.105) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at -1.27 -3.175) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.27 -1.905) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -1.27 -0.635) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 1.27 0.635) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -1.27 1.905) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 1.27 3.175) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 1.27 -4.405) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -1.27 4.405) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  (fp_text user ${REFERENCE} (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
)
