(footprint "terminal_KF2EDGR" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 323e6cc5-d0a3-41b4-903c-8c5d13fd4614)
  )
  (fp_text value "terminal_KF2EDGR" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a85df372-630c-4218-b6e8-59fd764ce515)
  )
  (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3588222f-c2ce-454f-9ff3-2b3fc8e4fd4b)
  )
  (fp_line (start -5 -2.5) (end 5 -2.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 950dd81d-998b-4505-a78c-9d00cc887fd0))
  (fp_line (start -5 8) (end 5 8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 9c93b19b-d31f-4047-b014-91de2d03d47d))
  (fp_line (start -5 9.5) (end -5 -2.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8fbd0441-2132-434c-99aa-50023aec67fe))
  (fp_line (start -3.5 9.5) (end -3 8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d2cbd753-4e37-40fd-bb3e-96399ef73566))
  (fp_line (start -1.5 9.5) (end -2 8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 1af57fb3-2066-41fc-9ba4-52b15f0fa0b4))
  (fp_line (start 1.5 9.5) (end 2 8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 4dbcb663-850f-4f67-9636-366c89760bf4))
  (fp_line (start 3.5 9.5) (end 3 8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp bc7cf793-91c6-4852-b7e5-40f28355eeda))
  (fp_line (start 5 -2.5) (end 5 9.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 7a98231e-4894-4483-8d07-7af8fd6b9b25))
  (fp_line (start 5 9.5) (end -5 9.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 1446f15e-143d-407e-9bcd-1e8e232f6aeb))
  (fp_rect (start -5 -2.5) (end 5 9.5)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 0b8dfb78-5654-4609-af2b-bd6b1a7e1c5d))
  (pad "1" thru_hole oval (at -2.5 0 90) (size 4.5 3) (drill 1.6) (layers *.Cu *.Mask) (tstamp 334fec1b-bfe0-4ad4-9f08-c8a07d489698))
  (pad "2" thru_hole oval (at 2.5 0 90) (size 4.5 3) (drill 1.6) (layers *.Cu *.Mask) (tstamp 47fc8096-c1a8-4865-a114-e5078726a006))
)
