(module pad-between-spiked (layer F.Cu) (tedit 5B6B1D89)
  (descr "Through hole pin header")
  (tags "pin header")
  (fp_text reference REF** (at 0 -5.1) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value pad-between (at 0 -3.1) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 smd custom (at 0 -0.06) (size 0.7 0.85) (layers *.Cu *.Mask)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.55 -0.44) (xy -0.325 -0.44) (xy 0 -0.765) (xy 0.325 -0.44) (xy 0.55 -0.44)
         (xy 0.35 -0.24) (xy 0.35 0.36) (xy 0.55 0.56) (xy 0.338 0.56) (xy 0.338 0.763)
         (xy 0 0.425) (xy -0.01 0.425) (xy -0.348 0.763) (xy -0.348 0.56) (xy -0.55 0.56)
         (xy -0.35 0.36) (xy -0.35 -0.24)) (width 0.001))
    ))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
