(footprint "QFN-42_EP_3.5x9_Pitch0.5mm"
	(version 20241228)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -6.05 0)
		(layer "F.SilkS")
		(uuid "9e0136f8-2a89-4c22-8acb-14aa4d87f625")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "QFN-42_EP_3.5x9_Pitch0.5mm"
		(at 0 6.05 0)
		(layer "F.Fab")
		(uuid "a1fa435a-16f2-4092-bae3-14797baff216")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "419931a3-9cd1-463c-917f-81668964baa0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3815213f-ea89-443e-bcd7-aedf86f04ec6")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.9 4.65)
		(end -1.9 4.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "099780cc-94be-4140-b02e-007f27b447e1")
	)
	(fp_line
		(start -1.25 -4.65)
		(end -2.065 -4.65)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "cd529e2e-ec2e-451e-9ba6-883d08c91115")
	)
	(fp_line
		(start -1.25 4.65)
		(end -1.9 4.65)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c5a56569-c59b-44b5-941d-5feda4f89710")
	)
	(fp_line
		(start 1.25 -4.65)
		(end 1.9 -4.65)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4b450853-f456-421a-a729-5f6c832ee3d6")
	)
	(fp_line
		(start 1.25 4.65)
		(end 1.9 4.65)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "83a0a809-38fa-4800-8544-8b08391fe757")
	)
	(fp_line
		(start 1.9 -4.65)
		(end 1.9 -4.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3d0a9d5a-bb06-4e66-b546-887efb81ba75")
	)
	(fp_line
		(start 1.9 4.65)
		(end 1.9 4.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "32cb200e-6548-44ec-be1e-9ba7f2e03760")
	)
	(fp_line
		(start -2.3 -5.05)
		(end 2.3 -5.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f4800407-d01b-441e-b3ce-8693c238a428")
	)
	(fp_line
		(start -2.3 5.05)
		(end -2.3 -5.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9d3371ec-82f1-4416-8909-cf3985ff3dc7")
	)
	(fp_line
		(start 2.3 -5.05)
		(end 2.3 5.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e45fdc7b-7c2b-4b6e-b3d9-625f86f8d23c")
	)
	(fp_line
		(start 2.3 5.05)
		(end -2.3 5.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "489d25c9-f47e-4f3c-a89d-582049634b77")
	)
	(fp_line
		(start -1.75 -3.5)
		(end -1.75 4.5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "e3a41fc4-9ae8-4e14-9144-322c0b23588d")
	)
	(fp_line
		(start -1.75 4.5)
		(end 1.75 4.5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "f2017e3f-2abf-429a-afe8-b7c6a93976a4")
	)
	(fp_line
		(start -0.75 -4.5)
		(end -1.75 -3.5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0d513ddb-1d11-4ff8-b2fc-f5c25dac6764")
	)
	(fp_line
		(start 1.75 -4.5)
		(end -0.75 -4.5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "b44d1d93-36ce-4d66-92a3-4c71d35ac0d8")
	)
	(fp_line
		(start 1.75 4.5)
		(end 1.75 -4.5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "47af373b-b7f3-489b-b316-f28bada51261")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "169f856b-79d1-4ee3-a709-97ff045da2ad")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -1.585 -4 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "44587c0d-7cbd-4269-916d-b94b4fa026b6")
	)
	(pad "2" smd rect
		(at -1.585 -3.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "b1d93b46-72e4-487f-8572-ea403ad11081")
	)
	(pad "3" smd rect
		(at -1.585 -3 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "fdd2db2b-b7b3-4e63-9813-b352a7389de0")
	)
	(pad "4" smd rect
		(at -1.585 -2.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "3d95304c-b0f2-45cb-91dd-40e35b3be979")
	)
	(pad "5" smd rect
		(at -1.585 -2 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "616e1afb-3a5a-4f3c-9306-dd0d06bc5388")
	)
	(pad "6" smd rect
		(at -1.585 -1.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "1d01a62d-7bb4-4a3e-a475-ec084965695d")
	)
	(pad "7" smd rect
		(at -1.585 -1 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "21b83a2f-ae17-428b-b5a3-b4886a4e1a97")
	)
	(pad "8" smd rect
		(at -1.585 -0.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a0291ad8-02eb-4e2c-867c-5ea64c8f5add")
	)
	(pad "9" smd rect
		(at -1.585 0 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "aeef7834-60a2-4d89-b9fb-d3195919aeb7")
	)
	(pad "10" smd rect
		(at -1.585 0.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "854a75b3-eec8-4676-91d9-87cd1c3f91b9")
	)
	(pad "11" smd rect
		(at -1.585 1 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "7b8ebe4f-9ff7-4747-9654-9738fdac2d08")
	)
	(pad "12" smd rect
		(at -1.585 1.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "713f8ef4-749b-40b2-9c97-ef86142aaaa7")
	)
	(pad "13" smd rect
		(at -1.585 2 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "4d1040a2-9f69-437f-a980-15bee11e24a0")
	)
	(pad "14" smd rect
		(at -1.585 2.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "34ed29be-1dfa-4413-a31c-cf46cf024714")
	)
	(pad "15" smd rect
		(at -1.585 3 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "94fadd68-2991-46bc-bb86-bbcba391dfc9")
	)
	(pad "16" smd rect
		(at -1.585 3.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c98117cd-a2d2-45c5-b19f-a2b35eae2bae")
	)
	(pad "17" smd rect
		(at -1.585 4 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "b8e7177f-c1bc-4db1-9fc6-602a18f61bda")
	)
	(pad "18" smd rect
		(at -0.75 4.335)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "292b05c8-a6b0-402f-bbf0-ec2f3f94c45e")
	)
	(pad "19" smd rect
		(at -0.25 4.335)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ca200546-421b-4521-9ac7-747a49ba7788")
	)
	(pad "20" smd rect
		(at 0.25 4.335)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e83391c9-2b79-44f3-9fac-ffefaf3e9736")
	)
	(pad "21" smd rect
		(at 0.75 4.335)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "8e7199d4-bffe-4c34-bac7-7831137b564c")
	)
	(pad "22" smd rect
		(at 1.585 4 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "1b7e717c-dcb1-46f7-be21-4f17c17edf03")
	)
	(pad "23" smd rect
		(at 1.585 3.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "bf40515b-c97f-4ebb-a4dd-8618a6a08328")
	)
	(pad "24" smd rect
		(at 1.585 3 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "61bbc546-5e1a-46d3-8ad6-dec4afd295b9")
	)
	(pad "25" smd rect
		(at 1.585 2.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "fdfc62df-1ee8-4e1b-9695-40f5cdfba132")
	)
	(pad "26" smd rect
		(at 1.585 2 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "2644552a-af07-4049-ab19-82b5db2cb693")
	)
	(pad "27" smd rect
		(at 1.585 1.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "0dcc7549-e299-457f-9e03-25aadfef6153")
	)
	(pad "28" smd rect
		(at 1.585 1 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c97f1e74-00da-4c04-ab8a-33414f5a5690")
	)
	(pad "29" smd rect
		(at 1.585 0.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "46a8b882-96a0-4a1e-81ad-20a1f5bde48d")
	)
	(pad "30" smd rect
		(at 1.585 0 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "caeed655-ad40-45dc-afb9-ace343b71cb7")
	)
	(pad "31" smd rect
		(at 1.585 -0.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "8c821c5a-b169-4f06-98bd-8439237adcf3")
	)
	(pad "32" smd rect
		(at 1.585 -1 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "bb1fed97-00c8-410b-89a2-27409a59aaaf")
	)
	(pad "33" smd rect
		(at 1.585 -1.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e2dcf515-46a7-47d5-905d-0503b84d7115")
	)
	(pad "34" smd rect
		(at 1.585 -2 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e0a62f3f-603b-4faa-a86d-3d42edd435d4")
	)
	(pad "35" smd rect
		(at 1.585 -2.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "24f099ca-7fd3-4d53-aee5-19b817c9ad0d")
	)
	(pad "36" smd rect
		(at 1.585 -3 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "02361ef4-97de-43aa-912b-1ae60241f4b5")
	)
	(pad "37" smd rect
		(at 1.585 -3.5 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "0681c02b-85cd-42fa-b993-044146f75f4c")
	)
	(pad "38" smd rect
		(at 1.585 -4 90)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "b74e8605-9fb6-4750-b59e-a4235131fa05")
	)
	(pad "39" smd rect
		(at 0.75 -4.335)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "de233562-9192-43b5-92a3-381ffd9558e0")
	)
	(pad "40" smd rect
		(at 0.25 -4.335)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "30b3accd-53d3-44e6-83f6-879cbcfd6607")
	)
	(pad "41" smd rect
		(at -0.25 -4.335)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f3e79cb6-17ec-41fe-be35-9dd361634de6")
	)
	(pad "42" smd rect
		(at -0.75 -4.335)
		(size 0.28 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e9b02fb0-f301-4fa2-872b-1eaad05b22cf")
	)
	(pad "43" thru_hole circle
		(at -0.6 -3.2)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "3a5fc47e-b3da-4f7c-af62-15650d9e36a4")
	)
	(pad "43" thru_hole circle
		(at -0.6 -2.4)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "9bd5aba7-05e3-4154-bc48-0bed80c1964d")
	)
	(pad "43" thru_hole circle
		(at -0.6 -1.6)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "66f4f88c-68da-4843-af0e-1f2ee46f8002")
	)
	(pad "43" thru_hole circle
		(at -0.6 -0.8)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "0264cd53-e800-4d04-9fa5-0abad7ff1dbc")
	)
	(pad "43" thru_hole circle
		(at -0.6 0)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "febf5f5b-1c9f-48cb-b082-4dd6c67ca708")
	)
	(pad "43" thru_hole circle
		(at -0.6 0.8)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "1faf91e0-1f6a-4bb2-9d5a-fc9d9837f4a8")
	)
	(pad "43" thru_hole circle
		(at -0.6 1.6)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "5b4a4baf-23fe-4a4f-bc3c-cd6bf530dd0b")
	)
	(pad "43" thru_hole circle
		(at -0.6 2.4)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "f53ac418-7261-4831-ade0-ab803c77fd21")
	)
	(pad "43" thru_hole circle
		(at -0.6 3.2)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "8da2e00f-14ee-45d0-994d-a7cd3520ab60")
	)
	(pad "43" smd rect
		(at 0 0)
		(size 1.8 7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "8537081e-0f72-4188-84fd-f8514accc38f")
	)
	(pad "43" thru_hole circle
		(at 0.6 -3.2)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "8bc78682-c101-446d-8f71-42ae92c892e8")
	)
	(pad "43" thru_hole circle
		(at 0.6 -2.4)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "696a7070-7261-4dee-9664-0cf3182da366")
	)
	(pad "43" thru_hole circle
		(at 0.6 -1.6)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "4e30fdcf-f064-4ae5-a9b5-4f68fca4a32b")
	)
	(pad "43" thru_hole circle
		(at 0.6 -0.8)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "a02132e0-4ec1-4edf-a1fe-6d03072755cd")
	)
	(pad "43" thru_hole circle
		(at 0.6 0)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "44c98e55-5437-4fe0-9f83-8fa2afc41d87")
	)
	(pad "43" thru_hole circle
		(at 0.6 0.8)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "0d0826ee-e7d5-4981-8591-d65e5c40b4ba")
	)
	(pad "43" thru_hole circle
		(at 0.6 1.6)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "0992891d-40bd-4c67-91b5-9c09d66b5522")
	)
	(pad "43" thru_hole circle
		(at 0.6 2.4)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "fa11c8fc-0a55-438e-97f3-87616e54e9b7")
	)
	(pad "43" thru_hole circle
		(at 0.6 3.2)
		(size 0.4 0.4)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(uuid "e1fbf8c6-ea3c-4bc5-9fe0-3979af489952")
	)
	(embedded_fonts no)
)
