(footprint "TI_RHL0020A_QFN20"
	(version 20241030)
	(generator "pcbnew")
	(generator_version "8.99")
	(layer "F.Cu")
	(property "Reference" "U?"
		(at 0.5 -0.5 0)
		(unlocked yes)
		(layer "Rescue")
		(uuid "dd6979e9-def9-417f-9305-940ac570122b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TI_RHL0020A_QFN20"
		(at 0 1 0)
		(unlocked yes)
		(layer "User.6")
		(uuid "785481ec-5016-499e-8ace-a8939849c260")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "57c2d7cc-dc19-46bb-b181-524730e149dd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e1197507-b454-44be-9a5b-da2da7448b45")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "324b6a38-8a13-4f5f-984d-1c56279ea75b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.25 -2.75)
		(end -2.25 -2.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "37f1d0e5-9a25-47ba-b14b-7369d8a1483d")
	)
	(fp_line
		(start -2.25 -2.75)
		(end -1.25 -2.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9da049db-13cb-4f4b-9f81-dfd5da52591d")
	)
	(fp_line
		(start -2 -2.5)
		(end -1 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "cc7fc38c-c9e2-46d3-ac9b-3a085810d24e")
	)
	(fp_line
		(start -2 -2)
		(end -2 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "aa8acf60-9b43-46d3-9338-5f59e32a478d")
	)
	(fp_line
		(start -2 2.5)
		(end -2 2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fe276a85-8d78-48bf-88f9-1ed27045ca56")
	)
	(fp_line
		(start -1 2.5)
		(end -2 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ee261973-597b-47aa-b47d-96f0f0ff0d3d")
	)
	(fp_line
		(start 1 -2.5)
		(end 2 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "75d307dd-d505-43c3-bd22-c169358818b8")
	)
	(fp_line
		(start 2 -2.5)
		(end 2 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "34d54223-3d21-447a-a8d7-e666f33aaf36")
	)
	(fp_line
		(start 2 2)
		(end 2 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f9f1ca0c-2e19-4cdf-b22f-8d29acfbe939")
	)
	(fp_line
		(start 2 2.5)
		(end 1 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3023c612-ce9a-40dc-ba2d-968fd719a218")
	)
	(fp_rect
		(start -2.25 -2.75)
		(end 2.25 2.75)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Margin")
		(uuid "8e572cf3-044c-4441-b840-ef2addb5fb1e")
	)
	(fp_rect
		(start -2.25 -2.75)
		(end 2.25 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "76f4b088-a2a4-446b-86fd-a6ace2915e84")
	)
	(fp_rect
		(start -1.75 -2.25)
		(end 1.75 2.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "ecd9526a-830f-43cb-8541-268cc3a70ca3")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "User.6")
		(uuid "27fce799-6f7d-401b-a274-fd628ae0065f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.75 -2.15 90)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "bceb2f71-7525-4f17-9691-369c21c406fe")
	)
	(pad "2" smd roundrect
		(at -1.65 -1.75 180)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "c0da6b28-bcfc-4b89-a479-e97a38139477")
	)
	(pad "3" smd roundrect
		(at -1.65 -1.25 180)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "899add83-7f62-424f-8880-2fe06a468713")
	)
	(pad "4" smd roundrect
		(at -1.65 -0.75 180)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "46c27728-7492-41e8-9d28-798a73116d11")
	)
	(pad "5" smd roundrect
		(at -1.65 -0.25 180)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "2aac3fbb-6e8d-4a97-92f3-981477fae194")
	)
	(pad "6" smd roundrect
		(at -1.65 0.25 180)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "d9dc2639-aec4-4622-be8b-985bc32a80e0")
	)
	(pad "7" smd roundrect
		(at -1.65 0.75 180)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "c2031dfb-41eb-4dec-8477-7e996bdb55b9")
	)
	(pad "8" smd roundrect
		(at -1.65 1.25 180)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "f7f395dc-57e5-4e8b-b85d-5ada34b37316")
	)
	(pad "9" smd roundrect
		(at -1.65 1.75 180)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "2d09e3eb-0149-4c83-a70c-5f9fb34a64d4")
	)
	(pad "10" smd roundrect
		(at -0.75 2.15 270)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "c4d95039-17ad-4659-94c6-b9763161b704")
	)
	(pad "11" smd roundrect
		(at 0.75 2.15 270)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "64814f77-dd19-420b-bc70-f2d60aeaa32e")
	)
	(pad "12" smd roundrect
		(at 1.65 1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "7caf25f2-75f0-4695-8eaf-e1d55e696449")
	)
	(pad "13" smd roundrect
		(at 1.65 1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "6fd344ca-d61a-4e30-bce4-c80a96a8b52e")
	)
	(pad "14" smd roundrect
		(at 1.65 0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "cc6dc1a0-9425-491d-9b61-4e5733eed8a9")
	)
	(pad "15" smd roundrect
		(at 1.65 0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "a05969d4-9057-4100-855b-75ff13da8856")
	)
	(pad "16" smd roundrect
		(at 1.65 -0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "f2fe08d5-4de5-4bc8-b594-5ac7a23fffee")
	)
	(pad "17" smd roundrect
		(at 1.65 -0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "62bc81ff-e12a-40dd-bda6-ea9fff872bc7")
	)
	(pad "18" smd roundrect
		(at 1.65 -1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "35cebd2e-8c73-46de-b2ef-494a9df1e565")
	)
	(pad "19" smd roundrect
		(at 1.65 -1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "eea4870c-fcef-49ec-8bb2-d1e4c53aab6b")
	)
	(pad "20" smd roundrect
		(at 0.75 -2.15 90)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "70080aae-10bc-4a4c-a381-c40e6d755874")
	)
	(pad "21" thru_hole circle
		(at -0.75 -0.5 90)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.05)
		(uuid "2bd035b7-a120-40f4-8fe3-57f905675c12")
	)
	(pad "21" thru_hole circle
		(at -0.75 0.5 90)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.05)
		(uuid "3401af08-84db-4741-8aed-1d06d0aecf64")
	)
	(pad "21" smd roundrect
		(at -0.25 -2.15 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.05)
		(thermal_bridge_angle 45)
		(uuid "0133a020-3c6b-439c-96c6-e1f8d33246ac")
	)
	(pad "21" smd roundrect
		(at -0.25 2.15 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.05)
		(thermal_bridge_angle 45)
		(uuid "c7a30654-15f0-48ae-82d1-40a8bdbfe06e")
	)
	(pad "21" smd roundrect
		(at -0.003683 -0.003549 90)
		(size 3.05 2.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.0243902439)
		(solder_mask_margin 0.05)
		(thermal_bridge_angle 45)
		(uuid "09c0f58a-d86b-4ea8-8ab5-7273cb1d943a")
	)
	(pad "21" thru_hole circle
		(at 0 -1.25 90)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.05)
		(uuid "abbf6fb2-216c-413b-9f5e-bdab3dbd7c57")
	)
	(pad "21" thru_hole circle
		(at 0 -0.5 90)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.05)
		(uuid "5f2a8347-33af-4506-bb8a-344db245e0e0")
	)
	(pad "21" smd rect
		(at 0 0 90)
		(size 3.85 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(thermal_bridge_angle 45)
		(uuid "e9252321-eeeb-4327-9a52-5f3d7f0a05ae")
	)
	(pad "21" thru_hole circle
		(at 0 0.5 90)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.05)
		(uuid "0c568fcd-a1a6-4cc6-901e-1e24b2f20543")
	)
	(pad "21" thru_hole circle
		(at 0 1.25 90)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.05)
		(uuid "f4f5d0cb-cca6-4c78-9132-6dc66b35c30d")
	)
	(pad "21" smd roundrect
		(at 0.25 -2.15 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.05)
		(thermal_bridge_angle 45)
		(uuid "e2e1f32a-5ecf-4cd1-979e-bb5a2b2d06ef")
	)
	(pad "21" smd roundrect
		(at 0.25 2.15 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.05)
		(thermal_bridge_angle 45)
		(uuid "065708c6-f8b1-48e2-a2d8-ae8687564ac4")
	)
	(pad "21" thru_hole circle
		(at 0.75 -0.5 90)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.05)
		(uuid "74490d3c-2f3a-44f0-8081-8c146dca7c13")
	)
	(pad "21" thru_hole circle
		(at 0.75 0.5 90)
		(size 0.4 0.4)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.05)
		(uuid "2c14fc0e-8ac6-420d-98a1-5f71c3f9b82e")
	)
	(embedded_fonts no)
)
