(footprint "QFN-10_EP_2x2mm_Pitch0.4mm_EP0.9x1.5mm"
	(version 20241228)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
		(uuid "fe472ed4-8001-4c59-a7bc-a3d18e88302d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "QFN-10_EP_2x2mm_Pitch0.4mm_EP0.9x1.5mm"
		(at 0 2.5 0)
		(layer "F.Fab")
		(uuid "8734a986-f4e9-40a4-b2df-57f46eeff446")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "fa872d58-f6b2-4987-aef8-699c0e633588")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "01f58471-3f6a-40d9-b48b-7ec003138ffa")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.15 -1.15)
		(end 1.15 -1.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fb6d5766-060f-4ff6-bc52-e7412487f585")
	)
	(fp_line
		(start -1.15 1.15)
		(end 1.15 1.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8641e07f-e988-4e9f-8314-d40955f73253")
	)
	(fp_line
		(start -1.15 1.2)
		(end -1.15 1.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "16dd474d-d294-46d5-a2bc-6494f79bea17")
	)
	(fp_line
		(start 1.15 -1.15)
		(end 1.15 -1.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9265c9fd-d928-47b7-bfae-26c2ef5211a9")
	)
	(fp_line
		(start 1.15 1.15)
		(end 1.15 1.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "44767928-f2e0-4971-8d46-c5d31ed63be2")
	)
	(fp_line
		(start -1.5 -1.5)
		(end 1.5 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "af5bfc51-0b03-48ce-95f4-b5b16a7b6be3")
	)
	(fp_line
		(start -1.5 1.5)
		(end -1.5 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "004ee1fd-9b48-4213-9314-75ddd9e132cc")
	)
	(fp_line
		(start 1.5 -1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c725f3ef-604d-4e85-94c3-5cebc5ba05c0")
	)
	(fp_line
		(start 1.5 1.5)
		(end -1.5 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4814bccc-e6de-4f79-a5e6-dbee29e98f3b")
	)
	(fp_line
		(start -1 0)
		(end -1 1)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "306ab394-33b0-4f81-9189-3e30022dde1e")
	)
	(fp_line
		(start -1 1)
		(end 1 1)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "b58e0fae-3284-47a4-b74b-9a8aef47642c")
	)
	(fp_line
		(start 0 -1)
		(end -1 0)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "7e1adc9c-5a8f-4a92-9006-97f02172ad41")
	)
	(fp_line
		(start 1 -1)
		(end 0 -1)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "8dcaa787-d60c-49ca-b779-06fa0c3951d2")
	)
	(fp_line
		(start 1 1)
		(end 1 -1)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "33318e10-d70c-422e-92f8-2503b345728f")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "e519bda7-8e37-451c-b8c0-be9fbcd457ac")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd rect
		(at -0.225 -0.5)
		(size 0.000001 0.050001)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "d8535d8d-2846-4e99-9d3c-8d1ed6777d43")
	)
	(pad "" smd rect
		(at -0.225 0)
		(size 0.000001 0.050001)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "0e12f920-f43c-4f6d-8a16-3c4a4c9f1db6")
	)
	(pad "" smd rect
		(at -0.225 0.5)
		(size 0.000001 0.050001)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "526d6021-9cbc-4551-9839-8645e3948532")
	)
	(pad "" smd rect
		(at 0.225 -0.5)
		(size 0.000001 0.050001)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "3774c0ef-1ce9-4b52-bf04-1414fa0f0199")
	)
	(pad "" smd rect
		(at 0.225 0)
		(size 0.000001 0.050001)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f6f9171c-efea-4dc7-ab9a-61747a4b0fa0")
	)
	(pad "" smd rect
		(at 0.225 0.5)
		(size 0.000001 0.050001)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "3181e8ef-1405-4753-8a34-e6dc63167601")
	)
	(pad "1" smd rect
		(at -0.95 -0.8 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "2dc0bac6-dd34-444b-9a45-aad16638a0c7")
	)
	(pad "2" smd rect
		(at -0.95 -0.4 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "d5a9ec53-70bd-4b47-8420-0c757b44169d")
	)
	(pad "3" smd rect
		(at -0.95 0 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "9e87cbda-e3b4-47d7-a0c5-dff73236f75d")
	)
	(pad "4" smd rect
		(at -0.95 0.4 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "7a810a8e-ba30-4726-8253-0441eae3fa36")
	)
	(pad "5" smd rect
		(at -0.95 0.8 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "d507ad8f-f366-40d9-8da7-120e3bfd08f7")
	)
	(pad "6" smd rect
		(at 0.95 0.8 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "61e0e995-516b-445c-823e-fdcfd604197e")
	)
	(pad "7" smd rect
		(at 0.95 0.4 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "178355de-30a2-4520-ab32-354d5b92b586")
	)
	(pad "8" smd rect
		(at 0.95 0 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a0c0600d-ff5d-4208-8c4c-10565de756d5")
	)
	(pad "9" smd rect
		(at 0.95 -0.4 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a855698e-8bb4-4752-bb4e-b9cdf78facf8")
	)
	(pad "10" smd rect
		(at 0.95 -0.8 90)
		(size 0.2 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "4d520805-7fda-4102-87b0-7d5e7c3a7421")
	)
	(pad "11" thru_hole circle
		(at 0 -0.25)
		(size 0.225 0.225)
		(drill 0.1125)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3b2cee92-be83-4071-b78f-1946dd598a65")
	)
	(pad "11" smd rect
		(at 0 0)
		(size 0.9 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ab1bae3a-3d42-432d-ac62-46e48bf4c225")
	)
	(pad "11" thru_hole circle
		(at 0 0.25)
		(size 0.225 0.225)
		(drill 0.1125)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "feb77a93-d5fa-40af-b26e-fd02ed9937d9")
	)
	(embedded_fonts no)
)
