(kicad_pcb (version 20201002) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (grid_origin 150 100)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber")
    )
  )


  (net 0 "")

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 03f0c419-f363-4824-9c5b-72a0ef71f2ed)
    (at 170.32 11.1)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3aa4a531-174f-40df-a615-534aba2c521e)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 786e73ca-9dcd-44a8-bf1c-e11e2c4d51d1)
    )
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 18a7a44b-e345-45e6-84cb-2222c0bb5f00))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1ac8e08a-b284-47fa-a582-9b0e482f5e47))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6ec61821-f288-49a8-a6c9-bfc1177b36c6))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c370503-9de0-4bcd-8449-13022b5b6b4b))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec20d7f3-5124-42fc-9179-7eee823b6d37))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6539191a-4324-4df8-8527-e1eb817646bc))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b7dfed7c-7737-4bd7-a8aa-50ceac74061a))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c21e3d31-e8f9-40a2-92a7-6489d8c85870))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ea42f2b1-9ecc-4f99-97ad-da5dc7ec1f87))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f0ad05f2-9dd5-4979-aa8d-bed15c5168ba))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3a3491db-936d-44b0-904d-940cfd2923d8))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 981d7af5-40cf-433c-b99d-54819bf41a6e))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 99ae2f98-b57d-4e51-b824-52a4937b3890))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9b809df6-79c6-437f-8b31-fcc4209aa7a3))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c1788fad-5d9f-49b5-9496-7d58ff4b0229))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00e39fd3-ee0e-4104-bdd8-18f07c7b6f7e))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 49362393-9ee3-4659-8eb4-642721e2c0d3))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 75d21d1d-07e1-4882-83d3-58268e2a8efc))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e87f81c-6e19-43d5-a5b5-1c35fd5292dc))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ef6d101-6e98-4e70-b948-4b481f6c8361))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 048743f5-ac50-4515-b2d0-4cef68893cc3))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0746267b-b84b-428e-b24e-f32d3b410886))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 504c43f7-472a-4d07-92aa-208d07573b01))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 583fbdc0-0ac0-4107-816a-c3a0bae6dd12))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp acbd6c8f-f9cf-4dc9-b7dc-c24c741917ef))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 085d434f-68e2-4d8d-9f68-8b81b058a7d2)
    (at 171.59 27.61)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0655dc92-4701-49ff-b6e7-6fa8a0339a9d)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1f7a0f4d-adc1-4188-bce2-a907a9e46513)
    )
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0944a6e1-5266-46cf-a902-9e8ce62d3ab1))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3250dcf6-835a-4d98-ab3b-75edd0ae3425))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 77b4bdee-7d81-4b7f-a933-0156257276a6))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7f5801bf-8f0c-4ff8-97b3-637295853b58))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 848c08e9-7b28-4d68-bc17-c68a0a9a6a46))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0fd97762-2f12-4799-8f1a-53333a743052))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 12d3eaba-d285-4479-9f36-6a3674302e5b))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 66eec086-1a76-4a2f-85dc-3672e1c6a32e))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 714b2999-d759-448d-9c11-58c5e515564a))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp baea2a64-ab24-44eb-86f3-420d20b7cc1d))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b65f3aa-e822-4934-bbd1-ce8e9cf806b2))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 85355cb5-4119-4198-868c-1218224151c2))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8c65f997-3d41-495f-86b3-a5312985130d))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bf2c0d10-cf7a-49ff-af96-a2aa2e84b37d))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e6e5dd5c-1cb8-436c-82c4-59b0560f6a3d))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2b59891c-a58f-4125-84d9-e5c7078b9dc9))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8f2b36a7-2123-466a-b45c-87f4af65b2d9))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c28a71a5-889a-470f-b988-26fa224b9b9c))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c33671c5-cf1f-44a2-a649-4272e52b56d1))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e6309315-9e4c-48e2-ba55-d010d06fa39f))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1529c766-49c8-44d8-8c9f-58e85773780c))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4217df6b-fa7a-42bb-9d88-f835b6c0cadd))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 655ad5c1-ea9d-465f-81f2-c7f4c2baf401))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aba8524f-8810-40fc-b07f-4dd5625d9600))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b07ed2e2-3399-434a-8e7b-d48c63fe8ef5))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 0e32df20-9abb-462d-a381-236ebabbfafd)
    (at 174.13 39.04)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 665710d5-73bc-4ba6-a1d7-9f42909a5cd5)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 828705c7-630b-45b7-814e-f11c0647c666)
    )
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 46e28d97-89be-4136-a9ad-2d2dcdcc8890))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 635097c4-f3cf-4442-b11e-c1009ed8c448))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 668d9a0c-15ce-4383-8817-3d122d7add34))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 702ce7c7-4903-40d4-863d-dea79acd7433))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4663dc4-3073-4395-898d-6f8710c64d1b))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 40b4cbd0-1a06-43f3-b92f-816153892fc8))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7b0ed724-976b-412b-9966-96750da26b6e))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 80626cc3-b6fe-40f0-8157-d41431e6c055))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 888e8974-ad9a-475e-b13d-d7868d402edd))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp db24139d-5797-424d-9b1c-c5f79af6362c))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 249a038b-ec0e-4a85-908b-a7e500306354))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 48c4c938-b4e7-4e9b-bf3b-a33bc15b3d3c))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c2c63d8-0256-484c-8955-1631f9fd20da))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f610b21-67dc-426e-bb21-120b44218490))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e51f51e1-1dbb-4ac3-9ec3-2ff65393876b))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 518d0e56-667d-423d-b9f8-9dd39bf37834))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a3b53382-73cf-4a07-b3cf-e7edb2435c38))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cd00ec60-8c2e-47c0-a5b3-4e636d9d81f8))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e8a72c6a-0d57-4caa-8480-1bf453495af0))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ea113bae-69e7-4d64-afc8-eda3d2d891bb))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2aee3699-dfba-45e9-b5ce-24830d0f5d15))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 450b2c83-a127-4c4e-ba76-034320aa1cb3))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4b252515-c286-494b-800e-44dbcf2ebcd7))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5abcd5a7-0900-48ba-9647-95f638a64b08))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ffe8dc07-1eee-4615-8a52-7fdcb7cf5cfe))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 10aaa1af-7fd1-4708-80f3-b832c3924c91)
    (at 171.59 39.04)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3e424c74-f68d-4fa7-9a54-ae6e4a1da639)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1c2b2237-d895-4751-b233-73a7f7fd6d31)
    )
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 07180455-87dc-4c31-a250-c87757ed20ed))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9cd0fd3d-3827-44f4-bb0e-df906cbd9419))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp abe83d8f-8452-461c-8570-ecf32425b076))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c241183f-f6b2-401e-89e8-85ba9de09a5d))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec7dacfb-bac7-4c43-adc7-fb9d0b60ca4c))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 086b6ea5-3d9e-42a4-bceb-3c4066396f9f))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e482678-0f5d-4187-b4d5-2e1741ab8713))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c7d3ed1-20c2-4bcf-8c19-e80f65c1f241))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 98bef87c-a775-4644-bf1f-e24e68acecee))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c568bf87-bbb1-46d3-a086-3a5d1161564c))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 51b2d005-cf6f-4f68-9517-35da5c11055d))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 72fa2973-d941-4146-b403-50bbb396e1ad))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a623cfd6-e497-4345-8687-90c567b8a661))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aeee6b56-30da-4458-98f5-cc12752cb69d))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ddf5c9bc-3864-4f3a-9511-60ebf7affaf6))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c598646-c88b-4404-94e3-1810ada8df03))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 98006e97-6b5e-4ebe-8d9b-2bcfd6d16218))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a9b37bae-4392-4d3d-aab5-70f9b188d49a))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d470f8c3-f56b-44d7-8dc0-f1c94bfe8886))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dc582a81-7cd1-4365-ad3d-2312585939ff))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 260c3dce-bad0-4099-aec3-cdf2f7be1f4a))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 78eaf93a-d1d5-47c9-b936-57b95cc3870e))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d61710e-8fa4-4973-b3c3-aae639f29dc7))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f3788fe4-a6de-44b8-b66a-eec6f09b23ef))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fae05ebd-a0f2-4cad-87ae-a6058e61adbf))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 10e2a474-9ba5-4941-b134-7fe570b9e7fb)
    (at 174.13 21.26)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 88a58684-fcab-44c0-8608-716fd0073cbd)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dd97102e-81ab-406a-a0ba-fa154e61c3be)
    )
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2a0c2d83-d254-4245-8335-06f59bba1643))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5d849785-80bc-4cda-add1-31dd72ddd982))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 90b2836e-9e8e-4e51-b3a6-4c57740c3f1a))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 94fe16d0-b6f7-4dde-a597-850268153d42))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a9341829-9a49-49c2-9f11-2e40def91c5b))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4ffc2a39-0d42-417d-a4b9-9982ea0a4000))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 827f7fde-11f9-4d99-ba8a-6dae0ea8b90f))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac557443-e50c-4c05-8dbf-e4f05c29be3f))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1fd9ea5-2808-45dc-88af-4443566a2aef))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fdbca049-af23-46da-b16f-9a9e76d5de26))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 196d56c9-e88b-48f5-b974-c5a0f94725dd))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 44fee735-2033-4d78-832b-67a6e3447e16))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 60857d62-c0fc-4737-b70e-6fad9cffbaf4))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 709d4693-705e-4d82-bb6d-cbc7d69f31c1))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a9081254-3eb8-4e11-910e-61d3ab8e4c8a))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0cd3d78d-47df-4972-adde-cb8da5b199da))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0d8494ce-aa68-4046-9620-8c9156c44b8c))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1f1f5d71-545c-416f-83d5-f8ea2bd06c33))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e1839f1f-d9d7-406d-b329-dd99df814674))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp faad712a-dd02-41be-aeea-36bec58c729a))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 71d57281-9f6d-4bcd-9efc-0c3141c5556c))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 747e2f2c-a6fe-4297-8736-e23f6531a037))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac9b55df-a296-490a-8ab2-e70652b4dc23))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c0d3db2d-876d-48b5-a20a-27c8cafcc945))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dba1d54d-8c9d-4de5-9479-f7ce8a519339))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 17dd19ff-e834-497a-a6bd-3f02257a9e94)
    (at 160.16 61.9)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1752b182-0bdb-415f-b27a-655a7f0f8b17)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bb1e07ef-19fd-425f-ae96-d69cf6d24bbd)
    )
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 098f7862-8bf2-4f01-9aae-cde3924aa4da))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4e35006e-031b-4154-a8d6-312231d8b3be))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 939ce3f9-2c5a-466e-8025-05a8e17768e1))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a52ccc0e-aba9-4ae4-8c26-18eb6abe1149))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp db6c2201-1bd8-411a-a392-437e6d816f3b))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 21f3e78a-35db-4ee7-bc6f-81bf86447e1b))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37bee6d6-fb30-4123-9c6b-57c7053fd961))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 92b2c829-4359-47ae-841e-47a716ba267f))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c483544f-1fd2-474e-b3bf-09b7b34fb76d))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d59f5c4a-7478-402f-85f6-ea4ec8a4c53b))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5645c4e3-c66a-4b64-9f4c-a72ac80f663a))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 900ccf9c-8530-4c10-9741-7acf344f4981))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb9cb026-6d80-4ba4-901a-1e011fe555f2))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d86e45ab-8ffc-4394-988b-17d25e5331d6))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp db772ed4-cb6c-4b6f-8e52-f2a9ff8a16c9))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 04c557b1-2e26-4a02-b9f5-08eb7dd185a4))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4523ee3e-7097-4385-8143-1e5058622d72))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6562b2a3-a573-47eb-9282-94d5fa33775e))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 941774e3-8e63-4e6a-963b-02db342954ca))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e35050b0-2373-47f0-9424-bfba2eb31670))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1f7b565a-c87c-4754-817c-8cc367cc9b52))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 301293ad-c71a-4ba7-9f85-135562f2354d))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 51f1e8d9-262e-4047-9b9a-76064379cfff))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 744961df-e016-4289-9d50-d3a9b11245d8))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8be80915-e84d-41e9-a790-57b368de933f))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 19652673-011b-4df6-bb8e-c2d31692a4d4)
    (at 152.54 0.94)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3ae3316f-e367-43f3-8f29-1e41f48e4ddf)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7c3f9a1e-934d-4009-90be-1c605a95d3d7)
    )
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0ac65d9c-269e-4869-ba52-a60d17be49a6))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e4f391e-d722-444c-b063-810f81232a57))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c0e853a-c789-4815-9e72-78a63573fa91))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c0375e5d-25a5-42ae-a5d9-f671f0ab3918))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d96def9f-2de9-408c-a0e1-fc599318f272))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 51eeeae0-cec5-43d5-af41-ecdea5e39cbd))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 53d2aac5-1723-48e1-a774-2e871669403b))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6d729fe0-2895-4e8c-b0a0-6b1da2257d43))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e32e51fd-3545-4f3f-a50e-4371383951f3))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fea98a7a-2b92-49e9-99bf-b087749148db))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2cf6336e-3142-42ae-815e-678ca2d9b5d5))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3658c0d7-b4a5-44bd-b03f-df93a92e4bfd))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 610db5a7-f191-4a34-b7be-4218b28b05bf))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d5cb14e3-b922-4348-8bcc-31b4370b9825))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8d5556a-7f35-4be7-bc82-e4c1c6fd99f1))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 18c26aad-c2de-4c00-93af-f953bdc733f0))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6476dc35-423d-40db-b912-c85fc9c278d4))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 905c7ee9-1292-418c-a658-ffab24ece730))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b54f82e3-7aba-46b9-971b-0cde82be73f5))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eee838b9-0962-4e7e-b9c4-216428d6351d))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2cee396a-62c9-4409-b8c3-1f4e68a3b8b2))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7a34d072-b503-4526-a3e7-b55db5855615))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 820ea043-016d-4be4-85b0-bffc740e7ead))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7ccc5bc-7911-4cae-b180-e855534b9cb7))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ad9fd838-1eb2-48b5-bd73-27532bfc38e0))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 232d1987-5de4-481e-a07b-bd5d87250007)
    (at 155.08 49.2)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7bc05c3d-a160-43f2-bd0d-c37719d3f3dc)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2cf439d4-d9ce-400e-8489-da6db2f58845)
    )
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b85bb01-e00a-481a-90c8-7450918a0339))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6e78aefc-32aa-41aa-84ca-b516e5f97b0f))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 78416a31-b4fd-49e7-a73f-96e4c3573cee))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e3f4242-719f-411d-bb56-3fd18f58214f))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9ab5449b-7695-4aa3-8881-dd62cab06d4a))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 45f0ae3a-07a3-4c8f-b4fa-94dbe7c5b1e9))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8bfe4a0b-e6f1-4090-b85e-3474175e7528))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a22297b2-77e4-4110-95f9-eb8ef2ab14b8))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp acc68b71-4e45-45aa-bb9f-06c90cc71144))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1606d06-fb12-404b-82dc-54a3447d0b0f))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0059abba-1f4f-406a-83ec-18a9316a678d))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 152773c9-be5c-423d-a236-c0a17bb72154))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50fd87c4-0eac-4c66-b764-78df4a45942a))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c16509f-a1c2-4f5f-ab4c-b5a496dec1fa))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 89e1cf6c-3974-4f93-a80a-9ced1707dcd2))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 143a1a26-717e-4713-b147-e1790cd93454))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8fdd5a1f-a189-4a47-b0a6-74a6e42143d0))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 945abe48-f780-43b5-bab1-b9a26cd9829f))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9ccd846e-3c9a-4fc6-9680-e50a8260bac3))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ad914954-7b0e-450a-930a-0eae8939ff77))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 68defd8a-87fa-489d-a48e-850cf727f579))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7983013a-3d03-4964-b5a7-1d207fd127e6))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a36f252a-14f4-46fe-b277-a05c0e7a40be))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e4ee97a8-7145-4894-8a03-96fe5673ed02))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eab5cd3c-9de9-4983-b172-584eb5c5f322))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 23e16ae1-22f2-449f-9984-a97860da898f)
    (at 160.16 6.02)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e81768c2-9d25-401b-b1ef-19dffa1078b6)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f6fb672d-7927-4165-b85b-a39795e142af)
    )
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 194971c7-516f-4041-b1f0-4c489229d03c))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 46914a0d-415c-4194-a3ed-f2dea8324258))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 819052f9-fbdc-4a8c-b33f-8fba90dcc210))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be74010e-9db4-4291-873c-160137bdb523))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fde95c02-32ad-47e9-bc86-a05b52a2e2ba))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1cb2d554-7453-494c-aa22-ac08db0676b4))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e1ecdc2-b2e3-4afe-8fe2-462cf403755c))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c4e753b8-1c6a-4f23-8ea0-371bfdad440a))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ebc64cb9-b9a3-4124-a4e6-6b616560ee23))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f32ba006-da1a-4dd5-8fd2-d0b2d83c7b78))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2851d831-2872-46ab-bccb-93c9ee6a0271))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 29e74bda-669c-4cf4-9674-e8aebc0e8613))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 61133197-f3a5-435c-a750-e6748ec09bee))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8f111770-f0b5-407a-bbea-f2e85e1c2edd))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aa942447-fe04-408d-850b-aadaedfabf37))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3e674e8a-6f30-4ff3-9ea7-cf34c4a36f62))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 407a007c-50c9-4558-a989-bfe7a39dfb17))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 496c9038-622a-4d69-a326-bdd640e17d05))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c4390ec1-bb00-428d-a684-39e9f020d9f1))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8d219ac-8b04-46af-9e66-a787c29c6f14))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 746f0e0e-cc5e-47ce-80a4-faf5f28ae768))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b522f9c7-a3c0-4f96-b2e3-6d89ac73d676))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ca419a94-1404-4c3f-a378-f7a75fda1fdb))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cbabfc53-0704-4194-bb24-52bc1ce01a48))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f100f850-c8e2-495f-8b3c-1cb3ee35c3ac))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 25e7b2b9-2214-4a15-af86-cec99311dbfd)
    (at 165.24 39.04)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 15da96ee-cec9-4b1a-9ffa-3ffdc3b01262)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 097a194e-9f95-4b0e-9864-7fb936b1a32d)
    )
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e46dc16-08d9-4a40-ac06-adf527cd4a1f))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 24dd7539-7be4-4025-8365-af2b1f2f5b78))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 734d37eb-c95c-4eba-97a6-f47cf236af5f))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e1517cbc-fab4-457d-81ae-3d161bfc3d15))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f9642719-b6a5-4368-8bfe-8dc6f04fdf4f))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6640e94a-2a48-4f3e-bf0c-6c40857d9cb9))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7546dc0a-1cf3-4749-8a90-b98765db0fda))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 84078e1a-5c7d-42e7-954e-a44c4ca2316c))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b465589d-3117-47db-b8f2-c6d2f3a9ef81))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bc0b7302-35da-4b1d-a28b-0c6bef9735ef))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 58738654-25ee-40f2-af04-c7be7055e058))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5fc0f046-7cae-488c-97e8-40aa9b5c9e75))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb028fb1-766e-42bc-a5b8-092585fe6b26))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fa21216d-2abb-4e91-b6d3-6a88af88a0ff))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff94426f-5ce6-4ea4-a463-f39f9219f06a))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 14861e64-182e-46e1-bd60-a61b670e1486))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 56a0bef0-22ec-44f5-99d8-f12de146ea40))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 605b7f7b-ceaa-45c8-bceb-b82a8eded75e))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8cab561e-3ba0-4960-ae1d-7304a9861ba2))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a5e57c74-379e-4f34-bdef-3156fd345d6e))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 159ac4d0-fd43-4979-b0d2-000a25cafd0a))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1e31838c-fdd6-4794-8838-acca045352ef))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8746c171-ccc4-4df0-8c4d-52136d4aa356))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bfd12eda-f5d4-483d-b608-59a660c06d29))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d377fd42-4844-4d69-8f02-2379a4e89ef5))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 2994418c-8e49-4cbb-8a81-e7e2f12b3abc)
    (at 147.46 84.76)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9706196e-d061-49be-a0dc-e81c1f0f198d)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 79275e73-b13c-41ec-865f-3f63d2c80907)
    )
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5957dd2a-5fb6-44fd-96af-cf44766f35c5))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7d26bfc-5e96-4a61-bbd7-9fd2a392b094))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b34bed96-02b3-4943-8a4f-f38086d65615))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bade0780-9fa8-4851-83b2-eb1b518ca26c))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d64b9015-b6ec-481f-96c3-a9bab4f8cb04))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3937ef0b-2a85-4bc5-ad4c-c2501368effb))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4599a44e-741f-402e-8672-75cffa4751bb))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5c7f024d-d922-40de-9c2e-828706b0b382))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 641b940d-fac9-4809-9f2e-4b68851e7b76))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9a80b417-90d4-40fe-9de1-391307544ee3))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 10c8043b-bf32-4333-a312-b59579d7ddce))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 38026098-9554-4e3c-a4f8-594d0f0d23f2))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4c231102-bb2f-4f15-96e8-4dda912756b9))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8914062d-7d6a-46bf-b319-0be1432160cc))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c0ff44a2-c84c-4775-ae86-f53e5c87d0fa))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0d7a8b21-886f-4a8e-a3bd-23a69d0ebab0))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 158d8c0b-f0a7-40c4-886d-58a34c89dcc2))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 356e48cd-08a9-44e3-ba2c-6a103e3a0cb8))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8aa94e20-1bf7-428d-8d5c-dff1f99c63ba))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dac7f890-833a-410e-ac46-037c882c8c13))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5bafe53d-a2c6-470c-97a8-0a720c89bb0f))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5f273412-29de-48b0-8ff5-dbbd3be9b03f))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6db7a9af-4b0c-438e-ba7a-e815d5bcc1e7))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 83dafadb-702f-4bc2-86b8-7d1a13e2d7d1))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f9941ba4-a25d-4476-a50d-b0535ff90e49))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 2ea9fcdf-9d90-49d1-b1d4-34787ccd4bd9)
    (at 167.78 11.1)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bc919939-db3a-4510-94d5-64f7bf1cf8c7)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1c2e4edb-e0f2-469d-a2d7-3e476ad734e9)
    )
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2c76df36-b2d4-421a-acaf-d321b34d9642))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96e49369-b5c5-4939-923d-2d87006aceee))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ab31829b-ced9-4a82-b61f-4c2914dd01c5))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ae41f2e6-8bb5-4bcd-93ea-a1a9dd91821b))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b6c9847b-f758-437b-bb64-74cbaa38d7bb))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 18f8febf-a4a9-4c04-a906-bd26402c494f))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1c8f3b6a-3369-4e3b-813e-60c30adf7fd7))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 49453f44-79b1-453c-bee4-612b5c0e1c38))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a4cc0751-8b93-469b-995c-d4a6be759b79))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c6dfa0d2-366a-433a-aa57-708ce1110f6c))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 02f2e8f6-0e7a-4d65-a93b-3aec9bef82c7))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 32596fe5-1e78-4237-897c-a5d403d44642))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 65ec2425-ea74-4f08-8e9f-23c947c22f07))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 89c264bb-fcad-4831-b899-20d10ad52fdf))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dc8f2ce9-c5c5-4828-9687-05b0c001588d))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 06486a10-e85e-4b34-93ad-ce8e44b2bd37))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3cb7e159-ca72-4f01-80cd-ac1bbbd15584))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8f30e061-3bfe-4d79-b870-2ebf36f91bf1))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9c268eee-e2ea-49f4-ab0b-2e2f9d5ea067))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f928b63c-2e6c-41c5-9948-4f227ff8394e))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 07b84644-087a-46cd-a9fa-b457e61d1482))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b3985f1-9655-48d0-92b0-ecf096fdcd39))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 585a2543-0f87-434c-b32b-5e4815e5327f))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 65c6e449-00b5-44d0-984e-1c2595e85cf6))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a4426825-ecec-43ef-878e-5e1d9d956353))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 32c2f019-8544-40a2-8bd2-7e85e847b950)
    (at 142.38 23.8)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 910e776d-956e-46a7-a7df-8ebeeb74fe18)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8030d733-55df-48e4-8229-f7031f7c951b)
    )
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 51ae50f7-719e-4626-94cb-b92ee1371ed7))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6415d0ad-b5d3-4eb0-9d67-ec4e19c82339))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a2f76e93-ccbf-4737-b976-c2656f3eb5f6))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c8a2fa6e-bd69-40a2-9602-3767bae2c7c3))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d383ef36-7abd-4af4-9657-f2ca518416ac))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 32f54336-f174-4866-a1e7-052c6a63023e))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a9697ab-7bb6-495b-951f-0e0f6d9cd0ef))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50cddeeb-6552-45d5-b867-21363f2b430c))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5fcc15f9-7d5a-4ac8-a8f0-f2e87a9bbc75))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a972d7ca-c942-45bd-bc5d-c8682830a201))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3d7d9b91-41a7-43f1-93be-6f7c9eae1899))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 790d7e90-43c9-4ddb-a95c-dd7a566f6266))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f283dbb5-88d3-4146-91a2-dbae648a3ad0))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc4247a6-464a-420e-a80f-9778dc8e1373))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fe67a3bf-a02d-4f41-9c70-a16c63e0f74d))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37afc28d-d1c1-4ba1-a914-74e76464a35e))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52da9292-c52c-4af0-bfe7-db45f6cd160d))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 82cb869e-9aba-46df-88c6-3943ee35558d))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9617a80c-f1a5-4c17-91a7-fc01d6964249))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8899502-a7e1-442b-90e7-d5bceb793ec0))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1a32e4ec-4d28-445b-85db-d1650bc3708f))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 49831754-1c6a-4357-bc9f-81272ae8633f))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b74ab8f5-29b3-47a8-8737-6b6ae01dc48f))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp da0a92f1-ab52-48c7-90cd-80a9c075f8f6))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f2e9e9ee-d203-4f45-a741-5c27c56a0776))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 3f10576a-2427-4864-a088-c6068b6ce1ca)
    (at 174.13 33.96)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cf7b9483-3f6b-4e2b-9f3e-94c6ffab8e28)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7b56fb94-ea2c-4869-988e-c117789681df)
    )
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 050409ec-bafd-4e69-a0c3-dde8f6b54fa0))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2a47f57e-e355-4d23-b70d-677769fe4c39))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6b07581b-9808-4c07-8871-d236d228386c))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 787123e3-e22b-4730-ba1c-70b748664c55))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff89f8cd-324b-4f8a-9a24-7b3710ae431e))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 02117245-bc22-4fdc-84b7-0021ece30e60))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0c74e262-4407-437f-a4ac-db28fd926d08))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cfc0324e-72eb-4968-8458-a1d972cf3973))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f015f177-0b88-43d8-8be1-788e3e0246b7))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fd48bc2a-74c6-417c-810d-7ddc0de1d8d1))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 319a1f55-63ac-43ab-a46c-faa17b6d4028))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 495123bf-4aeb-4f32-a649-7ba32115cab8))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9bdc0194-983b-414d-8ec0-cef1fd93480b))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb7d257c-332f-4fec-aec8-ea58c2c26752))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c72c5add-7969-4895-8844-7e5d4b283f43))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 007b0d24-21a6-4e5c-8258-8cd38486df61))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2271fabd-2f31-4888-a580-6440e60571bc))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52125a6c-cb52-4fda-a149-994642b7ca51))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ee513f9-772b-4c89-866a-4399f3ff2871))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8b01b4b2-128d-49cb-b31e-cc2543074928))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 07863043-41c5-4303-8f09-3d65b735837c))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3840f8d2-bdbb-4469-b480-e6307bd6b5a3))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 946de5c7-a794-4d9c-bcf9-f163f2cfe690))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aef6ad56-fd73-4681-9cc8-e940c806b433))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cbbf069a-036e-4a1f-952e-70e55104d1f2))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 3f1c58bc-74f9-480c-9239-7ac362554794)
    (at 157.62 49.2)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3fff5b0d-299f-4a1b-aa45-aa24f96a1e8f)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 025a91a3-4eaa-4170-98b3-e82bfeb6a23a)
    )
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 06a994ca-b2f1-4e3d-97fc-ba7909c5b03a))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 08a08014-ae3e-4e31-8508-5544391f17ed))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d7ba4d7-c0f0-443c-ae10-11854673465e))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b53efc9f-5c6b-46b5-97cc-055d4a8fa517))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp febda7e6-8892-40ad-a2d8-2d1098b78f60))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 080d65cd-9d2b-4a91-ad10-449e429e2f82))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3643046e-25ec-4cd8-9b82-14005069fade))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e2f072e-b52f-4edd-978f-dae2389b1dce))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c13f7da5-31d3-4980-8b29-5b05bf73905a))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f30d0cdc-b1e5-4a1d-99a3-2297fcde2e30))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 25d60a1a-d34c-4c3a-a31f-24da0147a436))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 512c382a-9856-4034-905e-07c6c09c5bf1))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7b7bf1e-74d5-437a-93ce-c3a89652b27a))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ddb36946-1244-4a87-8880-18e90d420aea))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec3f8b03-6e20-476f-b4fe-02bc73821029))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3506719a-bd75-418b-8432-1fcb6f01b89a))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5eb045fd-35d4-4d16-95fe-d7ad2e7825dc))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a168185f-5644-4852-990f-dca4f763a53e))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c32a5457-5e67-4eca-97e6-6e8975422103))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cb9ffa35-d004-4f6a-8cbb-412564cbf873))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 23b7bf0b-3183-4396-b1d4-6908c0915e73))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 346d7a81-dc0f-4c40-84ba-f7c97280484a))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac74758e-0cf0-43bc-9ece-de8824b06159))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d2c58fa4-0e81-4a95-ab6f-2308cc0a5a63))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d9814c2a-402e-4565-bc3d-c56a91b476e0))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 403baa3c-cd47-42e3-ad78-52fa5a2b628d)
    (at 158.89 27.61)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 71087712-f21f-4d55-8de8-b0e6070dd28c)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a1aa8ea6-dc85-4f4c-9e50-2b101bb7fd8b)
    )
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 302dee5f-fab4-44d7-a9bf-f4cba8efc64f))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5fe937a0-265e-48c8-b424-477fd07e001a))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4667116-ca55-444c-b0c5-2afc75f1448f))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ed983960-34aa-437f-958c-d060fd06f858))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fcd0b522-b8f0-4fb3-90b1-27ac8cd9a7ae))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 25154e03-ec17-45ee-b721-ace5370ee622))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2ad57143-f044-433c-bfe1-bac34585e5a7))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 597cddd0-8138-4263-b542-fb20cf13c96b))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5c8a21b1-aa55-44b6-b2c1-2cbd31a22359))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6cf1b4e9-c5ba-4634-bcdb-70b1510ccabf))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b859cd8e-7551-4a70-9d7f-037cacbe60a9))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c6ed8cab-45e0-479e-b831-e9e4e1dc5cb4))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d746ece6-c367-4c45-820f-3b2e6a5a52a8))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ed15e707-02c4-49d9-8a62-2eea3edaf5e1))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fee62906-971d-4280-8fd4-92490ea31827))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 13657812-a757-47f6-816f-64b392099f04))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 955a8dfc-0897-4c41-9726-00cc9a232238))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96da91c3-a63d-4a23-8675-6155ed4daa30))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bab8e3b6-fc86-4814-a687-b99e38167384))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e86e070e-12e0-4111-a994-bfb8292555c9))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 050038f1-f52a-4c10-937f-fd102325bd9f))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 086e4f49-7d12-47ee-8aca-90836a1a0721))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5bd3ee48-b89d-4afd-8b1e-8f891fe6d99e))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e90186a1-f0f2-4159-98a5-3219faf6bed0))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec50fc6e-e0b8-472c-84bb-6f5d4c4c7984))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 40b9243d-048d-4cf6-a53f-c60bbab120f7)
    (at 170.32 49.2)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3d15840f-62a6-4560-b033-bc081ce8a2bc)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13de297b-d5fa-4d8a-af17-d10a0ce0449e)
    )
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2db8dc37-6ec8-4ffd-94b5-d87b2e8d7e7b))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3542b3ae-916f-425d-b5e5-0bbe5be48f62))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5db88fa4-1232-4a43-8e96-b5d78a07c889))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bcf2d839-7b3f-4fbd-a8f4-f8d8ed0db7c2))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e10a0d1c-5053-4d36-9c76-136c47e8db88))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a04e9e7-9cf5-4adf-8661-beb9ac144ba9))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5de87f97-179b-4389-bf3a-0b4e9210f567))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ad87f4d-5848-401b-9dc5-872d6221d110))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8a3008fb-0a52-435d-802c-a66835a64688))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b7a1684a-f106-44ad-bda0-d6181ed08fe8))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 189d2d90-3a88-4edd-b122-19a0af7a5f1d))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2bc3a720-413b-4bd2-a289-f5f7d3478a1d))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a827bbe8-813d-4c7a-8e3f-39d2e678752e))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b27bccb6-5ed7-49bd-8398-c03d69038ff6))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cc78be33-f51a-4f4e-891c-806802aa339d))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 614968c5-ab39-4d3e-83dc-d8cd44525c9e))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 70da3021-598f-4e1a-b986-a095e7cef489))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7498191d-6a6f-4855-851c-04f9995aeff1))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74c736a4-b6e4-482c-860e-c5cd5fe65997))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b060c558-782d-4365-8a3a-435e48da77ab))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1fb2ad6d-67fc-47e3-89ba-dff635daecf2))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5c7ea48f-cc58-4865-92f8-5589531869ad))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6ff5c092-e6e6-47bd-9000-23ef28f67f85))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af9fc9d5-aa98-4368-b2f4-4d7bf97d4040))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eb821835-c2c6-460f-801d-1c853ad6c8ce))
  )

  (module "common_footprints:8mm_plug" (layer "F.Cu") (tedit 5F85D873) (tstamp 4106fec8-e953-431e-a514-2cfc9e53194d)
    (at 149.65 -12.4 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 180 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8b323cd6-c28c-4cde-b213-f5a67a6a8cec)
    )
    (fp_text value "8mm_plug" (at 0 1 180 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f321853d-a3d0-4b2b-b1a8-be85b31c0f22)
    )
    (fp_text user "${REF}" (at 0 2.5 180 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3db9dd6a-9ac2-42d2-8443-8f2ea2cc1d7f)
    )
    (fp_line (start -4 0.8) (end 4 0.8) (layer "Dwgs.User") (width 0.12) (tstamp 52f2d8aa-c097-47f8-a4f4-13a9c2a9455c))
    (fp_line (start 7.5 -0.8) (end -7.5 -0.8) (layer "Dwgs.User") (width 0.12) (tstamp d794e7c0-395e-412c-85bc-f61001b1e30d))
    (fp_rect (start -7.5 0) (end 7.5 -5.6) (layer "Dwgs.User") (width 0.1) (tstamp 9d16a00b-f812-4518-a7c9-3937b62e10e0))
    (fp_rect (start -4 0) (end 4 4) (layer "Dwgs.User") (width 0.1) (tstamp 9dde2b0d-b4f7-4d80-86e4-dc09bfd481d6))
    (pad "1" smd rect (at -5 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp c3d96cba-13ac-48ff-a1d9-434a3d3775b6))
    (pad "2" smd rect (at -2.5 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp 46990e00-447c-4900-bd09-8ce37549a86e))
    (pad "3" smd rect (at 0 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp 5824925b-766d-4420-ba78-8b7d4bfb4e88))
    (pad "4" smd rect (at 2.5 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp 35f50c53-de0f-4509-b06d-a0a47426391e))
    (pad "5" smd rect (at 5 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp 3e9bfa34-a12b-4357-ab7e-3ebc4c843b22))
    (pad "6" smd rect (at 5 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 94a4913d-0d62-496c-8bb1-593e610f20d8))
    (pad "7" smd rect (at 2.5 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp d28a8de4-656d-431a-b6da-c8e7ba680ed2))
    (pad "8" smd rect (at 0 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 94848fd9-7a7e-43de-8cc2-a616b133d2a6))
    (pad "9" smd rect (at -2.5 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 0d25dba2-fb59-45be-8f26-12539b84f165))
    (pad "10" smd rect (at -5 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 212ee019-30ce-41ba-870d-c420db1d3834))
    (pad "11" smd rect (at -2.5 2 180) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp cdf71006-4aae-4780-a15e-73d744ebf080))
    (pad "12" smd rect (at 0 2 180) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp c101351b-a5e5-46f0-8f3d-707c2a1040e6))
    (pad "13" smd rect (at 2.5 2 180) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp ef406e22-019f-4b5e-8f16-69b95739e52a))
    (pad "14" smd rect (at 2.5 2 180) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 86ae7ede-6e16-47b3-a151-282fa708c29b))
    (pad "15" smd rect (at 0 2 180) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 2380f517-1c9a-4f53-97e1-5162ccf04b6a))
    (pad "16" smd rect (at -2.5 2 180) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 2cb0014d-ec98-4877-ac6f-ae54e9bbf32d))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 437065ab-04f1-480f-94bb-af9fc69d6704)
    (at 147.46 0.94)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ff1c5b47-d7e5-495e-9645-25a171f1889a)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9e61ee49-44f5-4232-a2f6-f73e81adc10d)
    )
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 293b505e-e421-4b6b-a9e5-81033515920a))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 98b0a8b4-9019-49c1-ac0f-ec4acec084bd))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be91fbe0-c84a-43e5-92a9-566e7c96ec00))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c00ced10-041b-435c-9223-c298605648e7))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d7045fe2-f981-4f50-88b3-f33cf33ea7b6))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 80dddb2c-0bdc-4dff-8104-4f9946a35a2b))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8bb25fdb-c4dd-4b25-b995-65f2b3c2b392))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d277e41a-0071-4fb4-a211-0c2aecc3f102))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e48951b6-ac35-4945-bf71-1b9e81129e2d))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fa1d0d18-1913-429f-9491-76ae1483b1bd))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6adf8ba2-f4af-4cc2-9170-6f22d04a59ee))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7b18cb3f-bf0b-43ca-bde0-3b75dafa2430))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac8ec471-e566-41ef-803e-a890f473972c))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b79fc948-c9da-4cd8-a0bf-a9e3755462ed))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp de6aeeb8-7d26-41b0-bec3-17aae3378d5c))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 447e8e82-f8f0-450a-99f4-e5cb0c95fb33))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 44ecd885-68ae-4b94-b959-92a391aedae7))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 572cc92f-8cc4-4a4f-b1cc-57446f0371e7))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b6348e5a-8c08-4cc0-ab83-fa0b4dd9de09))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f94ab452-d25d-4c2c-9b90-f2274a2208fe))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0d7af147-2feb-48ec-809d-b0d8aff2b965))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2f76441b-997c-4f87-b9bd-31a7e3c80a90))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5ad4d7bf-5af8-4d1d-99d5-31674b46ca9d))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96a2e30f-f0cb-436d-a9dd-bdc12556d33b))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d71f89a2-f63d-420b-b478-e9c1fe37fa67))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 4478ea87-8f0b-479d-8432-9e401350d718)
    (at 155.08 11.1)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c701e71-b965-4122-a1c1-8ed5da09754c)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3a084d9f-f79f-4314-80c8-79f677a1bda2)
    )
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 30cf9e4a-a75e-490b-a010-ed9cabebf9d2))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5f9b9087-9bb7-419b-af2c-0ce3f08fa328))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 78876cec-59eb-4ebe-a1f6-48b97189f2d1))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c88fb858-d88b-47b5-91ef-7126fe7d6966))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f05add24-0415-469f-83f7-e400be2edba3))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 366720bb-b982-4f69-8985-53462cddaa0e))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 644d5418-abe7-4301-b807-61c38a9c2804))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 866b1aec-aa52-4451-b032-8fbabde48cee))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c79725ce-e229-44c5-9e77-428c4f131dda))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dc5d51d4-5c8d-44b2-b9ef-28e13914822c))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2ec6b0f2-045c-4efe-97da-c6f6ac6c6ad4))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 33796ce2-0a15-43ce-b96f-ba431e32a32d))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52b3bc33-b6c1-45fc-8d71-d15d12a74aba))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e98e883-0c73-44f9-8359-913e61ee319f))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be661825-fb10-4e4c-ae52-8804e572022f))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0349c9d4-452d-4100-a329-72ed9c0919fa))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 538eff32-8678-4a05-9034-614ba1e04bca))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 62bef8ed-3561-417e-8299-63c8b7aad2af))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c230bcb7-b082-4c20-9f13-58ed6c0aa24c))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c7abf5eb-19fe-4c30-9ea8-a769df7affca))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 229d89ae-1b67-4c58-8692-b4cf23d2339b))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8db8e78a-449b-4140-90d6-945608c5d4f7))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 948d5081-66c8-4bff-9432-46caee10fc77))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 965921c5-1751-488c-9a79-ed739e20de0d))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c8ece861-58dc-408b-b10f-fd3e94e37aa1))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 59d637ed-80bc-44e6-a92c-86632aa35f7f)
    (at 158.89 39.04)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7f4ff9d-4b4e-4b35-a3c1-add470a68dc7)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f933c244-4b3f-4545-b004-73df95370594)
    )
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 159498e5-8f08-4e07-b60d-628c30649595))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1aab1493-ad5b-407d-8d63-af7a3cdf36ed))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 327eb72d-fb2c-4a85-92a0-1d7eb22a7b6a))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 45be025a-8e76-418c-87fb-3ffe8e1a0d0d))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9506cb64-2997-414b-af8b-22d2f593a5b1))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2cce65c8-2c73-4fe4-a260-82af1c65f1da))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 30756ac1-b928-46a5-b6c0-7beba62ca4fa))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6efd9569-300a-4725-8459-c60f29ea1c8d))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4a78d61-478c-4d2e-bd66-9be9e43b41c2))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e136b464-af76-411b-a5c1-11a252992506))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2d99d446-0461-43b4-8b6f-f64e81a69541))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c509127-bebb-473f-91e0-1810d6ca6310))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 53b525ed-6b0c-447c-bc13-571dad85b30b))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b086e72-e1e1-46c1-80a1-0e96e1974d34))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5d51fc3e-ccf8-4f6b-aa8a-073eafef7c2b))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0349975d-0cb9-4816-a897-9721397dfaa5))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 23a9943a-cd7a-412b-bc3a-cb9df3264f5d))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2b8b7278-e623-48ce-a670-7dac26f564aa))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 332311b0-5439-4d17-a1d5-bba70b151109))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fdbea009-068f-4855-ac92-0b86b4fdb841))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 61f54b09-c25a-4a71-8061-8d85464f9fdb))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d2bbc5a-c921-4a18-813c-0eadac4a50d2))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d0f64cba-0a06-4c45-8f5e-30430c872ae5))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e9fdd7a3-89fd-4d0f-b5e6-df0f6744b6f5))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fb19a6aa-f2cd-48b7-820b-ab3b92ec0ad0))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 5dbde840-8210-497a-b2fc-1170cfc5a7f2)
    (at 152.54 21.26)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 00a29010-d6c3-4aab-97e6-6315e93bbc79)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5acc085a-c583-4943-bb8b-d4dd05aea4f8)
    )
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5f3342f0-e5d2-40f8-8d42-90872b079024))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c2f7e60-1a20-4c3d-8d36-8b555e18cf8f))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6e5b0043-5516-422d-9d7b-f53ca28fa1b2))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c64206c-a2c5-4de7-960b-34a840c0f4ec))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9dba7fec-c5c0-41c7-b3d1-5506e7a6c70e))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3456f5fe-1310-4c63-95c9-b11b7ac0a30d))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3d958deb-b715-4465-a4d6-912b5e4b61a1))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47f53566-7b6d-4acd-8bc5-b2f1fdf14d96))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4c8259d4-5c74-4586-817a-66f7c76cdea3))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 95ad5fc4-2b47-4c14-a05d-c2f593333bc8))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4623da65-91bf-4bb0-83af-fcdfae66306d))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 77ec0b7c-55c1-41b8-8bea-ad023fc179b2))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a06453b9-022f-4c9b-9dfe-7090501ea99b))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp baafdde7-200d-486d-b036-a704542bb0f0))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff337401-e0b0-4517-96af-deec9ca15cd5))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 49339fd5-6e05-4107-9c6f-3b6a527a3a47))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 505ed0b5-ea46-4f8d-aed4-5397b610784c))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6d3ad90c-aaea-49ff-a20e-31df14858968))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aaf61236-0450-471e-8144-75ba2972220d))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bea389b0-44f4-4124-91db-780e17a99330))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 255da6f2-0f58-4ef1-9895-38099139bb32))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5bc54e2d-63f7-4f5d-b8fe-b890367a82f6))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e348c681-623f-484a-ac05-0ea49a85860f))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e5dacee5-893c-4356-9f45-86888f03c658))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eb1d6ffe-821d-4f51-a408-363ff68a56b9))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 60667ab7-ee7d-4c02-910e-10bca2b7332e)
    (at 174.13 27.61)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f5333baa-88b9-4ab6-9fbe-679d813e7cdc)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 06a2abee-e3f0-46ef-ad1b-8abea99344bb)
    )
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0cbf7588-cc8b-4219-82b1-3a584acd7dd0))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 24db852f-4ea8-478d-8465-2af1484d8124))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 29020762-8786-4675-8c46-eee05b331f49))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e6b981b-aa3f-497b-97ba-9e7da4169315))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f7202655-1387-49fb-9c50-b5f5bb849fcf))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0656afa9-e063-43c1-b0a7-d642c8ed644b))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3f37f6d5-2498-4c3e-8e94-3722c94e8ccd))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7dbf48a3-ecd3-44fc-b662-d4ca830c39f6))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp acc57042-b293-4812-a1fe-c8d87e5c6ddc))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d21599e2-220c-47fe-b4a5-745d7018e97b))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 025440d6-9c88-4a35-affb-9ad78c91fe94))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6760430f-45bc-4473-aee7-dd7b75a3940f))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8311c8e9-2097-4ee4-aae9-f6c0f3a9c0f9))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e1f322c7-2000-4e00-be29-fc2bd160f652))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f11e5604-fb70-4e6d-84e2-31b1df0d1e17))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 22cbbe5e-af84-4b26-807c-b4df1897dd38))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2ad934df-08dd-42ee-9cab-0481d3590048))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 61ea1cfd-5684-473c-b66b-4b395e50377c))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88bf570c-fd95-4a7f-9150-07a4d9c77ac1))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e835f2ea-a923-44b2-8e20-2dd26c642b71))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2651c559-5b86-454f-8182-0ce2a13578db))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 307eb355-fe71-46a8-a32e-4ac62d7b7495))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 33b8d53b-e618-43da-a730-19cb68c8741d))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 426f72c5-7ce3-45f9-81fd-a2393c10483a))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5688f6c2-4586-40c0-8f31-899dc0b59dd7))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 63acfc9d-20e2-41e4-9ffc-247adfc0f54f)
    (at 134.76 61.9)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 71116667-45bc-4672-8426-c56afac7ada6)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba386db1-be5a-4824-8fa1-e8f6342c7d1f)
    )
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0d2d558b-1bf4-4f8b-824a-da7b293e00ab))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1126ae79-59d3-4f82-a53c-79f191002f32))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5dd46a51-3e94-4f34-b54f-1af32371b6c8))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96551d25-809b-4462-8b38-84744ddddb0c))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ea423de0-827e-4428-bdb2-3bee61f63ff6))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b5ba0d2-cc4e-4354-ad04-7cd9547e122a))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f81b8a9-522a-4e51-9e03-efe1130b24f8))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8af998c2-2bf2-4b75-8be5-36cb1a942868))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ce2d5e69-e2a2-45b9-8844-28801be5d22e))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f6e17d8c-9802-4617-8b54-21022c2c2872))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 35ea075a-66c4-40ec-a97c-0cdcddf0b108))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 75270483-e05e-4260-9d6d-16492ae4ff1f))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96cd0af6-f105-41b4-a662-d557e669c844))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp efacae47-b1ec-4250-a7c1-59885af56901))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fe06ab5d-f758-4999-b7aa-ea626bebc549))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f2524a1-b228-4084-89b5-db55ae465f38))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 57a750f3-f34b-4774-95aa-ae89ac4c4648))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 654bef3d-0024-4d8e-9555-5f2ca32f7371))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 680b431b-5b5b-405b-8b36-d6fc3aebf911))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3ed5038-1628-4cb6-857c-1452d805a679))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2d68f59d-502a-4f76-8329-79cc343f73ef))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4c75bca9-acdf-4f5b-9b4d-c26dce0d6e75))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8d325d6-9fb1-4699-9393-d0eb0266fb54))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bbbcec13-85e5-43dc-9ad0-8033f80256c5))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c73278e7-15aa-4092-985e-1423873b8a98))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 64d81cc6-ae06-438a-b2cd-1627ca05826e)
    (at 171.59 33.96)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c32c49aa-f621-4751-aabc-9c90d98be0ad)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 194e3e43-a4e7-40d2-a9c4-612b1f0b0674)
    )
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 247274d2-c136-4441-bb17-27fcaebcaedd))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9dcaf953-09ba-4c87-b7b0-5bb8ae842522))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9e8b47df-8389-41c4-9435-11ce2bae0254))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3d002f1-20b1-4b17-a3ab-7bb4b47a4a90))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f169c598-9953-418a-9941-6643d4389ed3))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 03471281-2168-494f-b139-8a8faa372a09))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 246d2c62-2c83-4bb5-b8af-ad7d7789ba7d))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac6984ba-28a4-4c3a-a504-6907ae23ede9))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b14626a3-3c50-4006-bd1f-78fcd1c42e68))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e497ae30-588c-4d83-801d-572dbfc4a4ab))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 018087b4-c716-487d-81fb-2e3e6b186cd0))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c3206076-40ff-4e77-ac1b-931546682685))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3092605-ddd1-4fc9-bd2e-06b431d5c802))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3f4e2ea-41cc-4f90-8f50-c4f66df9d03b))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e7974990-fc5c-491a-97dc-8a6faeed0010))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 416b1e85-4003-4fde-a905-91a346300eff))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 716c6c22-d8ac-4f46-9a9d-0e315c1b2ed5))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ef76868-7f2e-43bf-b8f7-49a56634d618))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 86c1a0f8-97ee-4c58-aa7b-8b514fec117b))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d181744d-f4fa-4378-9511-5a0da286405f))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3fd8a269-83af-426a-9c4b-4f04f9c642fd))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 45142fe8-9ceb-4e1d-b1b0-c74669da7f8d))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50356a33-8735-4fd7-9c57-54ee03ac7a53))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5235046d-8aba-4ae0-836f-bf935ee1371f))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 84e8700d-8ba6-4674-9ad5-19d64f723c09))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 691496a1-262a-42c3-878f-abb757ea209e)
    (at 129.68 36.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13577efa-82bc-43df-bae5-cfececd124ce)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3c9e98da-6fb3-4aec-97e0-00a45118ad40)
    )
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 12d51254-64cf-4eef-ac38-5d8102cc8385))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 313d9373-6560-4a6f-baf6-bd459ebe5f64))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b92ee39-056d-4b4f-93fc-28f670219f7a))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 82c5a3a6-289e-41cd-ac40-1993058a47b6))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c6b68a4b-83a4-4f5e-9dbc-05aa3cac3949))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2193f264-d3a9-496f-b028-310d8cb507fd))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c200b09-98a9-4c8f-8b21-48e953821e85))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8b1646d9-4c3b-4e55-a9ab-91160d601edc))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dd8e2733-149a-4376-a2bd-01cd0f866e5c))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f05ef370-f336-43ed-831a-89951840f42d))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 25130cfe-5037-4694-b161-8107514514de))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2fcb9cbc-c322-4624-8129-a4d345fe8651))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 32b1487f-7c9e-41f0-a93c-5422e3ec7e4e))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50a7c831-5e81-444b-aa71-3a91bfe03057))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e8167227-47d1-4f07-88f2-8de50c6ddd0c))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1e6f4664-1e18-4c11-80d3-4e6df774ae89))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88927d8d-d2ff-47ec-b5e4-be48ef16f2f1))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f90dec2-0ed0-4d7b-b58a-e0dd843732c6))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b72ff7d4-be0c-45ff-965a-839af2abe23c))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3ec620e-c5b7-40c4-9468-724a59e6bc5e))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0bc31000-c09e-4654-a4f8-0baf85b196c4))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 12418bce-4622-4210-a6ca-f2115ead28fd))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 565057f9-0a01-4282-adc7-36e984236fc8))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7425044e-8553-4387-bb86-072595072848))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc3c628c-0bac-4d1d-bdb8-86f7c96d69ae))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 6a97b6b9-c50f-416c-8f9a-4192fce5761f)
    (at 152.54 33.96)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61fb136e-904d-4981-8462-034a9ba8b1e4)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4313b98b-5467-4dd1-880b-e366ad391094)
    )
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 12301fb9-cf0d-4ac9-83db-7f5667a3f061))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37d25cdf-ed14-4809-902b-a062aee69931))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5046fdd5-6457-4c96-aab2-604a620959c2))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 64cd5a13-47bb-409c-ab94-ac3a02f0ee78))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e1411aa-a989-4b2b-8576-8fa346a63b52))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 17b9aba3-b138-434c-910b-e5f2d9a8b14c))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5815eb53-4eb5-48a2-a92c-271d925124e4))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96b5ff0e-ac85-4908-a36a-5d0976d7a738))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a874605e-53a7-42c9-9706-43fcfed6fd4a))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fca3a7f7-1c97-4bb2-b243-d54aecde706d))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2c0d4491-3f62-42a6-b846-f4117215ac7f))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4b08b5b6-0d5d-4dbb-9972-0e490cc3b455))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50438a48-bad0-41e2-aff5-7a5e16870238))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 59fa438c-2e98-4663-99a1-0c9c859582f7))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bf51523b-d1e9-4281-a52f-d0c07e3c35ca))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1c38e545-24db-4ae1-b376-ce153c586012))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1f865518-9425-4c34-93a8-b1d0dd1db059))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5f3e489d-db68-4371-8b8d-666582726e2c))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d9e35356-6681-45f0-8e9a-c34c4266bb20))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dafb650a-087b-44da-bb73-983a4a888ce4))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0fe759c8-4e80-4ff5-8bd6-4c0bb4b61ace))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2133918c-6311-473b-9df3-bfcc1cf9bbc3))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 30b6cc54-6c1b-4651-b8e7-5abda6bc9cee))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 468052d5-66a3-4c95-963a-24f808d4ee56))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ba95be5f-af1a-4784-bae5-7a6ae693a120))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 73449443-d7b1-41f5-bf3a-0c31e0595473)
    (at 165.24 6.02)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e4b14351-3ca9-4f52-bd76-d4ebc0bd770a)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13d8f81c-adc0-4ccb-905e-631cea65707e)
    )
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19f81aab-5f11-4560-ae39-b49920a27d75))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52283a43-2c24-46bb-96b8-e6b33f9924ba))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5fa87116-5a7b-4d08-9efd-31813df90aed))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c1b844f-acdd-45da-92bd-a616a18ca715))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f04c464d-4dd6-4129-8e1f-ad93d912a14f))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 02c3c2b1-5898-499c-a70b-bba52eda62dc))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 04f0d638-41de-4c56-b7e6-28bbeeb01408))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4251e0d5-6439-4e7e-ba85-41f267254d7e))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6bf212e2-0b12-401d-8d4b-3421ff316d57))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f4b36d5-4bc4-4542-a04e-66d6cf79a6d5))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0cd446e3-abc4-4f8e-99c7-572ea69ec621))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7631e547-f957-4438-9372-f177b089e1ad))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7cb851eb-de92-468d-90e5-634d53a78c9b))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a3eb4932-dc4e-4665-b91a-7bd80fa01c78))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b1baa2a2-e9db-4875-8278-f9cd49fdb7e2))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 35286ee2-b116-42de-8663-14cfc31547c1))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f7399f2-0c0c-4db7-a172-c5dee8b37e85))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c4233ab8-ed28-48f0-8a48-f9e101aee01c))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cdcd3199-cb8e-48b8-8f8c-a1a860564dd3))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f6b0201b-add3-45ff-8b72-0cd0f8156b09))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a2f2db8-b9e7-4cf7-9d83-06de88e80910))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d6e35c6-c859-48bc-a668-a7021b3f8c50))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 63835c8d-80aa-4ae3-b503-dba2d362300b))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dd93962d-b26d-4342-abe3-3fbc71492138))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1861c21-ea7a-4d6a-b16d-5a3ce57a4130))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 7e71d5f8-2b49-43eb-928f-8ec43c1c93dc)
    (at 170.32 74.6)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dbb9374f-c3f2-47bf-8b92-a08ed38a6eba)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f262c3a0-8570-40d3-bfac-e970ba33ac0e)
    )
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7cade650-6680-40bd-ba70-775b9a66a61f))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 94e29cd8-d8ad-4d2b-b23a-89e102b6cd7c))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9c331751-e89a-46b0-88d0-3764a2a38d57))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c3324baf-74ab-439b-97b9-1602ab37c4c1))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5ef4026-4cf1-4c7e-bf5e-0aca450f3f30))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1afc9dc5-6759-47b9-90c9-668952639eba))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 45e292bb-7ecd-4f24-bb89-d1d98191bd0a))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 78268455-b544-4c39-b7b5-169aaec73a07))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7cc769cc-c86d-49cb-8b1d-f85162be4997))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b58ef87e-206d-48e2-9a0e-d7ad55e92b3d))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3e3100d4-da1b-4c4e-94ad-09a713847827))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 768adab0-e22c-49a4-80c6-1d1d178254b4))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 97a2ce6a-5e0a-4de8-ab01-113c9309bac7))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c19ae553-a0d8-48e6-8775-9ffc560512b4))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e8b31948-6ae2-4945-8383-932750a01d35))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 01e72ee0-c12e-465b-b75c-7ae911a8dd4e))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 15251556-4654-4650-9fa4-fd5b7042c72d))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b5422a75-2ae4-4d38-aa43-aa8886177641))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b9f655e8-ac3e-477f-9195-2d00a8c1640d))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ba14f435-7be4-41c6-900b-22efbbb640bf))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 81525837-2ac5-43cf-9f5e-2b0b867be893))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8f20362a-dbc3-45f6-bdee-f03db85679b5))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 905afb53-1665-4408-9330-215e40a48c14))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 943969e5-0ed7-4c04-a6ad-f75838e361c2))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b3511d4f-f024-4f7a-9364-62368dac9552))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 7e824b2c-b1bd-44e6-a70d-b3d7b8b2c230)
    (at 129.68 11.1)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp df0e4865-847d-43f1-9618-c31b849b7ca0)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19508468-f381-4d2c-a422-e8e68460c2c2)
    )
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 09ec3032-dd14-42b6-ac3a-2aef3638cc7a))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a3ff793-bd71-4c31-b68c-b86c55495223))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7b1076b1-4743-4ace-8c1b-b73372e6811d))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7266ea7-6a3b-4221-a2ec-9ef3d966b952))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b822be3e-288f-477f-a602-c232bd1696ad))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0a50b5f8-de25-4d9f-bf6e-2f9d9d30c695))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2f26504b-db7e-4d45-b960-68c7c0515714))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f3bfdaf-7bc9-4da4-938d-02649b4d0dda))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a6cc196e-f50a-48ea-bb7a-486376a53e58))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e1967382-515a-4f3a-bf94-4f5507cb1ab8))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3438f6e2-2a74-4d59-8994-1fb2fce66cca))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3ab115c5-6013-4111-9797-86ec88ddc589))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3cc7f412-a7bb-45a9-8b3b-9ad0637719f2))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 92ba74a2-6b64-4671-8431-5bb7d94cfeea))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f132b9b3-ec38-4f32-8152-22eb77c50782))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1edc15dd-ee3f-4869-9bc1-21e6ee1ee080))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 69684971-1326-425c-8f02-732cbac2f3da))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a6a07083-70c1-487c-b690-e17ef1bedd8b))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af61452c-8f22-4646-a012-98bfb36233d3))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8d2d7e0-7a5e-439c-ab5b-7a6bcfdaa29f))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 20739758-d82f-48a1-8d29-4f31ca4d6563))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e81e696-c9ea-4dc1-bb0e-c5fb42d609cc))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9747841f-23a2-4791-bfb5-d52b6c576f3b))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b39f9389-1cf9-4f0a-bd38-ead619e3dc75))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d0f28dcc-3b67-4fcf-aebf-96978d21f96a))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp 82e908ca-9996-4882-a183-ecae676d6934)
    (at 152.54 39.04)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fdbabcb4-4742-4d3f-b4cd-ccce204cf82a)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3f73ec8b-a885-444b-b033-d2b6280058bf)
    )
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 38a8947a-64c0-4a25-98e0-b02fdf3b9fd8))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c1a782a-743b-471f-a930-b568eacff995))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 58bfa722-122d-4637-8a3e-168e680654fe))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c7319fd-3d24-454e-b6a1-8dbcfbf58299))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d2aa56c0-b00f-4c7f-b94b-5b356afe26fb))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 286fbe61-b15d-4ff5-aad3-b0c6f434ef5c))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 505e0377-7f6d-43e0-9859-8eb63d694b43))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bddba2a6-a6e9-4035-ac9d-eee7b85b5872))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dd0a4d50-1716-4f31-88ad-dd9c66433ce7))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f83949e2-ed83-4cb2-9b1a-c59ec4a87fa8))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47142207-21e8-4842-a03b-40227239df1e))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 69cb0a52-11c1-4c12-87f6-237cdfbb0352))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ee10551-1925-4c6b-abdf-6f21e574d859))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 90402033-883e-40a1-8d65-80cb1c8fbfaf))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9897fc62-8a4b-439c-bfd9-009457958e92))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3407713c-6f11-4d8c-bfc8-773baf3411d6))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52c0bca7-e609-428f-bcb9-ef7e7ed6350f))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 889de9bb-79a6-4d10-a5ee-9d0ecdc14e91))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8f729fd7-2f95-4872-bd0a-fc9e3a51970c))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e0b988c2-01ac-4952-87e9-3be0f8b7a8e5))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0b8530e2-00c1-47ab-93f8-351545842c94))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 54f307ec-cf78-4a0c-982c-030b5cda8bb7))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b33e1ae-86ec-4fe9-8b82-f30d9dab93a7))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8cafae7d-19ef-4025-a249-84e4b953c2c6))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1a113c6-3857-48c0-8578-442c2391abd2))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 84e28066-0a4b-4e0a-ab66-a8c281015b2b)
    (at 147.46 61.9)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3e4f97f6-41bb-4251-acfc-fca34024e59c)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6f908997-5559-4b82-b550-4ee6a625e762)
    )
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7babdfb4-6e6c-42f6-9a47-56928c9978fe))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a4c19b16-d78c-4109-bf45-fd10e82b1c64))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d6f5f120-f8bf-49b9-be6f-98b70642b033))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d75481ef-9a0a-402a-bee9-b825e4f15e18))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dd9d3fca-a55f-4fb6-8127-0b2fd378c82e))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a968ed7-a3e7-47a6-b5d5-404901be2e8d))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50ba7d4d-4522-4514-b8c8-94bed0c880b0))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7ffdefa-f5c7-44f0-b5c9-3bbfe191a706))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c9c051e2-2fcf-4665-aafd-ffbefec48e29))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d468af13-95c0-40fe-9e0b-5753d950cf6e))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 15870f4e-936f-4744-b140-2b08dff2f721))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 21241fd2-ebcf-4483-86e8-2a43de8a8329))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be13dcd6-181c-4a07-919b-6baf2ec8a655))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be4d9cf0-3faa-43e7-83d4-84dca1b8e01c))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec93427a-7618-4b71-85f0-a9e6dbd31238))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4aed4f18-708b-4442-9c7a-cd665dc95de6))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 63a05c15-101d-4d69-8288-dcbcb953ae22))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 65f8841b-3464-4f01-b930-5e17e2a8ff67))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a85d5abd-175b-4e48-beff-12d4c0cf3ccf))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp faa8f06e-46ff-44ee-8561-0665ddecde3c))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1e698b72-d95d-4edb-826d-31e024cf65cb))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 83af7672-2ed1-41b2-abb3-1fcb52383c85))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b036f928-72b7-4875-9d0c-a71c3b6a3f48))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b5695786-482b-4520-a5a2-63b108c02bfe))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ce029d8a-dc25-43ac-89ea-446106470e90))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 86ca8dde-9a22-40eb-a147-51a8b44769f9)
    (at 165.24 61.9)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e64333b8-b42c-4908-a4ca-a71d3a99198e)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13b63efb-4d96-4259-b117-dc19ff5d9c54)
    )
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 14737920-ca18-4a8c-b9b9-c77bdedcd178))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 217512ad-fdfc-40a8-b1e8-08450a7fda3b))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 78c43418-1525-436f-be79-901f039e1d74))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8f1d691e-6311-48be-badd-e92de49ed4f3))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4f1e66d-14b2-4290-948a-c5762197e2d2))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0a25e5a3-aa86-4e18-8e55-557167d8c19d))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1ed5b5f0-6a3f-4419-ac0b-c743c423d191))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3be1e076-b6d6-4a7e-8b48-134798b69d1b))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a95ce67-ae5e-4866-9ddb-2166e382e5ea))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f239bd44-0a17-4bea-a9b9-2ea2dc367f88))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 266578bb-2603-48b8-805d-7a8740ca1dd8))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 39e808a6-99cb-4978-ab9f-88595f28e3b4))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aa974c8e-bf60-4e16-bfb5-b76380ce2e4a))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d96a086d-bbce-4eae-afd3-1cf28db78668))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp feee2cf4-e892-45d2-a3ae-1f2cff2ced00))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 208f6acb-ed02-45b5-b896-d59ac7bb013f))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3a13068e-b4bd-40d0-b755-5d4110e150da))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 41312faf-145c-4f39-a256-247ee83f7e07))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aae34472-1f1c-4e70-8a4a-1f112a7c5b3a))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp afbaec0e-4e78-43b0-b6b8-b5cd13cba3d5))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 017c7698-3e73-4a8b-82bb-bdf4135b7c2d))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19078590-6c9b-40e6-a7d6-36d7a0d0584e))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 469bee5a-f35e-42d3-a1ae-bb92e8588c6d))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b2b7f477-affb-4098-aa1a-3d361b137fe6))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c84ff15a-4269-4415-9b04-783c83983872))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 87ded887-8fe0-4e3b-92b7-98eb6d257822)
    (at 142.38 49.2)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da400e09-fde3-4f69-b3d6-37daf618ea13)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e8c3ef8c-9da8-4261-8fd7-82143eec1f1a)
    )
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 16ef7221-65f9-4b51-bcbe-acabab55c77e))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b4b8308-0c8c-4168-80c4-e54c99ef299e))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 210e9e4e-7fde-4279-8cab-950f97b68026))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bdd4b73b-659c-47b0-873b-5e206cb79269))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c064aa04-8390-4e82-a44c-35b362f88709))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1eddaabf-c017-4d97-b42f-42e3c829e80a))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 557e3650-8f94-40fc-8684-7e36950b8cc9))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bad01ce5-9fb5-4a60-a976-456abbb64c69))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c23d8330-526c-4a08-a662-c1ab0dd2018f))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8220841-25a8-465d-8d4b-14cc7d21a26d))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 08dba50c-1913-4684-808e-b2a789c10e10))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 11cb5c58-fc3f-441b-8991-1e37335a9a45))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 87b06b67-4465-46e9-b8eb-fdf837d538b3))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bc964537-7140-40e5-aeee-5501057cd3d1))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ed4245c8-5129-4892-b049-973b75d1606e))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 71f3534c-d670-4562-ad91-3436a33177b0))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7867bec8-e41a-431f-8bff-5bc53d2b5158))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 82005640-8b2f-4581-8014-5bb044ecda34))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b1a2677e-6715-4d17-81d1-467a8ef03431))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e6f94460-8948-4385-8742-e7b78dd504fd))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 27341d06-9a4f-4f02-bfae-8d37a2b03d92))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 27d1f886-4576-4e89-bf04-645a37a9d232))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 928d3991-8c30-4833-bd27-fa0b6c2e0927))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 95ddf8c9-2ab4-40dd-a136-7fef8ab118c4))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a08aa3af-4efc-40ee-a17e-9ef8d1b03af4))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp 97cfd66a-8817-46f4-b0e5-fbc93f2cc295)
    (at 155.08 74.6)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 669cca3e-2cb0-4c40-a3af-bdcf31478e49)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e2a8b4b0-c35d-47ab-b3bc-4c70adc2140a)
    )
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 072e5d91-bc49-4eb3-a445-47538eebfbff))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2d7a4f7b-bcbc-4ec3-851a-1053036afc1d))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac821449-0b50-441b-b797-82885988b2e9))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af871dfd-6ab0-42cc-9487-8993d00cc70e))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1a3011b-fbb0-4b7a-8934-eff97c9f53a0))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 79537d71-21e8-4768-b0f3-39fdcdcee98a))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 895abf8a-049c-4b4e-8094-2c21ae3b43d5))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bddba230-1d73-40d1-85d1-f36a8bb1b31f))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dcd1c7e8-7593-4831-a752-1450a9b79d61))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e68c35d0-6207-4f5e-b12f-31c23ae87516))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 395ffd6e-497d-4ee0-8ef7-2923b1cffd90))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c1d341b-fabd-4d12-b8dc-60bdafd6716a))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4811e8fe-771a-46ee-9712-6636e8f006f3))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f0445b38-7564-4691-81b9-867023f2ac57))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fd8099e2-8a6a-489a-b69e-dd9b0bfab9e4))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 41f2f049-428c-45c5-8176-be43bffa81c9))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 86f3184d-fc7d-49fd-8efa-f8da8667cc0f))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8da4e045-f8b9-4dda-9810-9a28342d9159))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ea84ae1d-524d-46c7-9d7c-ce339b200c44))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f809b311-f077-43c7-b190-e89896149411))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 090112a8-a851-442a-90b7-41df7a0974fc))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 692a03e7-4333-41e1-a71b-d2d28174eeff))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6f3c846a-3001-4eed-a52e-9ca801ee0cea))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 91b7ae89-78f7-468f-af87-6ba59a1f76ba))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d48a14bf-07a3-4725-be52-611b703466f7))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp a6a75af8-0abe-4393-b1cc-9dbacde33325)
    (at 165.24 21.26)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3f6015f9-4db4-46d5-aa8e-b82386ba1ec6)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 421565d5-951c-4795-b458-b2ced7748adb)
    )
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 39031153-7c89-41c7-b4d2-dcecfa20e302))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3b34f2d0-3400-484d-93bc-67cba1ad9743))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 69723366-ecf4-4f47-90e7-68269c124947))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 843bb91e-2165-41b6-8454-66aa9fece716))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9cecd1dd-0027-4e76-9864-7deba2887ba7))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 54f0458b-1372-4cbc-8e5e-eb6c35f31aa1))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 55ef794d-cfd9-41da-b0bf-2ff7950a0b48))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5682cb4e-ce8e-4508-acf5-dff8386da5b8))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9183bc4e-2d26-469f-9858-3701953eeb9e))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9b3a2cda-5c87-4b6d-8f2e-0958c07660d4))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0b2ab623-4ff9-4c81-936d-fb7d51dc2ce7))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b42f828-05f0-40dc-a4e8-39e7213ad993))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a1b92ab5-f5ae-4eaf-805f-bc36ed602697))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bea90b90-6319-407d-9400-6c372a8aa520))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f8de19bf-ce13-4013-9bcf-deac195103d5))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9b013755-f101-4c4a-a067-fccc51986ac7))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b89a250a-7f60-49e0-9f05-96cedf0ad908))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c347b407-64dc-487d-877d-6e2e1176e3d5))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d1be8076-eca0-442b-91f3-a941646983fd))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f75c13b8-9b4f-47a9-a393-2691817b3754))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 25124f65-6c1f-40c2-ab06-ee9b6903a4b2))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 536ab7e0-729a-42ad-b4ba-545cc2de0d27))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 73071753-a101-425d-96c1-24cf3ce91685))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 82d9c073-0f70-4589-bb04-04ef7bd4bc1b))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e546c9c1-a179-4f79-82ac-5f293397fede))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp a7312f2f-34e5-4c35-a172-2df0b6166ba8)
    (at 158.89 33.96)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c850eaa-5dae-4f10-a5e4-bf0f05ce6607)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 28cb03b7-c1a2-4ef0-b739-63927bde4bc3)
    )
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1f12210f-bf01-4930-8f27-276b6172998f))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 22b443d4-a7a2-4740-8195-508333d49f6f))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2b342321-6dd5-4569-9976-08f289fa8578))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp df8019cd-39f4-4163-ad4c-e34991e4769d))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc2136a9-b798-4333-89dd-86898841bdf5))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 18511a67-3df2-4fbc-acab-29bbb98c28f6))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2a46f81b-5c72-4152-b829-ad8096aa333f))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ffd136c-4a21-41b3-b578-2d69e3a33507))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a1228698-d9e3-419f-b39f-d974b552bd59))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c8dfe0b2-0001-4c52-9fa6-487e027c3ddc))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0159802c-ea25-4ce3-9933-fdb997b26f22))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3ca0db13-43d6-4d9d-b388-61360b44d60f))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cf53bace-4358-443b-9024-ae52fbaaee24))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e5f0938b-33cd-4c70-a53e-5fff2d2da412))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ea10cf76-343f-4c68-9fe8-7317f421a834))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5153d074-c66b-4ed4-9f9e-58f138d5e986))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 744d2fa7-dec3-4fc6-8753-82f09885e33b))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7a9731fa-b275-4bfc-a6b8-94363e7068ae))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp adb5ff78-7406-49f1-816c-fe3d1ac49a5d))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d7e5c95a-cfa2-40d6-b2c1-cd76f86cfd8d))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 26413626-a57f-48f0-a4b3-161a3ef28464))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2f6a8bec-4153-4642-8282-4ceb94fa352c))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 55891c98-8cae-479e-a60b-afc87bf878e8))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7bb8ffb4-8aa8-4bfd-9fec-e9df1a5c71aa))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp da15e98d-8b98-434e-8515-a4ee3e0fd825))
  )

  (module "common_footprints:8mm_plug" (layer "F.Cu") (tedit 5F85D873) (tstamp a848d23f-dc6c-4ea1-9964-0f184bbf070a)
    (at 149.65 99.2)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8c0ff1e9-1612-4fa5-97e1-b6e01b1134aa)
    )
    (fp_text value "8mm_plug" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 84d5bdce-bfdb-4386-a135-c706bcc3f538)
    )
    (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 04ae141d-8bd7-4845-a276-65f94d1dca48)
    )
    (fp_line (start 7.5 -0.8) (end -7.5 -0.8) (layer "Dwgs.User") (width 0.12) (tstamp 2ea90752-b063-4caf-91be-695d8bc0edd5))
    (fp_line (start -4 0.8) (end 4 0.8) (layer "Dwgs.User") (width 0.12) (tstamp f8ab8abc-0813-4d25-8ee3-94de93abe082))
    (fp_rect (start -4 0) (end 4 4) (layer "Dwgs.User") (width 0.1) (tstamp 0d6929c4-ff22-4e72-856f-1282e75c3477))
    (fp_rect (start -7.5 0) (end 7.5 -5.6) (layer "Dwgs.User") (width 0.1) (tstamp ca90b94c-c12a-4d43-971a-28f51ab0317e))
    (pad "1" smd rect (at -5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp 16887d17-097e-4c3a-87e4-3ebcd69af7de))
    (pad "2" smd rect (at -2.5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp be2f6d5e-0b3c-42dc-8c90-b96bd471ee67))
    (pad "3" smd rect (at 0 -2) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp 8efb3946-8b4c-49b4-8b07-90e5beb725bb))
    (pad "4" smd rect (at 2.5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp be855439-f355-417a-a2e6-c3c62d4e16d2))
    (pad "5" smd rect (at 5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp a5e12595-bfba-4867-85b5-df0773c66d70))
    (pad "6" smd rect (at 5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 35d81cfe-7113-4316-a481-8f4e8940c3fc))
    (pad "7" smd rect (at 2.5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp f50b3119-fddd-48f9-9a23-faaacc5c556f))
    (pad "8" smd rect (at 0 -2) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 6109803b-1fcb-4994-9d30-0a3186de00f6))
    (pad "9" smd rect (at -2.5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp b0de999a-1761-4deb-b222-c57506d12633))
    (pad "10" smd rect (at -5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 2f1ec9e1-d52c-4643-ac6b-de80e3be11df))
    (pad "11" smd rect (at -2.5 2) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp acb4dfd1-c6d5-4e1a-b640-8af08c96881f))
    (pad "12" smd rect (at 0 2) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp d0faecbd-9bf1-4bf7-84d4-f4b2f8d8a343))
    (pad "13" smd rect (at 2.5 2) (size 1.8 3) (layers "F.Cu" "F.Mask") (tstamp d7cbe519-6587-4765-a56c-1a3fe1d84879))
    (pad "14" smd rect (at 2.5 2) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp eba4fdc4-0567-4528-b22a-e1bfebee7ec3))
    (pad "15" smd rect (at 0 2) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 97ab32fe-0027-4b3e-8c70-63f2ff02df2c))
    (pad "16" smd rect (at -2.5 2) (size 1.8 3) (layers "B.Cu" "B.Mask") (tstamp 2785ab57-d373-4221-9541-0e5fb693f232))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp aaf61a56-b5ed-414b-9e26-9d324706f2df)
    (at 157.62 74.6)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b653452-e7a5-4e2a-97bc-d1c96d9ed163)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 14edd886-4321-4784-8fed-b8e6a8c08122)
    )
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5be163ef-7583-4c83-9c0f-f1948e05f6fe))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8673db86-3657-40be-afc7-8cef970eac06))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9c131aa2-4c38-453d-be36-e6405e25c441))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c05b776a-b0c9-41d3-b747-f77e13e7d251))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c909d929-3f80-457c-a354-dfb04b1e5ec8))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3fdd92c8-444a-44ad-b131-428da50ed056))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 76baef8a-41ed-489c-88f9-f0f4cfcc601b))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 833fc1c0-2159-4df6-b30e-bcc0f10973e8))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cab934de-b105-491f-b98e-7ed067fffa1c))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d90db9fc-6062-4f64-bf2a-a0ce1673d427))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3211966e-d102-4597-8765-ffd857e2818a))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 49f52843-e08c-48cf-a6ff-c0945383c278))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5938c85a-af12-4a86-95cf-449d4c6e22b1))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e1b9604-20b9-43c3-a538-9774715efdad))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8bfced6-406c-41eb-8a3c-0b947badb172))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b802b42-051a-471c-8067-0fd103f73a16))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3188db64-27d3-4aeb-99ba-0f7cdb1918b0))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dce24524-c896-43c1-9b36-924730e14999))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f39e0d85-dcb6-46f4-849e-0e554aa5dd52))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f7042e99-7e1f-4fc0-9bf6-fa6dcaa79ae8))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6ebf09ab-5449-42b4-b5c7-df4f06fde328))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e3bdc9c-d329-4640-a129-d6c7bf41941d))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f0e0e1c-e35c-4a23-9ed8-5034d36209e7))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dace7d4a-3d71-4bf9-a48c-134621a3f8f3))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1a55bec-5c48-4e3c-9dad-4e4982e017cc))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp bc326980-2b73-4beb-a8cf-59bbb5fad349)
    (at 152.54 84.76)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0dc568fd-a2ad-416f-a604-4893488fc67b)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a28c3234-6439-4a3e-8244-90adca57021e)
    )
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 15bc7567-6953-4c1c-9562-1e77ff864f0a))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 23e8832f-4900-4b5e-ad22-363033864ac5))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 38b882f4-55e2-4fd9-afe2-29958c16e53a))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7a14b32d-75a8-4bf7-8890-a5d9eefccf2d))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 81b92c5c-f534-4390-aea1-87edb53d893d))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1663a163-622f-4eb6-8d7a-2b61c4b1df86))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 243909fc-2aca-400d-8be3-4d90fab08379))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 286aabde-df5d-47ed-ba8f-189495d2a8b6))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3fe09102-226e-4863-9914-5f34074a4c6c))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dd684eac-dd36-4147-b8e0-6cc4802ab190))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 321c4bf5-67b3-4e1e-9d56-be67ba35ac72))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3942d505-ec42-42fd-85de-b1e1ae69433c))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 59029351-5c60-4983-a383-53922b1b5234))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8375218b-496d-411e-8b56-d5d92e844cd8))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e1d2e3d0-f986-449d-9d37-62f4a20327f0))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1abb7de8-1146-4b8d-867d-a84212223a8e))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 450db48f-e109-48cd-a7a1-db8acd279c83))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 70b35d88-8c17-47ba-a9a5-2fe781da9980))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a36e1d77-068a-4a1b-b9c1-9b69cbb9de18))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b272ff27-8a3c-4877-b75f-b89ae814ca4a))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 08cab4fc-0e44-4734-a259-d3608c204d6b))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2f026df2-27cb-42b8-a2c7-23c83bbe8d1d))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 71289734-3b59-4376-91f4-3d3fc1c5f25a))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 83b99221-c944-4876-a05d-1c63e3cbf6a1))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5f3e5e0-a1e3-422e-bf68-f119a3f13051))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp c455fc23-12c4-44d7-a2b3-f2dc9840d3bc)
    (at 142.38 36.5)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 97291651-f6fd-4e63-beda-fea50285e38c)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e259032b-3fc7-40b7-8ab3-93b3df3c08a6)
    )
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 043cf2f7-83a0-4910-bc5e-5bec0a73825f))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 45bd69a0-2331-44fc-b357-6e64bbcc8673))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4ca1ba0c-2625-4c51-af84-93c942b2345e))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ad7603b1-d2c4-466d-aeb1-b75fba4e91f6))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c5b17d6e-dd0d-4978-a9b2-7530f6fcb527))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0170a62c-9394-4627-bc23-80d5ac7684a4))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 590633a4-911b-4be1-9145-5659cc50f852))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a54dff47-f14d-4554-8d06-5b5c831d6e00))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d799a08f-d388-4b86-a3d6-c67a250146bf))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e62b8ff0-d597-4245-8e31-cc12628149d2))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 359e9b41-6964-43cb-bdd1-69412bd7d336))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f9ebd39-da01-4069-98ad-f7f4e574f636))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5e59e1ad-3941-406d-8c92-965f27f927d0))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7b034d12-eadc-4027-ade8-9419ec417272))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f72c996a-6302-4958-912f-e91c87d13d38))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 02621807-f6f6-4e37-88e5-35fc28456188))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1a2d3d73-2b59-45b9-834a-ad6ecd69a31a))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 42709185-71d5-4079-9549-bbd2bcb7870f))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 952e115f-63ae-4d08-b120-088c42075aa1))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a490daf8-7c31-400e-b1a0-f069aaacbeea))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 227edbd6-c1c9-4224-90fe-d125a6f57839))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d16b10e-beb3-4228-93d0-2db88019cd9c))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 93f54e62-91d9-4f7c-aeb1-21fd6e9ac3ff))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e2fea93a-ee69-4762-a884-3491aba4d50c))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e948a3dc-44a7-478e-9718-be2cf171433c))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp c4d648b8-d223-430d-8114-2c227b47521a)
    (at 142.38 74.6)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 618b2def-841b-4e1f-a2c2-5ed6c2fb939c)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a0ef20e-94ea-4441-9d81-4d4fde896451)
    )
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 017f901d-ffb6-436d-ad1b-ef1bfcd402eb))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f295c3d-0b67-450a-b0c2-f51ee4e91b0a))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4bc24b8b-87a0-4deb-bf78-1e50a83cc871))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 518f6be2-11de-4b30-b441-c41fb3d20237))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dce72ea0-ae87-419a-bee7-c7ac9bd3096d))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 81787ba0-c6fb-4477-82ad-35e3fa07f632))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d8924e1-1230-4a2a-b9fd-aee08af2e12a))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bc43f9a1-e797-49c9-9bfa-c48f2ee9dc07))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d2fa5412-ebd6-41b2-922b-98e8e2d1efd7))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f85b1d69-8535-4ecf-87bd-4701fd374145))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 48d9e10d-c1d7-4ce3-874a-8f244abeb8c0))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8267c2e8-411c-4ef0-a5d3-ba7ce20bab31))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8533a824-ea3e-48ef-9c3b-750fa3e110f2))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a35e5929-0d9e-44db-a080-a4967c9376db))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7d7f0ee-1088-4fd0-973c-791be58a5452))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 64e97e9b-b7c3-4dba-acb9-80eede84a166))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b59623da-f14a-45a7-bc92-6e1ad0faec58))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bac3abe7-a518-4ba1-ad39-1face56adbe5))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d24954f9-61b7-4272-89cb-b53f532e4571))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dfd8e251-43d2-49c1-bd5f-4e014792c9ef))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3f694801-849a-4bbb-bf53-51a699e9ec0c))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 57dbcc6b-eda5-4f93-b48f-f1d327a9424d))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8f3884f3-e1a4-4192-a8bf-377b70d09172))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9150e277-5963-4120-8e06-3a16d7cecff3))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fd2241d5-78b0-498a-ab52-18a3286f8bf2))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp c8a3a5d9-a27b-4fe5-b77a-98b69885a020)
    (at 129.68 23.8)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8bb8fd8f-88c5-4503-83ec-94eb8b3320f5)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 924bf1e0-359a-40c8-82d9-af914d8048f6)
    )
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e11b77a-f84d-4c62-bb7e-8e243f5ac296))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3a2ad363-cc95-4cda-8351-071dc5ae6b00))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6100e6b9-efd1-4075-a41e-edfbd914d822))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74c88b37-c4f3-46fa-b1df-bbaa99667d3a))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aa8998e1-721d-4971-a3bd-e684179b5b2c))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 586cedec-a224-44ff-b500-592e55321eb8))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 69021f04-90c7-47aa-b41e-ca9aabe9e3a5))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 737e30b4-a62e-43e2-8d78-e5ceff3bce03))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7d8efbc3-b8f4-4a54-af20-4fa3b4485362))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d3bc193f-6708-480a-a587-fbc9ca07e45f))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0cc5e7d0-dca0-40ad-a94c-f5d1f749aef2))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e65ab05-affe-4704-a3eb-ebef6ebcc947))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19836137-f966-4a33-a662-c97a1e5d1540))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 22236a0b-c057-46d6-a3da-ade191d35403))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ef897a46-5333-43ae-9584-aaf4d0585ce1))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 895b0c34-457e-4270-a88b-2386ed730bd6))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 95cdae12-cf24-4220-8400-268c162973a7))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c083f69d-9e11-40dd-94ca-e9cfbdd6d28a))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c2038df1-d6d9-449e-83a2-515ab409103e))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e024fa5a-2c5a-480c-8058-5fd082bea42e))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6848faec-76d6-4c40-b86f-389eb9208cff))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b81a25e0-0692-4626-85a5-0fc61b9c2606))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c49d9ccc-63e6-4b32-9c79-2db62ea65970))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eeb14586-740e-4f9c-b3cf-b6241ba9875b))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f8801ac7-aaf3-421a-bfad-a6e5543b2ab1))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp c8a9f330-1e88-473d-87c3-641120cc217f)
    (at 171.59 21.26)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 49fb86b3-fd82-4927-9287-2906b549f310)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 923d70b7-9bd0-4406-ab48-664e06bd69a7)
    )
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 153c51a4-f39a-4f1c-8832-cc2173c6186e))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b627fcb-46bd-4eea-be27-e2da89ee27fa))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7bed99bd-b9d1-42db-a742-0e256a096126))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7f01741f-07ee-42d4-89ea-1f08df165973))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d371d2f3-af33-4a8a-8c96-4b288d22987a))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 62b8cf80-3375-4dc4-a6f0-04109325f059))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 98dd48cc-8c15-4e40-96e8-2bc5cb463507))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp baaae071-9919-49ea-b97a-5bfc635ef4f0))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c7324592-8b91-4957-a5d4-210ce2deed23))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e8dccfa8-b9b0-4979-afa3-b5fa2413a697))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b2602c5-c423-45e4-aa90-1c9d4730f180))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 55a1fbf4-7de0-4077-95cb-698e4169618f))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 686b0796-8375-40b9-99c9-0e3a1c223a45))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a8831b5e-995e-4684-867e-d5f215cddea3))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp feb719a0-035c-4ac7-8b7e-0f4be09f304b))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1bfb7800-3ec3-47e0-9778-95ff550abbf4))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 62e551fd-639d-45b9-b591-4a3d6f4a17ff))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e9f3103-98f0-4ec7-89e3-1c0c52173539))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b5f8fbba-00a6-4274-9c16-d8f1d7d82b14))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b9c72f98-976b-44cc-940d-1d1f4c8d786f))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 754fcce0-d0a1-4ad6-9765-1aba9c52a67f))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88fa0231-0567-4d3c-8bd4-974ec67e71d0))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b22e787c-ee52-4b2e-8ba6-5c559dfd5dcc))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b6b7da12-f0a8-4a1a-8861-bd9df59dda3f))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e8f70d73-3573-43b1-9227-7a61a5079c2c))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp c9d07056-aa60-4e2c-937b-c0323c40e227)
    (at 142.38 11.1)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f173bb9-6dc8-4c74-973f-7da9472cfa28)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7cc69cb4-fdec-44da-adc8-a99b0beb6bbd)
    )
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 09d1e5b6-6421-4020-8e11-4257ff1d8b5e))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f24931b-cb7a-4ba7-ac2f-4a9937396fe5))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2bee0e6b-9232-4050-8d27-1b4da1053568))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7458ac9e-ebbd-410c-8b80-9217cb8ae1ea))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac948876-9760-4ee4-9c8e-9cc737674760))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4367b362-3617-492e-882c-659c9ef368d5))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7b1cb0f6-8980-4ba2-a7ab-85795d03dced))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9a934e08-7438-4c94-8fe6-da03317a1e7a))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cd0afed0-f78e-4e0b-a231-f725dd29056b))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d86181f9-92db-4698-97d4-d0b8a2fa3d37))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1600d00b-b368-412a-8941-e3c21898343f))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 551372d8-d61a-47ab-b5a5-5f7e3c2961c3))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6e917eb8-5656-404f-a647-7c56a502de76))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c2acb6b3-c6c7-4414-b94f-1613b9a4c8c5))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eaef4308-8c7e-41ec-a359-17afdb949a0a))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 38f0b4ff-b1b2-43cd-9d93-f793259f0590))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4692deb2-90a8-4914-b763-2a9391768c3d))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6ade016a-98f0-4e07-8884-4609a4e23118))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9476fe48-3e53-4e2f-b6b4-8f0721fa0106))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ced2ae34-b39b-4ae8-aaee-0f4855ba1d30))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0c775260-d197-40dd-ade1-d6ad059d45c5))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 113c2bf2-6b0f-49fc-9626-125f86027b0b))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 11b5ed3e-7f3d-4d06-9290-6e7a26a81dbf))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6b1e8d39-5eb4-446e-91fd-65016e613585))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 951476aa-0a7d-4ce1-9119-020716d05b35))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp cf6138e4-c3bc-4506-a39a-d373c6d6cf9f)
    (at 152.54 27.61)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2cd7a9b9-9f62-4558-9e06-a728bc2169c3)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d4e05211-c6b5-4d1f-bead-15e96f13a209)
    )
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 445546c7-3a70-4faa-992c-bae95df0ba19))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 661a62af-9381-4582-88ac-63b7353a2963))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e7ac16d-c158-44f1-9c8f-1a29a87a4645))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e0c45ef2-731f-42c8-9ea1-9f2b42fd63d5))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ee20f91b-3476-4832-8462-c937f8d67f50))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0b37d0b5-0f4a-4969-95f9-844e0a5aa8a8))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1460a2d8-f1e1-47c2-af37-57d93fde0f2e))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 18633516-5aa5-4b81-bc4f-9327f86c311c))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d66c4b0d-1792-4dac-b2dc-3329c0212d03))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f275ecb0-17ab-47ef-a8c5-1491a0d16925))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2aacec5c-df7a-4cf0-be63-a5798d883cfc))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6fe9aba4-422d-4c5b-9c18-8da9bec1adce))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7eb6485f-a618-4e0f-b8fe-0fc013325925))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a3e5a209-9834-448b-bc71-5131ff63318e))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c0453ac6-f763-4a37-bc79-7e50bef04933))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0429f029-ce75-424b-8f97-1bc94697cfc4))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2546bb09-6bcc-4e9e-b4b8-28128368b4f4))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e3c1549-5be5-403c-baee-aedc1ae588a5))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b0d69c65-928e-430e-87cf-270daa658a3c))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1192e97-24db-4b1d-88d4-8efb34b83f79))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c4987ee-a4cf-46aa-bf0e-5a174f30a1f9))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 81587903-f8d0-40c9-8899-e5bdf4f26b9d))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 94747729-38dd-471b-8f05-68bbe979ac9d))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bcebc5af-392e-457d-b3db-61ba2eaeab41))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8d57e8d-cc78-4fb8-9d40-6de49e644f51))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp cf7361d7-b1a3-440c-b3e0-cd749865cc4b)
    (at 165.24 27.61)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1a100b11-dd46-45a0-a294-9c83718f4796)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d9aa9f5-56d7-4557-b06d-0f2feea063f5)
    )
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f8e279e-d914-4526-844b-266f324636ec))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 638455a8-c5c4-4026-a2dc-03c588871485))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c111bf2-44e1-43fd-9eef-88310b45e71c))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e45b6c2e-2977-45ae-ae27-93e1628ba06b))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ed8b0cda-76c4-4dff-90e4-7e2b78581859))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0634cbc0-49ec-4d13-8226-1f04800981e4))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 06e63009-37d7-47e5-a594-7b491236065d))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50c31151-bf54-4c31-9f47-7f93cdfa3c4d))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af749e61-6390-4b38-865c-ab4aa92cb492))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c3e2905c-493e-4d5a-8830-133b49cea763))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2d287a2e-2012-4a8f-a560-dd826d64f094))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6eb3f172-5f61-4d52-9a65-7b23a34647fe))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8dbe34b4-034e-4dd2-973a-5edc502db201))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a6375007-613b-48fe-a464-1a9dc50cc6a6))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f075eb89-7d1a-4818-b36b-e2a069b817f1))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2527e5a3-21ab-4840-bfd0-66c131c22a63))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 387afbc4-55df-48ad-879f-d6a8cf7aa36e))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 38fb3065-af94-4fe6-8944-4491b58b1e91))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 56ebaa27-f2af-4cf7-846f-ed2078b77272))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 951a9d72-c233-4ceb-8037-2199ffdb4e5d))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 07c56fe8-455f-4692-aadc-6da3199584d1))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 11ee47c0-9904-44c7-bac4-d14ee7b98a1c))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 279a092b-ae53-4b4a-9131-d85037cb8799))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 69d67bd5-4c5b-4e1e-abef-3194750cb071))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f08192e6-6357-4919-a6bb-ea6ca020c829))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp d747c19f-466f-45ee-8c56-706f9600481c)
    (at 129.68 49.2)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 01c4202b-4e7e-43e4-a53f-2863239b644f)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 523d7580-8013-45cb-971a-5a2567da4a2b)
    )
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00c36610-f788-4c36-87e0-80e0c72a562f))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2ed4c7d2-f105-480f-816c-a81cdff874c9))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 852dd56a-d8eb-4398-b1c1-6492d3193d27))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ad19279f-40b1-47a7-abf1-2da65912e5b5))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bc2bbd88-16a8-4435-a648-4b8e19cab956))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f394630-1ced-4044-a0bd-47181261f419))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a220317-7a96-460e-9f18-67dd8799b983))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 76b24605-0af8-4d9e-a0e9-6f5d5cc3d4e7))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b7b94e50-da5f-442d-8176-c302761a5863))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8755042-561b-49be-8087-3cb8b638e9bb))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 026fd1f7-9891-4e54-87d2-9e60ffc2f103))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0fa50026-78cb-49c4-ac67-844b5fc56b74))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 22500b56-317c-4317-a946-213fc6fe8275))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9b6d3e0f-64dc-44b9-b275-77d02a939b71))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c38b7f85-1d2f-4dc4-82f3-e97902146531))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 33d1b66b-3c0b-44c9-bf3a-f06d8dc390c0))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6cf3c7a3-38b0-49b8-a33c-a3ce2b8092d6))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ab42cd4d-23e8-4a2f-a0c8-7ef3854ef39b))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c693e725-5407-40f2-a444-a141ff044059))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp faf1930c-c412-4f86-88d8-c982db621323))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 05694eaf-dde6-41b0-879c-7d4220367c1a))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5959ca69-d760-43dc-93d0-c2c233834c4e))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 636fa99d-427a-49f4-9dba-94e54623c930))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9bcd76fa-cc4e-4855-b007-ec5460a490c5))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d6fa47be-8301-48a8-984b-ea97eb2d7b26))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp e7490b4f-9a5b-4874-89d4-0367b6316ff4)
    (at 158.89 21.26)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 06c4e8d6-0e6f-4c54-9c0d-a958e1a8139e)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ecb3806d-8e6c-41d8-aa36-5900d373c34a)
    )
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0ee1f4e3-62e8-427e-9a46-fc831f5cb411))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4475090a-907b-4f32-89e7-f42384ffe4c3))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 55793a60-571c-4511-a8d7-63067c38e32a))
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5e1a985c-2cdd-40b6-b9f4-7c8368561274))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c9b2755d-74fd-4a18-a01e-34294f8131e6))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0da0f27b-7664-4e92-aa74-3c5796ddcb3f))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7795f0c0-7732-45d0-9083-8504d1ad5032))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9ec9658f-c042-4ce6-9d87-36c544dcb415))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bbad573a-75a9-4ced-951e-6525c268aace))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dcc13d48-7d8e-406a-a0f7-c34bb048a807))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7075df02-5d78-4cbd-934a-e97207f02d3e))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 76d88764-5b34-497c-9c47-a177fa0963b2))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9fd95b8d-b197-4867-8a4a-76a10d012f50))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d11ab460-63a7-410e-8201-a20f16623a69))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec6269b1-5983-4224-a7f4-3ec123802c84))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 22a63e40-0501-4299-97ee-458e6ea0d109))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a57eb43-31b2-4e7c-bfca-0e7859be1cc4))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b3332717-bde9-466b-90ad-bc90579fb998))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c141ab9d-26de-44a3-9ea8-d36c1b84459e))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5f95ed7-2f58-4def-be10-0049a47c6915))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2c85f2f3-3df2-444a-be3c-7e2cef0af0b7))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 800afec3-2a42-4776-b92c-ee3a4ef2ae31))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e4dc759-0c3e-4802-b83d-52ca4a4c22dd))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac965528-921f-470b-a961-ceef0bcf501a))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c6a3ad94-5468-48ae-a3bd-d97d92b14025))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE) (tstamp e9ff9848-ceee-4df9-a4a2-d7dc8d47756f)
    (at 165.24 33.96)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca9d6efc-157c-4878-a5d4-fa30bcbd09d3)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 42d6a08e-47c8-4c15-b0c1-1128f61b4e1a)
    )
    (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2dbe9fe0-99b1-49f6-ba42-07ad1788f40f))
    (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 470f8a58-aebe-4262-8fdd-d9801f5d397c))
    (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9cebfb40-1691-49ad-becc-8dd1ff332b72))
    (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b2dff0d5-0750-4a2b-a111-a714910ebf8b))
    (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e81080f2-954c-43fe-b26a-aebfdc2e8ed6))
    (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6cf5565d-76cc-46a0-ba0f-ddd897d9f4d8))
    (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74c317a9-8d24-4d70-8cc1-11c59762c3aa))
    (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 768f6128-a2f6-40be-8447-7f074d903128))
    (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9cc73409-86c1-4022-b4fc-50ddb51d5657))
    (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c197c896-1a08-4bb3-b5cd-971ec5e13295))
    (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5c125758-f0a7-454f-a9d4-593cc757484f))
    (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5e9dd39b-be66-4f93-b828-a679250e7879))
    (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5ea0e912-c723-4619-b091-a761c275a484))
    (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9294677f-7e6f-41ad-9b9d-9ad625d6eea1))
    (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c155146e-974d-4dd4-a53f-6f4f49ba416c))
    (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 08712fed-d345-428c-9dab-80a9de03ffba))
    (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 129166ab-8c68-43d8-881f-e4fd850a50ca))
    (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be81b3c6-9c18-4c8d-8440-c15776eded34))
    (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ca7f50d8-c23a-4501-9468-a478e6da2d10))
    (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d94c5f95-ef6b-4012-a862-7da3b886d254))
    (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 21959b34-1c6d-4b16-88d7-346224bc093a))
    (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3b3d26e5-3981-4f74-a4ce-8d93d783cb9b))
    (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c0159c9d-0408-46c1-981d-c5f7e3da0c8b))
    (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dfff956c-3419-4207-be29-39ec639e2aac))
    (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e55cb3c5-3304-4c3b-a0aa-362f00d51672))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp f073b120-30bd-41ce-908e-9d1aa3c86208)
    (at 134.76 6.02)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0497c32c-8092-4f2c-803e-9afe3c592b96)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4e23e14c-3061-4ebc-8d8c-158ebe3c8b0d)
    )
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 048e4ba1-dbc3-4b9a-9b4e-717d841e1d1a))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e02cd4e-edbb-4a23-9b58-ba6be855c9bd))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5825099c-00b0-4516-915a-2c384100ae80))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ce427a7-eedb-4f70-8ff3-5d880f9e07e3))
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp feaa8d17-965a-4741-986b-9d8818230732))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 203bc26f-9d52-4392-bb0c-505deca75eb9))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a3fdbc2d-0298-4936-a117-63e33a092350))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp afeac08f-fca1-4c1f-b4f6-a465056a3b91))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be7a1650-cded-48df-b847-92b7ce4170fa))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cb568f3e-b0e4-42cf-a84c-317f7b317dc9))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 23f7062b-1b53-42a3-bc70-8dcf916edb02))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 490af31f-e15f-47bd-9fe0-6c95cd307746))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5f714be5-6479-4142-a5d8-582ff9cad6b3))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f401e67-db02-4f10-bfad-1f0c8ac8cd32))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ab948cbf-bf98-462d-b3a8-a397f7d26fbd))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0ae64af1-f06b-414a-bd94-ab3a3cc36add))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b5947cd3-7fd3-42c7-af15-c4022f864267))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b6c6fdca-6f4d-469c-9bc3-370adadb3b4f))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c528b828-7b11-4c9f-9dc9-8a12b8cccd6a))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff40d261-c5b2-4823-8e97-8d2e87ffd291))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 63511c1f-04f3-475c-b1fd-c7bd238265ba))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d7da2696-35de-460b-941b-c7dfc99bad92))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp df64d80f-7caf-4850-b491-40fe9fe5b890))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e86f7cc4-73a3-49f4-8054-9450f4a3df88))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5e3307b-f667-4321-bb98-e0f40bee4398))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp f94092ed-aadf-473e-9b90-1a3b96800afe)
    (at 129.68 74.6)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0dcde7d8-adf3-4f1c-a823-55c142d1383d)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6caf7133-1efd-4b93-bb0d-f49c0acc468c)
    )
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2954a767-f575-410e-b11e-3350d29789a5))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 43bb96aa-211e-4be9-8f21-816425bff727))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5e46cc3c-07b4-48de-aea4-52c10d882fbf))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aae1a7a1-df54-4b9c-955c-fa3561589904))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb306c35-e1e1-49f9-876f-d2ff717ceda0))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0a823cc5-6cb3-4a9d-a92f-90099a92f7f6))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 27908d0e-98c8-4ae1-9a00-211138091047))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e4f3705-9978-46bf-888f-35272a093719))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 49dcc200-2f5b-495c-855c-6673b894c18b))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp beb37848-c934-4fce-8bcd-35ad26edfd04))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 07675190-c1f7-474f-8046-d5c5b0ded95c))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e7bcfd9-009c-4cf6-8310-5938210f6ff1))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 898915a8-2838-46ed-8644-4b040ad8a3fe))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d48b1a30-9cda-488a-b0ad-f3570afad5d8))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp efde1eb4-70ff-451f-b5c7-ecefccb3fb89))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 08624e61-0306-4819-9580-382540e2584f))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5475e6ae-5ba5-48ce-8d2c-5cdeaa8d95e9))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5753ad99-f9e5-4525-a9a5-f697734c4c31))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 860b396c-f31c-4470-8e1c-702283cd0faf))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f9916673-a6e3-4b44-9d40-fefb3a1ed400))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 07deb088-7187-4b5a-ad59-fe1ddc8286e6))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 312d34a4-393e-4388-af16-2f102342f4e0))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp acfc150a-2a49-489a-8b45-3efae7f9f20e))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b9e5b4cb-917f-47d0-a4c0-35deebf2ee83))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d29572ce-b6ae-4b52-800f-a053f573facd))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7) (tstamp fece38ca-ad72-405b-80e1-3dc40a53f464)
    (at 147.46 6.02)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 66099011-9e59-48a6-9eb5-67dbee95fe68)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3750cc70-fbb3-4d07-9053-17644a1f2fb9)
    )
    (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 009f86f9-3293-42be-83bd-95b4f88b0172))
    (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0cad86e3-9bc6-4560-9f76-351b0fbe98f4))
    (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 21b89e0e-f0d8-4462-98cd-ef5bc205dae0))
    (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 44fd40c7-9768-4a95-9c73-8b128fd48ea6))
    (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 95343d5e-ac50-45cb-bd4c-75ed64e67f61))
    (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3fd3c7f8-bdfb-47ab-aec0-f2125ec1eae5))
    (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 60a602fd-6220-4fac-a740-da6b6da4ef15))
    (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6dfaeb88-a747-4df8-9303-5f442bd05a2c))
    (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7bdcc561-0367-4f50-b211-f9efac938f5a))
    (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7fbaa73-a040-41b9-a807-c664f78c497f))
    (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 015e9a5b-a445-49b5-b31f-e87fa11926b3))
    (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 699444bc-f03f-490c-a1df-d6bbc038ebe7))
    (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a67f9584-d054-40c6-9fcd-2971ecab57b1))
    (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c25f12a7-a153-4dc4-b569-ed0b2348cb15))
    (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e428ce89-cc05-4250-9ec6-cfd4f84d174a))
    (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 04280b6f-9828-42c6-8d66-c8bb44134645))
    (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4c512461-0f92-427f-8e87-e8d1e5b5652c))
    (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aee2b7bd-ef86-4628-bde4-fddc6f1fe80a))
    (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af767cc4-d8ca-42fe-9560-8bc22599189d))
    (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e215013a-b11d-4e3d-bd3c-dd34344cae9c))
    (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0868b856-bcb1-4c7b-9bbf-ef09867784f8))
    (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 13ad10ff-5a5e-4271-8976-ab764189f2cf))
    (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a127a3ec-c1a2-46f0-bba4-685be7b998c8))
    (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a5bb35c0-f468-42c0-92a4-4f0db8f9564b))
    (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be1dc6b8-6389-42e4-8ac5-801340b1f321))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 0406efe2-3853-430d-9174-584b38930fb1)
    (at 152.54 61.9 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 71f51ca0-0516-4ef6-be4a-c8a3312ecdf3)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f2760c34-228e-4e92-94aa-9feb53abb476)
    )
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00e76209-56f1-418c-97c7-1e7c6c85db01))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0bb32704-c996-46ed-ad7d-f8590fb50f1a))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0c37acc0-0537-4a1c-8698-38585560ada3))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 85d84a29-f9fe-4d07-91ce-57406fc3b783))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f9130e1-ad73-4e7b-b94e-3b0f81e18f25))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 226b9608-52bf-430e-b01c-8f4d591fa4e2))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 26fd8cdc-baab-4e82-9854-02440e8af28f))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3cbc450a-d527-48c4-ba46-4490c4fb7fd5))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 980d6c05-949d-4203-a079-91fb59395c24))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f06f1a96-ed29-48e2-80f4-948c97136fde))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00989d42-08be-49e4-8de9-40e0bb8fdc50))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 583e3aaf-4552-4460-b2c4-492b981b1e22))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6bc4ee74-ad6d-4452-8d8e-feda7abefcfa))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9af05e64-0db9-4ac6-bdb8-9f752d8f8e11))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c8948b59-03c2-4b01-b682-879e24524d03))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1bf33843-9ec1-4181-b2bd-8cc23dcd3438))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2de43b43-8312-46a1-98d0-3b3f6b2cd56c))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 97f6f426-beba-4a41-b89c-cc492ffe471c))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a9adc687-5600-4e57-9c90-916e57f57608))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b32e4b3d-dc6a-4c8f-8b69-190890557c2e))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0026d9e4-4e3c-4b0c-9ac3-aefad1392b7b))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 340917f5-7b06-4173-bac9-98e1c8e08adf))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8cde778a-38da-417d-8ea8-07736e5f5a57))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp adf9b552-c354-4160-a582-2c733e9f25d6))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d44b4ff9-7d16-47ea-9d4c-1bac0556b75c))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 0f27dd5b-a900-4256-b378-23925c6399b3)
    (at 147.46 84.76 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8b58e510-fbb6-4717-a7c6-90bc81cb05b4)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c07eb2c0-7358-4588-a2e4-02c7edc20e4e)
    )
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 09d58945-e2bd-42ae-a359-eba84d0adaed))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 46d2108b-9027-4f9c-a96c-1c0ec657cec9))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 582e36af-537a-4b3d-a2fe-7b95d7f43a49))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9ce6ab18-3384-4e07-a004-b0c47cfc6f99))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ba651e10-a595-41c4-ae6d-363c100b022a))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4925a193-9be4-4d74-aff4-944d139cb91d))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6a752b39-62e4-4843-a151-e5f8c1d771a8))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e866b3c-61d8-48fb-8a51-d4dc3f02eca5))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a55b5857-21eb-4a4b-8d7a-ad1cd1e4f382))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d096f49f-f781-4abf-8efd-efda19950a28))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0daff4c1-15a1-4a11-966f-a7a56feda931))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 63d3e2b9-bca1-48ea-8373-1718bc9a2018))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 93636137-412e-4e22-b356-848a5e08a623))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9e4753b3-ce17-4cf9-865e-e8789419b818))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c26f35ae-eb2f-47ea-8145-46abce721503))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3cf3738f-cb9c-4a39-8f0f-cf85299926ce))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 54e0237e-2c7d-4a28-9407-38cf538163c0))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8b7bc462-edd9-44b8-9aa8-ea37f381cfc5))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 99ef0d8c-217c-4490-a0f7-59683fa3c689))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e9a19f85-bc19-4d1a-8675-ebcc3ee17d46))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19dfd09f-fc1d-43e6-81cf-b1abd540c6a8))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1abc9017-4c4a-4d88-a76f-3dbea07509b7))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8b533ee5-441e-4ce2-8754-59b54afffd18))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 960d8c9f-c0f0-4b20-a5f3-f92e89ec2a9b))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fbf90dc8-9dca-4122-8b72-118b3191750a))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 13603671-cb48-4522-937d-6d63fc4d65e9)
    (at 125.87 39.04 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c3d07540-cb74-4bb8-a5bd-09e248a520d7)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bf62f59c-7fe2-4c87-9bd2-998ef6170dda)
    )
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1e21508f-db9a-4bda-9d51-18b6175e0f88))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4ba48fff-0ab9-4865-aa01-12f3825f0a77))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a04d69c-f2bc-4f4f-9de1-8fdab5d5bd0c))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8d42ea48-b7b9-45f6-a694-de8fce3acb97))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 95209272-2629-4703-9447-adc9362a6a78))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 799bb96e-125b-44c2-8669-bd6dd6b110eb))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8448f3f4-b4c6-4f0d-948d-c5ebc34d94a5))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c63d583a-4c34-4ae4-9637-7ed3973406b9))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d205ea52-0f71-4de4-baa4-1b29cc07fe37))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f0b46229-da90-416c-8f84-4e74937daf67))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1133287e-ebdc-4fd6-9805-76b1b574d053))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4007ff59-265b-4fdd-9316-c88973179838))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d52433d-70ae-4a60-bf5b-f29e6e63ea2f))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a99bb7b5-bf8a-481e-8ec7-bdbf4aba7dd2))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c391ef2a-ebac-43f2-8298-88a5040f1f3b))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 53dc63d9-16de-482a-a87c-4f24c315802f))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b9cdb05-4c8c-4172-be15-a418c1418298))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7d392427-0517-4a53-850f-3b4094447750))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a2e69542-504b-4fa8-b4ad-7551b00d7871))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c20b9f0e-9c4f-42f8-9b27-ed53cd8680de))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1380fe32-8693-49cc-b34e-550ef62c6701))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c0538e0-73d0-4663-b867-2366468d7baa))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a41c1706-12b4-4602-8ce5-2e712b5b5dd3))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8de8193-e393-4ca9-92c1-1c61597dfde6))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fe6d7931-be8c-4c78-8f18-b9708112bf8f))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 1478bd67-34f1-4658-bbff-048e37f8bf65)
    (at 157.62 74.6 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9e92a9dd-c111-400e-88d8-99f587760452)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 66b9b309-5081-4bee-a57d-5cfbbf9d4faf)
    )
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2124be0a-491d-4aec-9ba7-b13a89e92077))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3d0a8253-17d8-459d-886e-6a5eabe3ec69))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47857e0e-bbb9-47b4-92d2-2c45fdd49d74))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8703a0f9-9938-4d95-a058-1bdc6d6bc3c4))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f165fc35-5a96-4f4e-bda6-da27e8f973a6))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e1c90bf-5079-4eb1-b981-962b39f5a9aa))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19891985-752f-49ad-9cca-0e39dd5e999b))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 24a440be-1bc9-476a-bdb9-cfda721ab338))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e2391874-e59a-40a3-b664-b241c398a889))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fedeb893-b406-4ac1-9002-b94aec6bb077))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1283961b-273d-4aa2-a901-9b06ac2a6afe))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 78dded0d-b7d3-4dc5-8dc8-9bba6061069e))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 805a2982-7eda-4820-9e48-4e33e4496aac))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c68789ac-ebb7-48ef-9cc7-a5edbeab9fd9))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d1fa054d-85ea-4ec8-81ab-afb4d50d8496))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0d7dce41-64dc-46e4-ba49-c808efa62681))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1111b147-db91-4f4b-8904-bac94c2ec54b))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 500636cc-0a24-4e26-9ae9-ea4676e96aeb))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6573ba70-7f15-43e9-bda4-579cc7a35e63))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a3cc90bd-9a8c-489a-8f4c-25fd1d8eaeaf))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 87bd78c4-9ef7-455b-a814-6be9d3fc5068))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9fb41312-2ffe-4f22-9cc0-8c3dd66fad7c))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a4c3ebf8-9b82-4e94-9ed7-0c6be1207388))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bda343ed-6533-48a2-9e47-43af1af03b84))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dc5d3273-c5de-40b2-9b1b-6ed314236763))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 150b99fe-680c-407f-9e67-a35ced616c92)
    (at 134.76 21.26 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bec29cb9-0265-44bf-87e5-9e58e59e9a5a)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 47b55dcd-ea0a-4a22-aaec-59510f4ded4f)
    )
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 230dd90e-c44e-47df-96ba-6e1303703234))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 696e4c3b-ac2e-4830-8081-917407c260bc))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74f71e55-a3d9-49b1-962c-1880c18614a6))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8f0243e6-4c78-4977-bb6e-c176b7a04f86))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c2b4e105-c1eb-43dc-a718-ba6a8bf48fa9))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 576f8660-7e1c-43e5-a3c4-ce66378f389a))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5d78a343-277d-4929-935b-9c5c03acd318))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 698752e4-2510-4912-97b8-b15039b180ce))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7e9e1da1-8d11-4bfc-be21-a4b39d9f26ec))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp afd7e55e-be40-4b5b-9c81-387bb7f9b452))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 443f04ff-dada-4e04-9eb3-8d6a71774c00))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7f7ed847-3373-41d9-83d5-61f1c51c7527))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 85c1b788-fe52-42ca-b674-13db6fa740cf))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88e53c19-10ba-45de-8ab9-394f27a3f962))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ab688566-c276-443c-9495-882856f4bc94))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 244d45ca-3d2b-4d78-94b9-f3fa3f2d9a8c))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3f110ab0-970c-4845-9865-794dba23171a))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 474969de-cbd7-43b4-916a-bc139319b522))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5be74350-e225-4cae-bd0f-f28d7e5df5ac))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 60b22f4a-91cd-412d-857c-b3eaa1493ffb))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1581d477-2c89-429f-9651-1163cf171863))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 32740556-e6e5-4141-a505-f6340f6536bf))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4c07a3f5-fe8f-4ca0-aefb-72075878999b))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ef72a6d-0b53-43b3-970a-8503c2e34e4a))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c1a7522b-c8d7-446e-8d39-1067088f3237))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 17ecec07-54be-4b54-b829-e4716d7849d4)
    (at 129.68 49.2 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 6391c549-dbc4-46c6-b2a0-73ec3d812473)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a1c7e054-190c-486a-b06a-4703957747b7)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0203e795-c187-4081-8b50-11b2fa2567ff))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1e61006a-11ac-4cdd-91d2-f3f95dd440a7))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2b6f41a1-3657-40c3-aa39-9003cf34cd27))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6f51874f-bcab-486d-9f7f-6c6a80510384))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 86d1b32b-5307-4478-a1d2-268c0ae3b492))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e8080d3-fda9-4091-960c-7665d00be727))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 454ad794-3d24-4e28-ad85-2aa9bb758a7f))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8172b1bf-6d66-468c-b081-a22a17756b96))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 98132b3d-3a9b-48f7-8a8b-d4308bab1280))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f4076bc8-9ab0-4d5b-8a70-fa1815aec2a6))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 289fe748-e3e2-4a44-a1a0-18609be07cdd))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 71ced7d5-a3f1-4cbf-a84b-4079b2440bfb))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b40618bb-8717-41e0-b3f3-e363438fa2c1))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dc80f542-0900-4b7f-8af9-1271af846bfb))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5fb07e6-c23a-45ee-aa05-31d51961bd66))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2eb8c0b8-3eb0-4bdb-ad72-7a6375b67d2f))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c06d844f-5e09-4400-8912-e06377bea4fb))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d2a54f58-f489-441e-be32-abdd51462c00))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e0b381c4-47b3-4cd4-be9a-577109c7f5ad))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e268c7f3-f464-4de0-99c7-be2b0cf6adce))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 02604891-8be1-4767-b32d-1b63d6494055))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2cf4f656-e0ea-492c-a044-09faf4a91c37))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d52a453-580a-45b4-9b29-e1744fbc4f80))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d061cc07-6459-4a8a-95c1-06ec53e98407))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e1597c6a-fc0a-4326-a32f-69f7023aa5fd))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 17f913f4-ae0c-4391-873c-6f2248790dcb)
    (at 152.54 0.94 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d74d2bec-bf3d-4d80-b999-f701c8d96bd2)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4386c086-a30c-4e80-82bf-3f6057ac9937)
    )
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 264f2e2b-c9a3-4b3f-b06d-ca858f415ae2))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4fc7a879-7313-40b9-81e1-558236fafb7e))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5fcdbe57-b244-4efb-a027-df0b4f8ab9a1))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6d116a74-26cb-4b4c-a361-88cdec5aec76))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 986aa279-5259-476c-9398-75a70243ad21))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 48c4b6d4-f91c-40f7-860c-8f881ca09763))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 549eeaca-12f2-4cea-b53e-fe7b7e4f5d84))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6167b3f1-b4aa-4aee-abac-739c31f3a9f4))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 67ca210e-e6b8-40ac-be9b-d1c3636123f6))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f59bd353-9c06-445d-ac2c-85465c0692c9))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 77650455-349f-4db8-83c0-e9b377ef3505))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8557755a-d414-47cb-94e0-727d5ab532a9))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp caaf0524-121c-4898-9ad1-c022d5c2905e))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cc228fd6-35f1-4864-a1d9-e27c5c2ef38e))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e2ab2d04-842d-4d75-be98-ed5458736313))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 01613788-9de0-4fdc-84b7-b0a21d517a9a))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47d70525-df09-455e-a2b0-29dbc5b80833))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5372e148-70a4-4217-bfec-6320993b2dd5))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a0245d16-9d62-47f4-a542-81d583c805c5))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f0e6d01f-1f0f-452d-af56-be299b84481d))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0962d502-1a53-427f-9757-cf66f6e5475f))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74cd585b-7810-41a2-a939-af0104eddb26))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9888ba00-f5ed-4943-9cfe-bdd0946a80c8))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp adce9970-16b3-47e8-b54e-44aabb400abb))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eb7062af-534b-4341-b9d0-8b6eee74fda0))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 180b39e7-10cc-4019-a344-41265275222d)
    (at 157.62 23.8 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bd107ae3-6d3b-4b9e-af9e-370e593fff12)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1818ecba-191d-4a75-9d73-c70b21f3c72c)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4284d7c4-a16c-4d9f-b697-522559cb6f95))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 533cd5e9-11fd-402a-b3eb-2a4952abbb08))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5ee482ed-b7d6-40fe-8300-a2f90a263c2c))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 66dca4fa-11d8-493d-b2ab-22ff3e167e6c))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af77a8fd-bdf4-4090-b903-411878bb7c8a))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 70692350-a45e-45aa-9ee8-116e5d33ee08))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 87268b15-3be2-4d2a-b95a-d104f9a959ef))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a2f6a610-1462-4df5-b1e1-1cabc68cd9aa))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a3732212-a876-4a5c-8464-5b1336aacc4d))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cfb59385-008d-41d7-a0ff-9e6494947a3c))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 15a6ef4f-cc9d-4728-af85-b85d8b6fc30d))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ae3cf6a-cc59-4323-a413-a2d5d170f2d3))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aa0ba2a4-c547-47a2-bb2e-9cc0048d35de))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ae3253d2-1029-4dad-809f-2e14287c56dd))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d623e8d0-b41e-4f07-b922-6fd76c7343f8))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3852641c-750f-4964-ae90-3a73770d2c34))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 39e5b030-dfa9-4d77-a767-43db8daa3548))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c5fa2ef9-7e69-4550-8e46-bd2a50f9a1e6))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c64cc64e-ab89-4212-a17e-bcefbea3c9d2))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3892469-9eb2-4f8e-a9fb-8df9c2dd149e))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0b181814-29e4-4093-bf8f-506286910f8a))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3b2f971d-037e-4d86-85bc-1819edcfeb93))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c404961-7386-445c-9fed-70644b03530b))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a98f089a-54a3-4657-8882-04c5993e2777))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ae3b93ca-9961-48bb-a7bb-abac95472ad4))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 25625558-c987-45a2-92f0-10839a9ae2a1)
    (at 125.87 27.61 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bc7170f7-dedd-4ff1-9fdf-0b0c2bcaaf7a)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b3771f5b-9bf8-4413-9b85-85759242d485)
    )
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 15aef296-b8fa-429c-aa72-08d3b93b771a))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 53af0367-4136-414d-81ca-51e2a9b7651a))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 766634fe-7d23-4187-b43d-28dbbf711675))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 975fc1d2-9b18-4497-925f-0c1c3f9732bc))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ca618b56-bef0-4ca9-8e2f-e4f2fda6d3fd))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3def6de9-6ecd-4849-b022-f793df15421e))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 67812190-fb53-4f4c-838e-db6555b35b46))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 731742e6-8c01-4c8a-9519-9a3a569f4b06))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ca75a36-e9f9-4d91-97ca-bfbfdbc01e4a))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f159ec3d-a0ef-4830-bcc8-edd415f3fb70))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2343d015-08c2-44da-80ee-657a5ab5f83a))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4db72202-70f6-4f7e-bf12-8546ff4b8a1e))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5f507234-9e25-4024-81e8-b15719e08a51))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a276741d-ebf7-401a-b530-b8b19ebb5e60))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e7af6cbb-ff63-4714-be06-0bb30a4523e6))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 824b54f9-e4b9-4f5f-a0b8-aa4b0f5c5fc3))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ac8e48ff-e9a4-4622-80f0-a42c38010e55))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8f34ed0-2835-445b-92b1-f6c106f55277))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d1ad2c63-9ec6-4ec4-8306-cf907ed38699))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f098301f-3e25-45a3-b119-4f6f62a545c8))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2dcc3ad9-56ab-44a2-8896-6be119c24faa))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5ef2e9ec-19d3-492b-877b-d16c58d9f3a0))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a6d41995-5709-49c8-b366-323f22d09acc))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c23662aa-b9a6-4115-8bc2-d5ddbd8935b2))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ed80fc09-6063-4a1c-a385-11bce998741e))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 3078d5b8-5a56-45ad-ba67-fd162aca9c88)
    (at 144.92 11.1 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4436254f-5bc7-4162-a127-a5d737a256f4)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8d1869f9-1a1d-46ff-bbc2-092daf508579)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0a5fe1d1-6062-4a50-9a76-72cd52f9ac96))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5772128f-0d7b-40c5-b709-e751bb6d10cf))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 830a296f-2d4d-406b-a214-bc8c82f6015d))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e925328a-90e6-4169-8b0c-198135cfb25f))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f24d733e-4b57-4a6a-a242-9bfcf6c355c4))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a780c9e-0947-4e0a-b6db-281ceade630f))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 682c54ca-73dd-4132-abfc-14d56f33420a))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8a0f8a1b-b2eb-4274-bb30-8ae48763df33))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9e55e638-dc1a-4b43-be3c-180d94803225))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bcf85b57-4994-4aa2-986a-d39a43db3aa0))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5c384ac9-c45c-4404-b8d4-15e5c0552285))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 617bd779-a8f9-4ac6-824b-085e4b465ed3))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6309fc43-0a09-470d-aa7d-faaf1dc8572d))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b2422d38-1460-4453-94fa-2520ebde210d))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp deb678f2-bd61-439a-a669-4733281663b0))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 12f0aab8-52c1-440c-9530-99ed287bf0ec))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 595d7068-775e-46e9-b5da-2f00a3d01526))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 823d012c-ec82-44d8-a820-2ea8ec748223))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f6160f25-15f1-4e23-82d3-54603056ca48))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc14e574-a9e9-46b0-a1e8-342e86ac5262))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1be6e2ef-7bcc-4f71-a31c-6a6687385859))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2ced1aef-aa28-4a9a-8198-46a08c7f640b))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 31b5e49c-0e5e-4015-b042-f6f110b9ad7a))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b17c6730-bf79-493f-80d3-7b3b2a44d491))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fbe21144-4f6d-4c7d-be6a-8fa60c440732))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 438e4211-82f8-4aa4-b620-1aad56fb0490)
    (at 147.46 33.96 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 65d20463-665c-452c-96fd-4969b5b368e6)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b73d6f3e-7e39-441f-80a0-afd92ebe9e26)
    )
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 30000884-d031-456c-9f1a-d6424e7af9e5))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3726e3fc-cf70-4598-a19e-8c86186271b8))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 509c8788-4af8-4230-9e7c-2635732f87ea))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 916a52cd-a6ec-4c22-b593-27eead9ad6e7))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f673b58-9052-464d-b72e-41099b44f09a))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2ee8ff8c-7ec3-4076-bc97-16da5a84c395))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 863e7fb7-392f-4309-aa1f-f9a7684ac786))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9050f383-6bfa-44fa-a9ba-66c375da29f4))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bf06f43a-baf1-4f28-8cc3-52df0fd9fb69))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e5b7426b-308e-49b5-9ad6-7f20436f2e77))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 339e1f7b-089c-44f5-a21c-186ec5fc08f8))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3ab0523a-65b0-4c3e-9381-c4ec97b278c9))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c36cd49-8dda-4f2e-98d8-88031fbbe645))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 72b16a79-1030-4666-9a29-b8e2d456caf4))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cfcf0f3d-9b79-4ca0-a4b7-02cd8622ae29))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6caec61a-23f6-489a-b34d-077f014e8684))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 904f9160-5eb7-4913-901e-bfb4e871b188))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 975515cb-689b-4c58-a7d7-084c1bb51223))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c354eb51-9a7e-4360-8275-05811769ad66))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d04e8ff8-e6e5-4054-b238-9eef3dd758b8))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 33284a47-14a9-4c4b-aace-7914a47f4519))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b1971cf1-c56b-4b46-84fa-22d25c6bc0e9))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cbfca8f0-31d1-4cf3-ba3f-1bc99380c394))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ea169683-0a88-4294-a7f5-85774e59e3d7))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc76d09b-30d7-40d2-a463-3920f6d84a68))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 45731c20-1ee6-40f9-997f-fc53764784df)
    (at 152.54 6.02 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0c74d9b7-a38a-47cf-9ed4-50d7217bb455)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4e18cf60-d50e-4e55-bf86-bde14e91c150)
    )
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7dcdff1a-1802-432a-9021-a04c144a706c))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8554e88c-d7ea-471e-942e-510a8c86f1ca))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8860f65e-d313-44da-a337-ba863f25bead))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88b5d334-b542-46d8-949c-7feadb648e78))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cf2f54da-f7ce-41ae-aed7-378a08021d78))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0541a206-47eb-4946-8e74-a00e27104e92))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b4108f18-b31f-49d1-afcc-7a2f232f0940))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c3d0cb86-3257-4286-aa16-cc9f7a0456fc))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cacbe27c-0be3-43c2-862a-8860581b21b2))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e77f09c9-76cb-4f6d-a7e9-314980c86a5a))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 250f6802-aaae-411c-9ac4-5f21765e6f61))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6f59e327-3c4a-449e-9c3a-4f9f59101152))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8a9c71cf-9c52-4103-a41e-049203dac514))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e18677c6-8536-4724-81b2-0113ce54a05f))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f02d429c-b0e8-4c91-b3b2-cd7cf34137cd))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19adbe74-f0e0-42a6-bede-5c527b434d23))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2165dd71-122a-4813-9262-8b4ec75a2968))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 30384e59-62e6-4905-9d87-a94a3b53facc))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8c4fbe41-4232-4a65-b6d6-5f03732b09ab))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8fabda7-8e26-4972-8f3c-28567fe1c3e9))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f5cd513-b788-4eef-a430-b6ed38c2718d))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b8db7ce-6ab8-4fde-957d-7a6bcbe9340c))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 62b21101-e266-477a-93aa-feb349dce3cd))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a960f8e9-4503-4c56-8c39-d5e653e593d1))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f2bf2146-f07a-460f-85eb-ace308d24808))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 4aba80d5-5f11-4c69-8eda-070bd0008cc5)
    (at 157.62 11.1 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 05581715-d195-441d-ab92-56cbbc5790dc)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 79531c0a-6ba0-426d-bb49-2b6c109b686f)
    )
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1ea522a9-1131-484b-a0c3-c9a96ba626bc))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 41fc2c2a-cf49-4d67-b4a1-da13cfd2817e))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 73f9804a-a89c-4001-b24c-a327cff99dfd))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7fbf14ee-3136-4ac5-83a0-7ba829676fbb))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5920c67-af86-4347-a145-935d7cdc8ba4))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 047e58b4-8ab7-44ef-9544-69abb6109527))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d6cb45e2-c59b-49df-a0a4-0fdcf5885fcb))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f102c9e4-1ee0-452e-9a69-a8e1cacfdff2))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f580ec05-62f4-48ce-81d1-46402af7e1b3))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fa933535-e8cb-48f6-8e47-ea64f175855e))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1caa063a-5a8a-480b-854a-a907452c88c4))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 325e5c68-2c6f-4382-8029-62a3e753ab7a))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 453001a9-2eef-41c9-91cf-eb3bc96a07c7))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 72b30527-f4f0-4e4c-8f0c-4f28dc63b699))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e4da355f-d53e-4ba1-8d01-9396c9720e11))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 56fe990a-099a-490a-83e4-9bafcf4f89ad))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 70a458b2-b2f2-49c3-9683-f214bd8178b7))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 998e240c-2e28-416b-9ff0-be277819231c))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ace1d1f3-69c8-4f33-b867-f3cca242271b))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d3e3183b-120f-4a01-9c58-8a8861dc8400))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3e69612a-0cb5-4209-9b62-1578fc509632))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a8556de-c8b4-45c7-aa94-5e372ad158d1))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 972375bc-b9e2-40ee-b12d-88c7403fb5d4))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 99a3f228-a113-4b3e-b46f-880a584ee720))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp acf2d1fe-4051-4879-b29a-f128a636502a))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 4b89323c-2839-40a7-8d39-794ac73aee05)
    (at 134.76 6.02 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7abbcbd1-39fb-47e8-89ee-eccaa4dc6d4e)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5368d802-c2c7-4153-826b-b7b343fc9400)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 12c36dcd-63e8-48fb-a770-403be74ab230))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 137d473a-0fb2-4c05-80d2-79b8fcbe5fc6))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 73ee5211-b29b-4826-bacd-ecb6ac2e6393))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e2bedc6-2b64-44a6-86c0-80aa15ae7d1d))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ab22c824-1e1d-433b-9ccb-a07fdd399906))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00aaaa25-04c9-4d43-b1e6-739edcb3a06a))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 640ce52e-e41e-41a7-a15b-b09681c06681))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 91b5c652-862d-43e8-b166-53575c0afd31))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d220f84c-fef0-415f-8e12-d866cb11cf8f))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e23cd7bf-9cfb-4dea-ab6c-9db584529ffd))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6683876f-008f-40d5-be47-8a236ae8db6a))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9e7e687b-13cc-456f-a47c-e85bdfeeb9a2))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c1ade0a5-ff0a-44d4-be18-fc488f72b8c4))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d68a0928-101f-482d-afd5-632a127d6728))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fa08e465-e99c-4db5-b00d-e747fa4e7033))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 177ef55e-7ee8-4bd6-b2a4-f3ce2b44cce3))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6226093b-b837-4c51-8e2a-78ab11e32370))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6f8d8129-7297-4a64-b98e-8b3d1c5611ce))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9a148fd4-21ea-4498-8528-7aa15d3d8d5c))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c9f5c615-890f-4ed7-87c5-90306018a695))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5f64094c-30d4-443e-a4a0-a130d5f6a9cc))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9537b5e9-73a1-47c3-96bf-1daebceaf224))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a05c5f8e-acde-4dde-aa98-16bea910d809))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ad8713eb-2a77-4c55-80e0-0df3e9d2008e))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fd229b12-8794-4b36-8739-ddc22a75409c))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 51e6b8ca-6bc0-48fa-9af0-5c89ea0fd67e)
    (at 142.38 74.6 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp be7d0a86-7800-4e42-b836-6ebd27993026)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ba57b7aa-b1ba-4a1d-a278-c76d20f548fe)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0b8d3dd5-cc19-4873-aec0-03087c722dac))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2d1343c9-5a06-4f50-bffe-856846e11c72))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4669fc3c-82c8-4ba5-95a9-d3c9ff17168e))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 48ff51a3-9d7b-40a2-84b5-ba65a92c001a))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7af4f807-36c4-4d21-96a0-4bb7b73b792f))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3a424326-ceb2-4ff9-8c6e-e40447811ecd))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 43da41b3-650c-4d90-a2fd-e102d4ecee25))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6874d308-a9c6-4f2c-965e-037d6300bb41))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7076eaa-ffd9-4f6b-9891-2069971ad51b))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e296ea7d-adeb-4202-a429-6b9aaf810586))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2a3722c6-5b39-4fbe-8393-081de11977f1))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 60414099-1bdd-4e6f-b26f-85770d766778))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6adc99d0-b4c8-45e9-a06a-13310d848864))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74b0cefa-280c-40e2-bf5d-71f3ad9128c4))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp afb8bf2c-d05c-48e3-ab05-c6281051bf52))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 25991afa-572d-4066-a31e-0df96cecc162))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c5c8a5a-1ed1-481a-ab26-9928676de1d8))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4873b01a-e27d-4c32-a7dd-0cc1376cef1b))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c0497c1-0503-453c-923f-a980e242c0f7))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7fa7b146-fb52-484a-bd13-05825761bb06))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 134744ca-477e-43b8-a554-8c325128234a))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 32f8d15b-ac19-430a-ad7d-1876082b369c))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f1f829b-da03-4a36-8009-b8eb0939770f))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9bcfb829-bf28-41b2-8a9f-b35669974453))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af7d81ab-799a-42cf-901a-20ce5bdb9fbb))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 5f7d2ffb-4c77-4425-8ecc-b940f4c16ba4)
    (at 142.38 49.2 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0750e09a-83fb-4bfc-a7a4-8cb74268d693)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 7c9d8f02-ea5c-4c1b-8326-ddd9a32d37f8)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 28dc9094-cdcf-4fff-bbcb-d4e4f5be5e09))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 31680256-3097-4dee-9835-de094d8610ed))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 60aa7770-dcf5-480f-aa05-753789185200))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 80b0f115-865e-4a9d-9587-8e8cad401949))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d99fe5b7-04c2-4bd9-a69b-655ff07f0cab))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 76e11e41-4688-4989-8591-14bcf776d773))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88d57af1-3795-439a-99e6-c7fa8a079e52))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9cf7a961-0b4e-4815-ae84-fbd3509742c3))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ae4a950e-7e4d-44ce-931d-b9bc1a53861b))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4aa1ef8-50ee-4619-9b48-bbddddf3000b))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8344bcf-c236-4f73-949f-6902c1b840b4))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8378ca8-736c-4b0e-9cd7-784a5e69f056))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c67fc824-0987-46ef-946e-79fb11605a87))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d1948385-a5dc-4db5-a104-1ffe19861758))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp df9800f1-d16d-4a1f-ad42-9b8d18fb1f8a))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 04116c2e-0ccc-423e-a984-f1a370253222))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3d7bad12-0055-43de-83f3-1040e118636e))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 637a87c4-46b7-42c5-9c60-00b4b5ccac91))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c59ab8a0-fc22-4ead-8019-cc82a196307d))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ee326ba5-b777-4773-8006-afbfc09a5253))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 34476697-eb76-4fa1-ac18-d84a85824b6b))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d789363-667e-41ad-94c3-82d1ed7c69f2))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74f187d7-47ce-4d20-b6cd-00cbf7db8a8a))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b1711bf4-14e6-400f-9616-f7d481e479db))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be808494-83d2-4814-a8db-17c9aaed0805))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 60cde841-342b-444a-b23b-32f232565aa2)
    (at 139.84 61.9 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp be08231e-9ad9-4847-a141-b0e655cdd969)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp acc47340-56c9-441c-8392-09a2fcd00762)
    )
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 238e368b-de97-437f-bef6-dbe62533ccde))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6e2fb3cd-2870-4c4d-b960-ff6025857f83))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7518d3eb-cf0e-4881-8693-b2fbea3e6470))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b7afb5a3-946b-46f2-957d-678f8709fbc9))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eb847f72-a9d7-4884-9867-f89b7d20f664))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00e27955-89b5-4466-a796-6fb4347d393c))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0a0d6c37-95e7-46ba-8350-b93c02f8200e))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e10f5e3-28b6-4e91-acf8-867a4dcf6cf7))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4cf8c1f9-38d2-4983-89e5-e4d58a7e9358))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b17501a7-9aad-4919-a6b4-b7c3253be405))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0437dbd9-13c0-41fa-95b7-079c7d4a881b))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 21e5cf17-69ca-4656-b941-4dc89a418f40))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 254deb84-346e-4dc2-acd1-a04d114e4f30))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c008b3bf-0788-4bbd-89d4-f767daedf719))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff9b00ab-b8d0-4ba8-a99e-9b147ff0f3a9))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 09d1db34-c3e6-420b-9f4c-24a495696c3d))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b7504df-a6b8-46a8-966e-4111191bccf7))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8bc0e2c5-31ae-4206-8c51-6caa81c73bcb))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b28a5ee4-f8db-4090-a386-a7ce84bae2a6))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f209ff7a-2df1-4d84-add2-0136377c345f))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 24c43507-d302-4c52-bde9-5823600c25b3))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 77610ef0-0e2e-44d4-8067-b8b3b94d6771))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 955c4bdb-92f9-4134-8138-0d6b57a38922))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b3bc5681-c0e8-45eb-ab0c-21e3783c5218))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dd1b35a0-b865-4a63-a23c-3545105da77f))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 63190337-58b3-4a84-a3a8-bc2347f54430)
    (at 165.24 6.02 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0af5633e-914e-4cf4-9b46-e7e5e6aee23f)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2bf63144-4428-4d5b-b520-5c06b9fe030c)
    )
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0041bbe5-8d9e-4720-a915-3cda8c14d0f6))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 20dec056-3de2-49c2-88e7-1533b1500862))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 58a9f57b-fef8-4c57-92fb-03c4a5d08a93))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 61534c71-ba7c-45a1-8faa-72a116bbefd8))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 83e7e1b6-1f92-4461-9cdd-ff08549934df))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5092d3f2-fa8b-4298-8b94-195fa3395e1b))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 510ebdf5-bf25-4585-8d95-97700710b22a))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 54018c96-4712-4f2f-b862-413c910bdd7f))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74c8ef14-f61c-4a11-8b53-41d1d6b87da5))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1e010e9-d425-4d74-86ec-0e62776f1e51))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 528a6ac9-cf1e-4490-80ed-ec7ecdf5c81c))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8bfcb1a0-bc25-4437-96b1-a5cf0e39fcec))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 93b1a902-cbba-4c4b-9fd7-c8b089de54f6))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b3c2169a-2af8-40ed-a5e4-cbf066c8b3eb))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e14381a5-8b1f-43a9-813d-0ad682bdfdaf))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00498169-a4e6-4465-b045-54ecb65a15a4))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5508f734-0b3d-460e-8314-5c986f852a16))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a1deede-034c-4c80-b535-181aeb45a48a))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 80ce4c35-a4e0-4125-b881-26978d20cbbb))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a1faf041-e496-4f57-897c-7facc92807e3))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 322a17e2-e59e-4c32-a348-78b99824d738))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4c9fd52d-8b39-4304-8318-b6302017c2b8))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 993b27ce-88cb-495a-9e69-9fc08d295d14))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a8504bd3-8422-46ff-be21-5bb0842505c4))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aeb1e954-303d-43bb-829d-feb389b1ddc2))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 7043557e-7598-44a7-a919-9601a96d2c7d)
    (at 141.11 33.96 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp daf0436c-8cf1-4dbb-839c-45d5e15f211f)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a8b3223c-31bf-42de-9804-579a2359674d)
    )
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1a0e40c7-6ece-4bbd-ad99-a88cc72e3d83))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5507ee8f-8a53-47f8-84d2-647abd1d58ab))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5e49acb8-8e4f-4679-9bb8-d17f9872269e))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d2f12111-88e4-49c8-b18d-e664b38dfffa))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fd1f0c69-6d77-420a-a19b-ed3c2df19def))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 768ef2a3-264e-4434-a8f3-f1e361eaf4f7))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c1be8ce5-154b-49b1-beb4-aa952aa71fd3))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c4b5a476-3ca8-4948-a42e-85ef02272e74))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e2c31357-c8df-4243-a57f-fb8d1cc827db))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f21db67c-a48c-497f-abca-86d9a72f79b8))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 40ccd436-2093-4593-b1bb-d80a30e74178))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 423d59be-8a7a-4efa-8985-4ddfe52a942a))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5bd0b282-adf3-43c8-85c5-4c261552f95b))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7a0aa5c8-d77a-47a5-a174-92f46e0c1959))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff30710e-d6ed-41b0-ad3f-fbce65fae2ae))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 06596afc-50be-41d5-86d8-ceaecac283f2))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 11bde723-446c-401b-aaea-9c51da9adf78))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 646e9cb1-49b6-492f-8697-34c512cbabef))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 98a605a1-2e05-48ae-87ea-6e0618150571))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ebef2dad-1560-4043-b918-9879b0864c36))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2305a084-b2e8-4acc-8971-77c829e35153))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a68e990-d12c-486d-9679-1f93f04f7d61))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 57556a7f-d5a0-4798-9664-dbde4434b703))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8a8076a6-10dc-46a9-8b5f-39edc2cad994))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f232685-f2fa-4351-920d-10d61b9db4ac))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 7047fdb6-26e7-47a5-aff6-1c8b78e0b1fa)
    (at 129.68 74.6 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 9636584d-1ea6-41df-9550-c2ec62476b02)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fbc2126d-ea67-4617-9c02-1a1dc4266641)
    )
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 234d00b2-058b-4d20-b4dd-2872659bcbe4))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5bc718d6-3270-473d-8067-da5c6c889894))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 904aa6cb-05bb-4cca-a776-087679d3504c))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 978e4347-f9aa-44d6-a5e3-49f1dd3afdd5))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9eb89936-b2ef-41aa-9b81-3edb64565718))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d28ee0b-e173-46a0-96d1-fd55f525f077))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aa3a7973-9344-42e4-8431-a0c91c2a8e3e))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp db66f3c4-6ddf-44fd-9ca4-2aa25eeffeb9))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e04df0e2-2255-455c-8821-0eb3b32039c0))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e6f48620-1fc3-46a5-960b-2230ba8b94de))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0595ad10-62ff-4a13-8356-f57cd4f7b70b))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 06027809-3aa1-4e61-9b2d-5346ac85b9ba))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f2838e2-65c4-4348-ba67-5e0494b9d0ca))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 625da1a9-f061-4074-bd55-75c8dccc0ee7))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3bef28e-fe2d-4270-a728-34cb785da5c8))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 26169330-7567-4c53-b440-c9385b21ce7a))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3ef23e8d-d321-4706-8f82-70a813c724e5))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 46dde0e6-e385-4b7a-8975-3c4562ec1f45))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 59f031de-ed2c-4322-9644-06050b470f9e))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bcc8c781-4aaa-4f19-97dd-dd433ad0e6bc))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 205274df-5a8e-45cb-a474-65f4b5fdf3b5))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3ca2d953-5265-4a96-8a61-a0d01d20b344))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 76b69451-2fd3-45a1-85eb-46b10b7958c4))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 910c62ac-d69f-4b64-a7d9-8ce6e73c0734))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ba44ec49-f925-47d5-a3d5-b0218f75478f))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 7688bfea-08c5-4fef-9e6a-2ffced47ebb7)
    (at 128.41 27.61 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fc6883be-a454-4a80-8837-f5e8594386fd)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 004000e9-5c2a-451d-b6d7-185af73a7ed7)
    )
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0cfbd201-f0a5-4481-9d1d-b827eff99c45))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 20c38eac-c03a-4836-baf3-1c073bd26024))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 43e6f144-d565-40d9-a4a9-e64c7a640f42))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6614115e-0a54-4182-b041-7cf57025a24e))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dc1ca3d0-6b1c-44e5-92cc-398f1a47f532))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f90c338-a79f-4936-990d-78de09202c44))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 16e40144-0370-4651-bffb-df9e8671868d))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1dcde1ce-5951-4511-94ff-b81d5b6493b0))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2b056950-6650-4fff-a85e-e07974e8d587))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 570e00ba-955a-4966-b709-bc18f7a09c4c))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1783b1bd-ec9b-4215-81dc-287b7eaeaf35))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 59a164f5-5de3-49c8-b8bc-6da3adf87fb9))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a73ea76e-24a0-4576-9911-d41ae4463cf1))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bf66b2e7-ff4b-4abc-9b56-92bc2f9a4da9))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c95df7ec-c8a0-4df6-a872-9c8a6f09ba84))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0c558ff0-3660-4123-a974-b3405afa57a3))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1770b1b6-60b6-4362-927c-e30b0cca1e81))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2642632d-1774-4f85-8913-a28eeaee6f1c))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a8c334f8-ea49-4516-af58-3c234fc84840))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d00722a2-ba6f-475a-9d00-6566790c589c))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2563d926-44a0-41cc-8992-ae9dcff2346a))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5ec4334b-5562-4e52-b805-5b1520c6c6f2))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8fdb70a8-3fa9-4efe-8191-b4cf9460447d))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ca7737e4-9aa6-4df0-893a-e20401acacec))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f422e642-b6b7-45f7-9fce-fa1aa26f6f79))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 776d3a13-3695-4a9b-a3db-a26a4b26a2d7)
    (at 125.87 21.26 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 23da28c3-f694-47a4-b796-b23cec25ccf2)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 910b0ed2-7e51-42d9-9e29-4e96a2cd2eef)
    )
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b7c23a8-ffec-4f18-9b3e-ebafa561b38c))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a0789d3-8168-475f-a6ff-22b00040061b))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4b82d31e-300f-41e8-8d6a-7eb231cf4306))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 817a20e8-19ac-4dbf-b496-0c7b1172f326))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ed54bf12-24dc-487d-a913-2d73fc85b249))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3e161c72-6151-461a-a3ec-07e46705c9d8))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4dd82010-cbc6-42e0-b4ac-ec7ba4c21e42))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a0fac2a0-c56f-43e1-bda2-180bab6a3032))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7f81de8-7463-4b7d-a1c5-8b11269b6c94))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b433f3f2-b1b3-44a5-8868-975dd4584529))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 83828fec-eaf7-47e7-a003-76b9e04d4ed1))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b9c0c535-e010-46e0-8416-344e8653dfa6))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c89513e4-53d6-4caa-ab00-1dd5d17e6a58))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e8515522-51d8-44d9-ad1a-4854d9708920))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f64ef777-a948-41e6-9d90-0c0c8e59e17c))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 18629df8-5402-495c-b239-b701d67a2292))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b856dd5-847d-4594-be1a-0ff52b7ce566))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 215cdf86-7465-48a5-83dd-94981188bf3a))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a1eee275-f8a3-4182-b91b-a28aae79a258))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eea28440-3f18-478d-b9f3-b80198ee0035))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1eb2c6fc-7e0d-471c-b6db-a8febc4e8b27))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5705380a-ed20-487a-bab5-7b985370a1e7))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5e744071-da47-469f-a654-b0e9baafe175))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 721b24ae-a62f-4616-a53a-967d7444c89e))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f4bf13c4-7ebd-41b2-9e8d-c1f63c60a01e))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 79593c81-adab-4367-8c3a-68ece6398c0c)
    (at 134.76 61.9 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 542b8ec3-fc9c-4d06-81cc-a41f1511d58f)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8fd5f218-ce39-4c3b-88c2-c87c3dabb34a)
    )
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6b4732bc-3251-4ab9-b81e-f47bf05902e9))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 836ea43f-0593-4f1a-ba7c-9ae90df732e0))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9cd8990a-64cb-401e-8adf-78a3e49a10b0))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e4561cba-cc5c-4148-9136-524677c11f44))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f366515b-2bd4-49dd-9179-3cb2d6a46f4c))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 16e4f733-71f6-4d42-b470-61433f5b62b4))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 17d137bb-62c4-4485-88b2-bccec673e8de))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 36060fd5-8807-44a6-a525-49b234e68465))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4284da71-310a-4496-8319-e0765411d949))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 59032b56-585c-4915-ac95-6a123b424d02))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f2b60ec-485b-4253-a3e5-64883863642c))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1658eefd-0131-4ade-891f-58e4a6114676))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4c03847c-7fc4-4935-803a-9adf059542f0))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 81ac5c91-8723-4955-a19d-7656e492a374))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9831a756-6379-41a0-94b4-3f78a1f82f5f))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 118ead64-210d-47ee-9ec6-a57f4cd9f9ac))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e882ec2-15f3-49be-8bb9-26d7349f368f))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 343abe38-7cde-4f63-a558-5987d1b586ae))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6a4db1fa-ef48-4d81-a4cc-13dc5130623e))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb627a9f-e388-400a-8678-7569caaad215))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19667109-4560-45a5-99ae-7df73a91db15))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 242b68b1-6f56-48d8-84da-177fc837833f))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 43b2bc4f-7d4b-45b7-9838-d9f273d83e64))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e6bbb032-76f9-49fa-a972-8c74a3556548))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f86bc608-d81f-4291-9ba0-23ac9b93e6a1))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 7a7b5593-3094-4c53-9aaa-7500c43361a7)
    (at 134.76 27.61 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 537fcba8-2fdf-4e71-89f3-0d30263c92e1)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ff4166b3-6c3c-431b-b435-cafc65732ada)
    )
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 91cf6df4-20fd-490d-bbff-aced71d5190f))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b1ac6d9d-4b0b-4197-8206-32963b90a7ac))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b701cc6d-4c10-45ae-b3ff-c74261179461))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cd6fcee4-e9f7-40d4-8914-524f2125f7d5))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d2b67af7-ebed-4921-9743-0fbd29743098))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0109489c-dd35-4f37-8ef2-f86a08689800))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 81f9a97b-a007-4155-9fd7-65b517fa17d3))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c45a3a68-2722-492f-b0e0-99e334275ab3))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c5d5f1ae-1d74-4a40-88bf-f63dd262d852))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ce09c563-91ee-4627-b301-bb7413f6de37))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 10f34560-5dc4-4857-aebf-18ec7748a4a6))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1610e8b4-082f-4eff-bb09-04022fa76374))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6126164c-0cfb-40dd-b24a-90eb658d9fcb))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 654affed-6a3d-4074-9a81-e7398d551fa7))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c7ce498c-097f-4f98-8251-a9deb9c16154))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00f65263-433d-4035-8d76-fb90a7769abc))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 638dee69-6f4f-46c5-9634-837aa4c4fb64))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b6e4fc35-c583-4556-abb1-8f5af5d7168d))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c5f13a5c-cce2-43e5-b4bd-9bd2d496e966))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d1d6ea47-2b6a-401a-9927-f087aa592826))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37ced403-4208-4400-a2e9-190363a3e454))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 426fc398-106c-42fa-8bc3-745a9d91f1ba))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 523ae2bb-23d5-40a1-a632-65c7da07e33f))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a637d3af-623d-4f5c-aead-a8da523da6ff))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c231028e-92ac-4318-aafd-3695422af7a9))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp 7b63faf0-5da6-4342-a8aa-0d43a4533e5e)
    (at 128.41 33.96 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2003206f-23cd-45a8-ac15-af1cfd7da331)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 696dc5f2-9815-40fd-8308-95a9b718d051)
    )
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ad8ae88-0bae-49fc-bf14-8c0544200c3e))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a1af487c-6eb2-496d-8f48-597d62dc090d))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c9b90f81-163b-4b60-bda0-14882ca559e0))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cee2f012-7a4a-41a7-a59d-482a74045650))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dae7668e-26ff-45b4-b512-b0619416aea4))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 18f0f862-aee8-4141-9b26-1c31cb73a4a4))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 38a9dde6-8cfa-4844-b95e-8f97b152221d))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 878b2b64-3fca-4527-852f-4be9b78a7585))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aee4c8e8-a6e4-49a4-9833-0fa8dca71767))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b4e1c4fe-3e0e-4f7b-a590-804ceb944aa5))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37ba84c0-5418-45d0-bc56-5278b3def7f3))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7080180e-f2a6-4fe8-b45a-3c2a8a42d55e))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b0753141-a162-446d-8623-2c37aa26809e))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f7d0b437-b52e-4c33-8775-2bce281b157b))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fdc708d4-1158-4f43-956c-c57c9ed0db31))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2848a98f-f974-4422-8df4-3157ae8facc5))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 45fb33d3-3d55-41e2-a0ca-250856bd9930))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d709dbc-e670-4503-aa9f-5524fb67ab7d))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b951b232-b7c2-4ea7-ac88-c20587e65734))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bc2deac6-8f53-41f8-8e42-9913174d6d4a))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 015fa466-7637-4897-8e92-473cdd0f1e54))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e917b98-f907-42fd-9f06-6555b0029e19))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 15675035-c9b4-4669-9614-dd276c259352))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2f10d7b1-85ea-4253-a700-8637095f7c95))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 339c0113-1c8c-4cef-b1a2-2b4e5f1b30c7))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 7c00715d-eabc-4a26-ade6-8f7680057f7c)
    (at 144.92 74.6 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3816b9bf-6e0b-4533-a94c-08a2d2b0d28e)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 8dd51cdc-feeb-4979-b0f8-2c74ac555d33)
    )
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 04ea03ed-ff90-47d6-ad9c-56b3f20cfa99))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 43904461-a9c6-440c-87f7-14e278f6c7ab))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8dc1fe23-506b-4437-af9a-89471673847c))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 954d6662-88d6-42d6-aa08-1ac0b697ba66))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b45bf167-56f4-4879-bd6f-2ad2e928cd27))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0408452e-07f9-4013-87b1-f9373d3d61b1))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 43a42c0b-eb22-4920-b81c-34b5749a2452))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f9cd3f3-54a7-43ee-8a49-bf78669c74d9))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4a874a6-325f-4198-9594-6ce7f1bc9c51))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d643d428-c4f2-43bd-8cef-a49182301b15))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 077b57dc-e2dd-48e2-b41c-f723a10ab20f))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 207ef2d5-141f-4b29-b551-fca2d963b0ec))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b88f6a01-f629-451e-99e8-71825b770c04))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d1775999-19a1-40a5-8748-5c99b7f0bf11))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ea19304e-ec35-463c-9277-bff026719c8b))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 527e9232-a7bd-47e7-b774-c65feea06697))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7da5f90e-110b-4b6a-a648-b3aab117ac7b))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8001b6e6-1c2d-4d98-b94e-e4e809004bc4))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a2c3e21e-7fcc-4be6-ba69-ea985a546d6b))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f948fb59-c91a-4efd-a9f2-cbe82b174233))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 477fb14b-8de8-468e-a708-28a67cefb6e2))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8bdf0337-f1a0-4f98-9846-922ab490cd76))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ca80d30b-e11b-474f-8af0-2dd3a6a517c2))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp de084e19-b9c9-47f0-a1e5-deeb7f9fa838))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec53a338-f22c-4756-b0d7-1e69de419338))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 943d45b2-ee35-4351-9504-14d7aabead8f)
    (at 170.32 74.6 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 905f8c13-bb80-4eea-8ca3-67e021384bd0)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a1d8d410-668d-49e6-826f-a9d088930d7e)
    )
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 05c4b04a-f8d1-42e2-99fd-50006c7d7d72))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 17136974-e6df-4c01-bb61-b13dbde96867))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1c2fbb7f-f40a-4f5a-b82e-2437b354d969))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b6911ab6-c409-464a-9e8d-c099335a51d2))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp face6aa3-f307-4659-b1e1-750214ee2b6a))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3e2dbe46-4cd0-407b-b8e2-932826026d3b))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 765c2bbb-61cc-4a9f-b93a-a30106d85e1f))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 893e6dd8-3834-4616-acb5-179fb71c89cb))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8d05f3c9-0740-4c9d-92bb-85167fb238a1))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e32cb43d-6a36-4891-ab62-a0622d7db862))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19c38216-26c2-47a4-b36f-d191eaddacd9))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 35020c3b-d399-4825-8385-06c862244feb))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52cf302f-31d4-4603-a6ee-d93ec62b767f))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 578b7203-6fb6-48f5-a85a-8a819962dc7a))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6bd2ae91-279a-4f64-af21-375ccd97c351))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8dd62e08-98e0-4e28-921e-a911333fd9ff))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c28a7b35-f0c0-43d2-bc9d-5ac2d1b4d804))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dcb59560-d6f8-4beb-b714-86abd79e7fb3))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f11eb32e-8a31-4a76-b21a-a0a818abf689))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fb2f625b-af6c-4e09-be38-81cdc8a18de6))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 053bedcd-40f4-4bff-95ee-079d04b0a422))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0e697ded-8990-4111-bca1-467ae9b53ece))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c0bbd366-3ec1-4757-bcb6-e945bddcd962))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c1dd2e72-f08a-44cf-8483-985072826851))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d92cc91a-548d-486e-b4a4-22a983cff7ac))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp 9e40c88b-cb37-4cda-b94e-04da594d6585)
    (at 147.46 0.94 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3c59e593-df7b-4a19-b5dd-a57d237334ba)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 132baca7-8b38-46c0-8173-3c9d6a359e78)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 21aed428-9849-4c6b-b349-031447d50bff))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3f2f3271-ac84-415d-8237-d236a7cbe9ee))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6a1be057-d01e-4406-9033-1b3809261498))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c133e6a-d652-4e56-8073-155044b3c06e))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d9f261f4-1b57-4ae9-adb2-c1451a6be0fa))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4715472f-6141-452b-bf0e-69161574df86))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 67f2a4ee-66a0-4c3e-b0a1-20be4fa95324))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 799fdde0-c0da-4da6-8797-045ce41178ed))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c3ce618c-478d-4792-bcb6-e9ba467de0de))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec3b73c7-91a4-4034-aeeb-43541ef626b8))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2ed151c7-7d36-40a1-bb1f-2e5bb422fe4b))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6218fb58-f39e-4ce7-8262-faf4203ca764))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6a65e25f-ff1c-44c8-b7ce-398efc9210fa))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9ba921e4-e756-40b1-8ec0-443edd782cf9))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9babdc74-9687-4e35-a85a-ffd914250af1))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 400c8d1d-0162-4edd-852c-954a5455e2f5))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8538b13f-aff4-419f-97bb-7ba3e5a88870))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b5db3072-203f-4f00-8715-d214b7235142))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c39f219d-e8cd-484e-af92-4201ced158aa))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp feec8fe6-d5a0-47c6-a11c-3ed02d642ec9))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c6eca27-b14c-40c0-b684-8beba87b0e9a))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3d0a1719-cbb5-44e4-8040-ab048e283ce6))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7935af96-5759-4a31-997a-a31c6fe1b5b6))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8d700b8d-4086-4d8e-9e82-573dc906c694))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ec556ad-964d-439b-808c-6ea80fcb28ac))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp a930bd81-44cb-4c1f-a50e-5c3703a2ae67)
    (at 152.54 84.76 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp cd669666-be9a-43eb-bc4e-8f07e45419dd)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5add489a-43f9-4f28-bef6-78e918b6663c)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 23b9c849-a63a-4c5a-8027-d8e2d5576852))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 710287c9-a2a9-4c50-9845-8fe5aa43ec19))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8a55432c-1fcc-4845-9436-c7fc8d7b1d14))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 98dde6f8-83d9-4278-a226-688b7cfd5b3f))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a8454bc4-65bd-4c24-8cbb-6b68dbe3d7d8))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9ee4abc7-51c9-4752-9500-fe149e79d790))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b0f74d3e-059e-4d1f-b057-58e1ccb93330))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cfdc7c1d-5c87-4d2e-8ea2-f023c3de21d8))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp def18a9b-dcc6-498a-8f45-533b97cb159f))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff795e1a-122e-4560-9400-80ce0ee0f79a))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f818839-8098-4ee3-a589-e0ed84c07713))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 67069a2b-dc3c-42f7-a392-3ff692f9fadc))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6bdc988e-7148-4c10-9375-23f83664dd98))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8fdd2a0b-04c8-485b-837d-2700e84d011a))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a50cbecc-3d52-477a-95c6-3ec4fb284aee))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 109c4a2b-69b5-40cf-ac37-885d0dd4424f))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f653c88-cc56-46cb-af78-870fe081df44))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8cd97e05-38e5-4827-b584-f54c7f8e5aec))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96202b4b-6e98-4736-8feb-f17722377c1e))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c3bee16e-9fd2-4fb1-bb71-7ec25032152e))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4baf4da0-da80-456f-8311-71bf2fbb538d))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5194cb2f-72cf-4a3f-9007-30d9da2b4ff5))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 694c7553-a311-405c-a65c-44eead6e77fc))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e9e35857-4490-444c-8b8b-ebcbff65e73c))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ee181e9f-025e-4c14-8658-e441400b43b7))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp abffddb8-6c79-4840-8662-62159e82761b)
    (at 170.32 49.2 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bf948ebc-824d-49d8-bfc5-6ba99829a6fc)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f4f40a4d-d58e-4a47-a46f-ed1f5aa1b65f)
    )
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 02566d18-9572-47fe-9b59-61e6048bf4e4))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0efad704-d9ae-499a-af8c-9b79b2ca2288))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 541cb9a7-eddf-4775-80b8-d7b3dd44e59a))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9bd4307b-9611-4f4d-b8e1-5d24c530b86a))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc332149-0b97-404a-8061-1ac6cd536c7d))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0b0b577c-9c2b-4b61-8427-e10a87825804))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 610f5b34-3921-4f37-9f17-c01b40d56852))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 69168663-21ac-4d0b-8070-8cc35eff829d))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6db8c33a-23d4-46f1-b52b-77ba01e6d454))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7db26895-7b9d-4892-8dfd-027ec506a663))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 22b60264-aecd-4102-8c2c-e8fac6f286f6))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3b907d49-c46b-4c3e-a764-aca19a3d960c))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a41d0f9-9494-4548-93c6-9777e98ff98f))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6595a2a2-1e13-4c11-b4ec-af7c47451c8e))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b95bfb65-3ec7-4ade-991f-d807def1d78d))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 44e79e39-6f0e-4aa1-a469-3776774ca62e))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 84f430e5-5fcb-4cfd-bb4d-0cb5ce480b0d))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 929e43ca-8cb0-44fc-a893-2f5e5c58d36d))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp db52bb69-b41c-4e5c-995e-751383c48a8f))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dcd30f1c-d5ab-4bc5-b11b-2dfcc24fb929))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 238627fe-2e02-4ad2-a5e8-7d43b09f0621))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8857c551-8fd6-432c-b3c0-c00cd0230b6a))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af4276fa-1bf9-4632-9f45-89630c42c0b7))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d3826d7d-1e62-47cb-b5b8-48e804a18e88))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dc717815-b88a-4959-b530-6368133a81be))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp aea4e92a-1ec5-4dec-abf6-2f1cc2c75176)
    (at 157.62 49.2 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0dbb7461-2243-45dc-a6e5-3bf442632102)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp eb70076b-1600-4157-a646-02c4c060fc01)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37ae357e-4b4b-45e0-8556-f18c52755bab))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6748458d-ddc3-42e0-bad9-c7300d2101b7))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c0d4666-77cd-4799-8d1f-62eb3eab49df))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a87cabbf-aed8-41c6-8806-2681f04f38e3))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d0e1d585-421a-4a5e-bf5c-628638757ab7))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0fa8a586-e8b2-4856-98c5-9a34cc57f88a))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 92fdcb2c-7f0c-41d1-a66e-c53be7db436c))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9b92b3a6-6e08-4dee-a098-1f4d8ba36417))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d3e66daf-5fa9-4043-bc82-2a55a0ab6dec))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d7e8dcb5-b077-4923-bd41-b07787d1ab93))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3ae4efd7-7d98-46f3-b129-6024f6bee026))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4b388837-de67-44ed-bf05-f0f644dd27fc))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 58001672-edc6-4d41-b862-2d15545b3307))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9568a680-b6e3-47ff-aeb8-d673e0813ed3))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f4541b5d-fd94-42d5-bfdc-84360a850cb5))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 107fbcc2-7f5a-45eb-9f9d-978e9c441d35))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 13252453-85b7-4b35-a096-9ed88597d1f0))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d4e2dba-2e39-45b6-b360-79b397ea72f4))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 651ad084-d16a-4b04-a51e-0c75f1adfa36))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c723a607-be44-441b-808a-37258f424a1a))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 041d65a9-6dbd-4a42-b6a3-859221a7a58e))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f4d3256-ea53-49ad-8cc3-2d91a517c222))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88265092-a102-411c-a4c3-754e9f5aea80))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9b968d0e-8acd-4c5a-8e04-b7450ac10305))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp edd03ba4-50f4-47a3-a02d-c58d6a1a3747))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp b0359dd5-f456-4378-8d2f-1efba396a076)
    (at 141.11 21.26 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ced3dcde-86d8-422e-8577-842d839aa008)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3e5d4ad1-7fb6-4891-9fde-c5c6c39c2252)
    )
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 00259b70-ebb4-4fea-9bdd-cb2bff07d315))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0592f041-3e8f-4af8-8100-f2ef72dd018b))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4667d70d-7a95-4d74-8729-949cbb0e85ed))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 46be4b8e-e690-4d7a-beab-2644c7265672))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af987bf9-ba7f-4d69-8662-59d73b7df041))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 086d5653-94b4-4565-84a0-bc2fa9d9a6f3))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 41b1996f-1629-4a79-83a5-488ad70b3335))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 44c394c3-3c06-44af-8b20-34ad93a4f834))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a202b724-05ba-4eb0-97e8-2cfb71b6c66b))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b10592bb-6102-4d40-8261-1435f3b7d06c))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 563fb52a-f21c-49b4-bba7-4cc0d31bd117))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 741f083c-9c45-4ec6-8646-ca1cc46813d9))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 865ce2c3-cc76-4366-b9d3-8f58c1aabfa1))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f27d041-49e5-4b58-9728-22580d914a86))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d354acd0-9f7a-4e58-8e6f-4f9319b6cbcf))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4fa89a57-98ca-4466-8225-d6feccddb1d5))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 63c5f3ca-932d-4153-bb07-c9e881e3e3c3))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 64872417-b9e0-4144-8d27-2ec0440215ae))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d84a9a95-8fc7-4fd3-bcf4-518ac442fd33))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ef904945-5216-4883-b30c-40e7c7c604df))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 51198c67-3da5-4d17-a7df-a00fc75fe3f5))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7360af88-7e31-433b-84c0-826f5b715c74))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8850facc-5264-4b70-ad16-3e53822b46de))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bc58cf16-95ec-4646-a2b8-cd596607f43c))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c721ce49-adbd-4904-a004-8d584bddc338))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp b0fc9217-b94d-4dcc-b577-7a6450352d8c)
    (at 125.87 33.96 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 680a79a8-77b3-4699-bcdd-7e9dc475c3ab)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 581698c0-dfac-410f-89ea-873d2c5cb5b8)
    )
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 097739b2-852a-434b-b90d-0d6d89063956))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 305be60b-ccac-49be-a7c4-ba60ccd7c982))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52a71bd7-08e8-456b-a300-af12d05801d5))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a389df5-5f6a-49eb-b8d3-c63507477686))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dbc8460f-21ee-4dfc-b6ee-e1a437ff10e2))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4e99020e-1a69-4fd9-a160-34de031bc69e))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aa60d880-bd75-4618-a722-d1ef86961e2a))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ccc429d8-4e83-4198-9dd0-3cfb0a94efb0))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d045f862-d33b-4f31-b996-1464714abcb3))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dbad8ba9-793b-42e1-ab02-aa69c12a8656))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 14588f2e-611b-48ec-87a6-7f6c6a12db16))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8fa1de0c-d5c5-46ae-81be-db515c99cc66))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb181fff-2b5c-4db4-90cf-759b1cf3f06a))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f7fdd944-0777-45f0-8bc6-81f99f79896f))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fa3643fd-c32f-464f-a67a-64a72b95aa0c))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 845721d4-dbf1-4723-9f51-18a395826086))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e706873-78fe-426e-8214-6ad0a463cc56))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a947e097-be16-4320-af85-3e5f1a20d36a))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e4de5386-285b-4c47-9042-a07967633f09))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e61241ee-db5e-46ff-ba8f-e78e4317a0c2))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1785823f-0563-401e-b20f-8348e2de97a8))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47a4404e-0dd9-49b1-864f-4b5f37e1cc46))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52d1050b-b431-4efd-9d84-e94d75372821))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 889e5b2a-f53b-440a-a184-f3bfab9630dc))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp db5f2cad-e0ec-4729-af3f-ad5e18f53cf6))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp c294976b-f8e1-4f93-a6f6-372c4a0f9b24)
    (at 147.46 27.61 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0b42025b-b1c5-4bca-9f0c-9887ee305ae8)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp dd4b4267-6aee-40df-90a5-7237f4517e1c)
    )
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 11a78da4-e8be-4f69-8e2c-3e48f9abeb7b))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3cf38ced-2f31-481a-83aa-32c8ccefc053))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4422f7d6-d736-4b56-9f7e-8592b23e8a07))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7bcc2476-7cfb-43cd-a552-d7f72e371475))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e92c692d-3519-4926-8406-c167438ddf01))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 047add90-5da4-40bc-a586-c24c7f584f84))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 26f4c143-6e36-4831-bce0-c2e0242eaa06))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3fbc2ae9-2bd6-4d51-a5bd-439b644f83f0))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 893ecfc3-a038-402a-b68d-1def2be2eec0))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ef63bdaa-c001-44c6-be52-0c917020bc90))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3581fb4a-c594-4d3e-855b-69c19e270f48))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4dd46a74-8858-47f6-a30a-bf7d5d340821))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88065696-ad0c-497e-b9da-52c9c6d243fd))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ab24eb0b-dd7c-421e-b093-0c349b87fb0c))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f6356cbc-5375-4b2b-9ee8-375c1a532fc3))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 066ac64f-09a8-4388-bb75-7d57d0c83251))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2f70df47-7620-4096-a4eb-41d097dc2501))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a972a606-6b60-4976-b21c-ff7d69ee778c))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b3f18077-7e2e-47ef-99ee-1e2366a1bdcd))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f24aa777-f971-4858-a784-e253f50fdd9b))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6b797633-9005-41b3-b02b-b6eccef6ff62))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6f1070ad-4751-4bd5-8786-84eb301a3fb7))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 76b7b7f8-cd8c-4711-ad1a-ffb18777a8ea))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a85f5a16-2645-4452-bd22-abf82201d341))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bb3a6813-2965-4402-a8aa-a877daa1299d))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp c4511854-12e7-4ab9-b233-13a01fb93af9)
    (at 134.76 33.96 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5c8d7774-04ac-4648-8f4a-f161cda8d1a7)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 00fda4dc-3506-454e-bbe8-818e9e4123a8)
    )
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 267a5ea3-60d0-47b3-a489-69b385493e36))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 28b373f8-3051-4a57-97af-bf515a7f5e15))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 66508fdd-2818-41fb-a0a9-11d1e12aa3f2))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c04d3a36-5648-4f0c-b695-f93b05fd6782))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fd55be14-5ae6-4399-94f0-9dc565a3a2c3))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 331aac49-9886-43e5-b0b9-b48cb55fdef6))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7f3a5964-4c11-4d7a-a527-9b6c20977e91))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 92cf45c1-aede-45be-9add-e9592b47f742))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be4691e7-1f51-4d8e-a72b-19191db300d9))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c409038c-45bf-4d56-bf53-a5e682628740))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3fb3df13-df6c-4bba-9320-8c2161c826de))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 63fc8a9e-f49c-4252-848d-eeac0a86f0eb))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ae53c27f-9c04-4ac6-a554-b135fb2c14b1))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d7d339a1-843c-43cd-ba26-45dd7fc12a2f))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dddacfe4-67e1-4875-976b-77df665163da))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1af342f5-f2fa-4c92-85c8-2a4ac22a5c52))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b2876385-0070-497d-84db-df42ea9ee4a5))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ba811148-7978-48c0-a521-b27a3f453722))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bd38fffe-078f-4efa-9075-c81412dbdebe))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cfd69910-5760-4286-8130-aae0e8b02a95))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 05c7b21e-2cc3-4ce1-86bb-0b415e337c68))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 30ad0354-d074-47f7-877f-1cc2aaeed19b))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4da68107-33f0-4b7c-81da-d050626b7ef0))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 51d8d95d-1641-4f7f-98a5-aa019fb7face))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cb41d63f-990d-4f58-956b-10983c3b8f33))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp c7234249-7d2d-4798-a76f-0a8513cd028f)
    (at 147.46 39.04 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 24237231-a2db-4161-a2c3-16d335690365)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp df620c5c-caa5-45bc-a81f-23fe18bbf01d)
    )
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 06cdf0cc-b33b-458d-8c06-4b73c4f37e6f))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 101b403f-7723-4f4d-ba16-78d00b507ba2))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a937ef3-fa19-46c4-a5cc-db174937c9f6))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 69a761cf-6c3b-4a91-bf8e-132ae7796577))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b04b7b39-6d5a-4df8-867c-d80b2ad99bee))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5c65b376-37c3-415f-9fb1-d47b0bf99411))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 743a72a9-cf1d-479b-9a49-48ffcf6cba69))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d8f620c-f1bc-4ce1-aa4a-f1263a83b86d))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d53593fa-9b22-4651-8efe-471a17e12d9b))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fbc28f3b-6458-4859-b99a-d3951a698402))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 049896ea-0961-4121-b54d-bcbb5dbc8254))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6d6d61cd-1618-4a52-9d92-728359dd7c5f))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 84611b93-8559-4181-9b67-90abd38acd26))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a75013c6-88ac-4abb-861a-860488cbcd96))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aaba136d-6cb9-4840-87ad-af5f25887e5b))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 64860687-1ec0-405d-9c38-04feef962af8))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 86c435e9-b421-43f1-a48f-7573fdb11166))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cd47b96d-9541-4638-a77d-903384ec0a9c))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d475f9b1-4834-4ec4-a41c-cc280640adf1))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff358270-4716-4736-94be-fd9a45812175))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6066a79d-e98c-43f2-9cae-306350b4e848))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 692bfe96-bc3f-41d4-b285-c58c42415e0b))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9f1aecad-e4eb-4c90-9bcd-97f3fe3a479c))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b01abc17-12a1-4faa-8007-aea72cd1d69b))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cf2c6e44-9e70-4114-88d3-6bdcad511b88))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp c8f1a5f5-56d9-475b-8e1f-961b4c66112f)
    (at 139.84 6.02 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a7e0a930-090e-4448-a9d9-79ffeb15c917)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 53ee8919-b158-4be8-a794-bea91dfb9330)
    )
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 023f46c4-f97c-4c24-8eb6-ddcfb907d0cd))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 25110eaa-63b3-460a-a7a8-9729fe2cd869))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 56998b29-5279-4729-935b-7044cdc4bb0a))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 57cb7aaa-f904-489f-8c4e-f3ba25df3e00))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6860965c-458e-492c-93cc-438cd50db543))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3b228649-a1f7-487c-a41e-c757bf254e27))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4268b77f-63c9-4865-a501-0d77af487054))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6ef3c655-af31-45ea-a5ab-57965bd7e333))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 983d60e2-6bb3-40ff-8f9d-48b903277fe3))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5c4b065-ed80-40f4-9e9c-816e9a516578))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 17d01af4-07b0-4ab6-bfed-5a9b1963b772))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7a7b9668-c3b3-4d1d-892b-21d85d181d33))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ccb06ea-a208-4859-a8a9-cc6fa3e9e4c9))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96f4348f-7844-48ae-9dc0-51ea414e6dd1))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bca66fde-1625-4779-abbb-cf1c78e22e60))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5b51a90c-5b78-4a54-b940-ede3e2013e16))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ab907e6d-9a70-4d61-9b39-f27cf8fb4873))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b9a81643-0fc6-4851-98ba-2a0bee519611))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c2c59427-51e8-4191-a4bc-736e5d8e3396))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e4bae193-d4fb-43d6-a89e-32ce4e644c6e))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19611a07-ea55-4361-bc58-d86a78ed35ad))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3da78191-2d9a-49fb-9a03-c4f62179b105))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3ffeaf3b-e9eb-4872-aee1-57b808f8f134))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a07841eb-f4fc-41c0-896d-3265de92ec72))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp af115c16-1737-4c2a-8112-72bb5462ed64))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp cc086c59-1380-4f62-bbb4-40ac94aa1f2c)
    (at 165.24 61.9 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp ecec39be-6e6d-4d6b-acbd-5d14c6e9553b)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 4d7bab7c-5f23-4efe-91a5-cd386ca0c714)
    )
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a9a5394-ce04-466f-80c0-381002fea3e4))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4eacac80-f07d-4dd0-ad53-41d83e8159e0))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5a3f1132-0a0e-444b-a578-edcf7c0c0d5f))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 99847bbb-0e83-4293-8625-5c21cbf0dcbb))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c09af807-88b9-4c34-9126-ce28727cc98e))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 428180b0-037f-4898-b478-1cae2c8dd48a))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 76d5b5d9-8c3a-4d61-840e-8c5d090d584e))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ba75f63-9d46-4b09-961f-7e5440b9edd3))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7cefbe5f-9b41-41f7-9656-736c7db73529))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 94f20dbe-c777-4afb-8b96-9b3a6f101a33))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c06fa04-816e-42c5-bec6-1c1eb6d882ab))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 43ab9ce4-1957-405e-903a-b359f16f1802))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a70a098a-ff66-4d8e-864f-f2175c7747be))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ce9dd6f5-d118-4afe-8bea-0a846bfcc8a4))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc6edf63-c598-40f8-9df7-8ffd1a71b965))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3b75f333-2079-41c1-bf38-0e881d5d419e))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 63887106-904f-4ab7-b097-36b703c303a4))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b56cb554-bfc3-43e6-9a32-eaec36e8132b))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dac508d9-a887-4b8c-8be7-089115df8fed))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e6178c37-fef2-4425-ba1a-5265865144f0))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ab91e8f-b5bb-4643-9677-70a806e88adc))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a5facb17-03db-4747-a3ce-ff112b11ad28))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d6d97d14-b5b7-4ecc-8002-aca5503f4946))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3e6bc91-5f18-48e3-8eec-2c3f0edccfef))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f2736d71-6458-4810-a5ca-d020fbf326e8))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp cd124e77-1ed1-4ebc-896d-3cde1aaf9530)
    (at 134.76 39.04 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c0e8c73d-c5bb-4e69-a0c3-a9b7806bb3b1)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp b2f71ff3-85da-4509-8a58-9de72d6aa76f)
    )
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 05f91830-abd8-470d-bed4-e225d70cba91))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0db3634a-ad3d-4060-91b2-f6d94d6b7674))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0fb74fb6-0c7e-48fe-9610-b1945aff0dab))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4a0c0dc0-5c37-4d59-ac4a-b3439857cca5))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b75453e4-ea4d-449f-8c8c-f757c622799a))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 439e196a-9db9-4c48-9386-6ba291245982))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47807e67-b013-4608-b5e2-5c568b5bcb03))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 572cf80f-901d-42b4-a0b6-4875dc64e456))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5ab5a3b6-95d6-41de-b98d-de9bb015b5b7))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d52658e7-b5e4-4a11-a05c-1df80a03971e))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ca83ecd-c745-491a-b371-7d7817356557))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9b9dde40-c9b8-4b2e-9b81-85d88a8eeaa3))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a3e95178-f7c3-449c-b05f-3b40b5bab6e2))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ad9ba3a4-f48c-4339-84a1-aa5899fedfe3))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fc957a5e-90b9-49f8-bb3c-705fc6e61648))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 120b128d-36dd-451e-9502-7d758ec5a4e8))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 34df49af-7594-4758-83c8-612340c04f98))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b6d28679-b7f5-414b-bb06-66f9cc44d637))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cbca3b00-731c-4623-8c1c-b21ab9b7fd27))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d62051f1-c2a1-497e-8f10-837e3d1c10cf))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 51cf9546-ae1d-4c14-85fc-7ca61891202c))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6ca29988-b94d-4335-8ff5-763a8463be64))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 73e1be02-ad25-4eed-9121-fba2f489a8bc))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a7ba8a3a-2b21-4351-b0c5-26b9d93ea034))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp daeb6d18-7951-4a9a-9b80-b9ce5519e9cb))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp d314280d-0381-499d-a8b2-8a82744f6e5e)
    (at 170.32 23.8 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp c179046d-44a2-4712-944d-8f8a5082904d)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 5f64699f-068e-49a4-ae1e-a8a02d66a109)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 26a57c26-3eae-4560-8c2b-beb1a4c7879c))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5c2d6e97-4023-4acb-934b-1ced94f8359a))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 77fa8f2c-a197-48e1-9c50-85839698a29f))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8ce6ce0f-acd3-4589-aabd-bd69cc1078f2))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b40937ed-0100-4261-b4eb-09516017e5fb))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1b3035dc-d833-4658-aa97-f70b485e412e))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 60d336a9-c6ab-4f47-aeb1-afd4e28f2ab5))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b4a8dec8-b513-442c-8578-08e94055c962))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c28c24f5-4274-4ee1-be5a-8a1e7e338454))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f7f1cc22-2c60-40fb-9bd4-ef6472069a8d))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 058d1e1e-2fef-4793-99c5-9f14b4dd6e76))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 270dbaa0-2773-4029-9927-1bd86d1d01ae))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e780abf-6e69-4417-8949-a31abf035d03))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 903ee6ea-011d-453a-a2a6-c821929dd874))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 92f5e081-7464-475e-88de-85d170edfdae))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 178c6fe7-1d4e-46dd-adaf-a08356b705c8))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2048597c-6981-465d-a82e-b56c5bd34447))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 296f7954-5d54-462d-8c1b-41ce1aa22b7f))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 947da361-1ac1-46ae-86ef-2e33469c1497))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 97724b0e-8815-4c94-b0ce-6db96821d69a))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3d70693f-8f69-4113-950e-875aff1975d7))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 42efa47c-6506-4d33-a2a8-7df022e30270))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7c841d9c-e54f-445a-a50a-8b3cedcc7f8c))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 807ae988-3d4c-4b86-939a-049985d35cd2))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a13f1ee2-bea0-4d80-8ff7-c0c87cbd013d))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp d4f9df8c-1926-4d30-bf92-e8c49533edc4)
    (at 147.46 21.26 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 51ad0692-8edf-49ac-b426-3b984b505d60)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp a3a1e0b3-fd9f-4b93-bc21-9f7fb7ac300c)
    )
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 331b7daf-4ee0-4a2f-b281-36cdba54c55e))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 33e91c09-0515-4750-85a8-51e2d4939278))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 47eb83f3-d851-4b14-b8df-a49b6d9dbe90))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e459c3e-784e-4312-84f3-d2d2f8d1eed3))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c346ba3e-083e-4130-bd03-650b597ea971))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 473cf36d-adae-42d0-9b3c-34ea03f16946))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5caae0b4-f987-4acb-b9bb-2c5556027adf))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 89469805-996e-4086-8627-7c4a3e1034a6))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9823183d-c12b-4bc3-ae3d-8641dfb41bfe))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e71ba148-9a5e-4358-8852-ce770976fe03))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3f7eae45-20e9-48e1-a9bf-6360efe80730))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4469b5f9-59c7-45fd-9403-2c3ff7948c5f))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d3caf8e-e1e8-4b2c-b04d-51ac4c9b9de1))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d4977df-9254-429c-8153-753ca01d05f5))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c6df7f5c-33db-432a-9e38-a43a99c217aa))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2bfc2139-4188-494f-9854-029af0c89d95))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2cd67c8b-a593-4b41-853a-5e31e6e404cb))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3682c5fb-6246-4680-b70a-fb5292ec3dd5))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9e5153fe-8c1c-431b-8250-d8b4414e67e5))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aae59f76-545e-46fc-88de-6231175ebe2d))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ad07ecde-be28-4af9-9963-f2db393d5c19))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b90b87d1-d68f-4527-ab25-bb6fef35c188))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bc42aa61-3ccf-4034-b375-ddee0f5fad90))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec209ec2-950b-4804-90d1-9120e92128d1))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fd5eddd9-4947-4324-ad88-34c37e8d8e4a))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp d609237a-4363-41d4-89cb-54e46307f344)
    (at 170.32 11.1 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0a4d1455-8220-4c9a-8a2a-3c3bfa9be1b8)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f5633bc1-c4a9-4865-b8e0-0a8f49480aec)
    )
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 17b6a1f5-fbdd-45b1-ac6c-957bd010d837))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3611459f-63c2-48bd-b580-d6342ba10158))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3dd8def2-6a47-43c3-9524-4ae3fc3a9700))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8302c7c3-7055-4a23-9801-951d4ffe48aa))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be4b8f13-7923-4306-80ea-c4817c1461e7))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9522424e-0897-4327-b6fd-28e49d3fffab))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d5c8f689-facf-4bcb-b81d-7aa68f2a5dc6))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dc3effcd-8fb0-4e93-8fed-87ddc30e14c8))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f024ac8f-7002-4b19-977a-a78ed8e44f96))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fb444767-2640-4518-b624-967e8d92dbc6))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f867b92-1829-416b-8355-1c3798e4dc44))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3a13eb5c-fb22-4f0d-a77c-cc65b3383d2e))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7047643a-df9d-4d40-b340-ca2f1d5e3e13))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cdc741f8-1a80-467b-bba0-cf87fdf26e15))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f43ed5e1-ed07-40dd-9f18-97004b32dcf2))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e08eb26-1188-4599-92c2-ea93e0bcdcf5))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4ce9b46a-7604-46ad-b020-d9b276e5aad3))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 87741323-d514-49ce-af39-3a0583a53cb7))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d428e622-d6c5-465d-9446-12f96315f0c7))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e534af6b-af7b-4398-b699-9e1f289d16a9))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37558250-7cac-40ed-84a6-346f548d2c83))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37c26b6c-e5a0-4ed1-9de5-743d3c67ef52))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp efa41f96-9aa6-4244-b36b-cc420219f13d))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp effc6438-051e-4bc1-ba04-bf7296a1d8df))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f9349609-2b8b-4c31-9150-ef874536850d))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp d91058f1-501a-43b6-b9c5-1f4b8beb16a0)
    (at 129.68 11.1 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 0af49468-96b3-4bbb-9219-3bfadfcd4580)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2b5db90d-b869-4dca-bec7-28ea2b5ff567)
    )
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1db3a568-b051-4192-a24b-d2119c82922f))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4d8ceabe-ca0f-421b-828e-e713c026d94b))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 66723d83-f242-4155-87aa-1b433d1d91c4))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 90dd2e9f-0718-4438-a9c9-1c5c177fa3b9))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e7ec4fe5-0628-41b4-a95f-c54680e59f04))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 31e985ec-e6b6-4d0f-9445-0e89a88fe29c))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8be05d39-378e-4834-9237-547a5ceff3c1))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8dfbdc73-338f-4fc5-bdba-d3e75e7045b5))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aad7d2bf-f594-416c-8666-5afed641149e))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c8837f8e-5834-4a8e-be4c-b0e2a7d66956))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 10f232b2-7a16-427d-992e-db3791402aed))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2446f74c-6a99-465a-9938-8b805877e1ab))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 908562b8-3b76-41f8-adc4-a74d3bbb9145))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 92950445-70a4-4379-a6fe-10d9335e9469))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f9e100d6-1239-471e-89e3-3e1465eeacff))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1c2e11d1-2d64-4df8-950e-e7610b1acb1a))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2c309c81-c1f9-40fe-b4b6-419e622aa21a))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8730ef73-f57b-461f-a04a-18c6c5d34601))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b3e0f0fd-b928-4559-a553-2e8e4d185dc1))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ee07f8cc-83b0-49c1-9cc0-ff93218d4440))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 580ef17d-72b8-4302-9b7b-a3e67c7b8b3a))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 76723ae0-98cc-4b81-9d3c-3a3c4510334a))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7b95e6af-2b34-4569-b69a-50ee61eb247e))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9d5afffb-404a-4df1-97f4-ebffaea3c353))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f1db768f-c3e9-4720-b237-12e8da6c81c7))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp e25be556-b739-400e-b7fe-2959e0971b1c)
    (at 170.32 36.5 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 101f9d5e-8f2f-4ba9-a64a-ba186f64f944)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 3adf9bc6-8272-4b49-aebd-2477a633eb61)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 13a6a7c8-6cab-4fe2-87d6-0cb45845ff7d))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a1240b4e-cb2f-4f6d-b9f5-f942cdf2b6d2))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bef895c9-a9f4-4c29-98d7-4c6a869171ba))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cf3191ef-00b5-4b97-890b-e7d7d29daa88))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d020bba9-b800-43c8-aec1-846570b099b4))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 07d40de0-a66b-4fb3-9dcb-eb890d830c12))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3b7f25dd-5f4b-4c4e-91bd-6cdadb942565))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5d2ba00e-cb36-4b7b-99ce-a26a47a55f32))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7af5bfa5-0c7c-4f9b-8352-2fb999de99ce))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f5306bfe-e616-4295-b0fd-63c136e1f813))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 31fabb25-4e8a-4732-a636-e576a92a97f8))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4bd6cec9-d265-49a7-bee4-95beb3bacc7f))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7ece4323-7b9a-4abf-8788-d3ed9a53baf3))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 81552558-1778-4181-8154-a74fcb1f76f7))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cf78983b-317d-44e2-8239-53ff96eeae5f))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6eabe17b-7df5-4898-911d-ede5ae11bd47))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 818f88c3-90fa-4c52-a309-019e96a572e3))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9a3dba5f-f0db-44b9-bb8d-6b1ec60d082c))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b3cae61e-30b8-46ab-ada2-10be0f56a126))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e2c3ef92-2c8a-499b-91a4-f718c876798f))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1f955138-ba03-472f-993b-2b236f79a844))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 31728259-ebe4-4003-9ec2-62f953905b2f))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bd1cbf47-0f0b-4607-b85e-40ae09b9296e))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be84a8b7-e590-4d11-96c6-8c5dc8238c76))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cbfb93a2-34ae-494b-86ad-2b926d7462af))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp eea561ac-cdca-4397-9cd9-bf78846106c3)
    (at 128.41 39.04 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 119513c4-14ed-4bd8-a24c-1f96651e6811)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 365779bf-d46b-4861-851a-b69868fb94f3)
    )
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0bd5482b-c6e1-4ab9-b927-068ec39aa293))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 10596ddd-bf51-4a2f-a6cf-63b2b12f3342))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1e422d3d-2a51-4901-a35d-a611e9fc77e8))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c97bcc74-4de3-4eb3-867a-1b4d6077d40c))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f6d365b3-b792-4478-94eb-022d1a33b281))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c00c433-7bec-42c8-97f7-6d0f5ac902a6))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6d488c6b-983b-4e8e-bf9f-52b02cd90a79))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 83841bcf-34d1-4bf7-9c8d-96fb907ae7d2))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c50a7518-8d3e-4933-8588-bbc05669b89c))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cf5e9240-df01-48c1-980c-cab2c7ac49c3))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0fed8ef0-c912-4a15-b407-77a53351fb42))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4b3e4a5f-86a4-4470-afc1-d7560dd392d6))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e952e442-6114-4b19-94e6-63f732ec4ad5))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f2c58c6e-3654-4320-9f8b-8ce0f5daf24c))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f6223394-491a-4832-8081-65c005188895))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 27ca0301-271c-43cc-9d2e-91ee85f38f2f))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4e81f740-1741-4128-925f-d7bb4aa4c335))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 74529bd8-4d38-4a0d-8e53-be70f233fd30))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 775f2ec4-adf3-4882-8153-faaada2afed6))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f2bd6c29-dd90-41fe-b2ad-0f1be4fa7af5))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1a5a330f-1c12-48de-be4c-93cf8ae09a0c))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 306d8538-62b8-4a4c-be6e-dbcbb8190464))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3e1c41c1-c7b3-43a4-a5e1-9385656c5c34))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 88657e80-6f2f-45d4-a4d8-8e5c282fb8b5))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fdee7268-2824-4475-8a6e-2ead59e978c6))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp f1ab38a3-f272-43cb-b2d6-59417d4e8f73)
    (at 157.62 36.5 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f2185c80-1ce2-486b-9a84-d607c8c9888a)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp bd903049-4ae5-42fc-b90c-57959f37bb37)
    )
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8450dfb0-409c-4b4d-bf79-c4825b34179c))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9e988241-be9f-48ce-a8d3-471d25ce55e3))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d2a5be67-aa1d-4493-ad5b-666fbb16f9e7))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d34c8c58-54e6-4349-832b-e5903ebee934))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d85768af-067f-46fc-8403-1f760d49a291))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 09828520-c9fe-4a90-adfb-5e5d4fd7f063))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5803d152-4282-4610-b767-f47ccbdab1ac))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 96a7910a-eb22-43ff-b685-a0a26ec06660))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cd05c88d-cf54-45c9-a624-0c18dc580a23))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e47794fb-3120-4239-ad74-476ccf5a7f34))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 55878824-7dd3-4780-aaef-27e4f5bc52b4))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 85c630de-e784-43bc-bfea-d0223721445b))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a8f2a9ea-8116-4e11-97a8-1f3b4d6d4bb7))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aa2701ce-f60a-459c-a3af-3912e2257167))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d1ff1398-3dd7-4efd-b5b1-22f13650366c))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1fccbe8b-3a25-44c6-9289-afe42f0f7f6c))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5c301c06-2b7c-4ff3-8aaa-af0b2d45312c))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8bb6578b-272f-43cc-a24f-af9f507e804e))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a838dfc8-6ea1-4085-afa7-9cd931eca754))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ee25e884-0318-45f8-902e-ade5958d18fb))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1ea7bcbe-48d0-4529-8cde-03eb18f4badc))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 25ff11a2-99f0-4ea0-9962-25db145273f8))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3dfc1213-6923-4fa7-af36-93a20e6dccc1))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8b66fb26-7a98-4114-bdd7-90bdc35f46ac))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d72ed358-4218-411d-8527-9eed5d006398))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp f48f4a24-3d13-4012-aa77-1750ab85761f)
    (at 141.11 39.04 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fcd33288-a50f-4db4-aab3-0fe9b799656e)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp aeb629e1-15e8-4cf0-ae50-355fac59a219)
    )
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 53bb7e1a-17c3-4c36-acb5-77d86e0be842))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 589f9cdd-c91f-4f54-aa18-2415bc2f4a08))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b8ccefd3-977f-402b-88dc-89fb6baa064f))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cb4c0e56-dad6-4306-ac04-b2e3e53b4029))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d5f90916-a870-48f4-a620-3da8e692a125))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3253b248-50b2-484c-8d45-85afbb019e06))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 37a70c70-c305-41bb-b7fa-6b7ac39b07ee))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3ad61f9-5ded-46b7-ba2d-750010d6df39))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eaa47c74-d866-40c9-b7cf-4f775f75c5e5))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec8f976d-a79e-47d6-b3ed-58418f84280c))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 954561fb-fe12-44a1-a970-74cfa825d604))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 989b308a-dd01-4737-a504-a9f7d8be4fe2))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b92a41b1-1a25-4501-ad09-72db0470758a))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bc127c9a-bab3-4414-84ec-5303bf2ad081))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c2834905-df75-4cb6-bb76-b357a92f5e46))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2d9fc354-8fb9-45bc-bbde-162014316444))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50cbc82b-cc5e-42a3-ba32-3f1cdd5cebac))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6cba58af-01c8-4fb6-a9a5-221281d72883))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9c38405b-491f-4e14-8446-a8b13b848a35))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a50ef61f-f1c8-44f3-a27c-cec56e67b09a))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 678318ca-a542-4fce-9da6-f1cde7ca8242))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6aa9bccb-e4d8-4739-ab55-50609188ceba))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b7e17a20-16cc-4db9-bedb-0606ca625b0d))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ca0664bb-c5d9-4a16-a6fb-2fcd6dc80fe4))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d8b5c194-2ed8-4f1d-bda2-e361ad2634f5))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp f55e5214-143b-44e3-b462-14fa074fd82f)
    (at 141.11 27.61 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 47bbc4c5-a1e5-428c-9cb2-467694aa6047)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp fce043e2-447f-4b54-b441-98c4f98351d9)
    )
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 276cf77e-24de-447d-8fe7-4983d63bbae2))
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2863b31f-8cf1-41e7-bb2d-d40fa2565159))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 495945e5-2b16-44c5-90ad-3d95dd3f7749))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5d91cdc3-4a3c-4c5d-b863-ed11bbd24009))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 80528b51-4a89-4169-90c1-48e86ee6e126))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 28d8c444-ea4c-487f-ac39-869ba7d3227d))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 60124d47-e91e-45e8-9787-0c5099e83cf4))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 64ebfde4-49ca-479b-b4f1-a23d3678b2a6))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7251770c-a074-4cdc-a844-84ac147ddda0))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e01e12c4-bbd6-41bf-9c50-e6dfec24f299))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 55b194a5-9869-4cfb-ac00-b8da320c7fd9))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b418d24e-3fb4-424c-a135-3698fff21ff7))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e7c2c9ac-03c5-4438-8dc8-dbcf177eb881))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e84b3d62-a8b2-4a50-9dcc-ccb5a3bb0d1c))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ec9ef8d1-4784-4fd4-8c26-c115a39edda0))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3272679a-e358-40ea-a6cc-f43d838e53c8))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp aaa6bb9a-047b-44b4-8702-467f08990534))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b79fe11f-4e58-44c8-981d-c914e1351e1a))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ceb6b965-0c35-4fa3-b9e3-71801e555675))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e6af92b4-827a-4155-a1f6-bb92fc2d576b))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 40e56fae-3a9d-4b58-859c-6797da4e12b3))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c6f2a53-0b76-4709-b672-4cf98da1d212))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7b9f76bc-9531-48dd-818f-8f786d13fc1f))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e21fe3a0-7a46-4609-832e-e585e9f49e8e))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f6ee206c-7f04-4c28-aead-42e3476e15a0))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp f6260e6a-101d-4452-86da-1f20ce050767)
    (at 144.92 49.2 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 889a094d-1d6d-4cf1-9826-532cac4061b8)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 1c0559aa-693e-4d96-a822-e58c71e58f0a)
    )
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 19b21f7e-36e8-4721-aea8-a5a3cb55d5df))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1ac9b251-5b8a-4570-a8f2-bfd49ee3b5b9))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 279cefd9-0d39-4af4-b8fe-f6a3c2e4a80d))
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 73183617-e16f-4ab6-94a5-3e5cf37a6bc0))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8e5623d9-983f-458f-8c5b-5776596ddc26))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 10b91263-30fc-4681-867c-9ca5787a2ec9))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2d44c007-5370-4445-9270-3b3b98781cf4))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 7398c5c1-ed19-4163-9c60-c32ea1d55012))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 82de0ca7-3fa9-4bdc-90e3-c3d8d1fdbe28))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3db08ad-da83-4243-8b31-b0b02089ba71))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 015de922-8509-42af-ac65-8a9f89583e3c))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3de4811d-9273-4a0a-8c0a-0f8342b0b31c))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5137fab0-1df9-4591-9e12-c77ec2516b6a))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be54ab4c-8da9-414a-b1bb-43428b384b3e))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eafc3e87-a8ef-4d42-9eac-527ef5096c0c))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 057e30dc-f5a7-456f-99a3-664be32b9f8e))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3ea1ed80-176b-4007-be48-e2150c95e86c))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4c385439-93f3-418c-b3e3-a1ed1a0f9719))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8c8858e4-0fa8-408a-b305-67c9bcd9c547))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ff21fb09-8aee-4472-b252-5b4757295128))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 22acc3b7-e5e5-4359-b454-3e0fb9f18a19))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2d58625f-785e-4924-bc55-56401ad52280))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c5bf0e43-a6bc-404c-baf1-450a88ae4f40))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp de2714ac-73b5-463b-9793-8c605caee6fe))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e34e8d4e-601b-4480-9661-e8f9a77741fa))
  )

  (module "common_footprints:5x5_proto_array_1.27" (layer "B.Cu") (tedit 5F85D7CE) (tstamp f7d43d55-8210-4680-9e18-ed2184826bd7)
    (at 128.41 21.26 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp d7045923-24b3-401f-b7b2-0a0155ea2b32)
    )
    (fp_text value "5x5_proto_array_1.27" (at 0 -1 180 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 2698646e-95c6-4e71-9e93-2cce87f33801)
    )
    (pad "0" smd roundrect (at -2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1ee07f9d-7c90-439a-a35f-dff60504f28f))
    (pad "0" smd roundrect (at -2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6d5b476b-eec2-4abd-b4f1-485a037f4904))
    (pad "0" smd roundrect (at -2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 844ff4fd-d3c4-45dd-bd24-dfd786eebba4))
    (pad "0" smd roundrect (at -2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp db8e8004-0758-469b-ad6d-986bc835f687))
    (pad "0" smd roundrect (at -2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp eaf57576-606e-4ea4-a60f-8c55fc6d0f8b))
    (pad "1" smd roundrect (at -1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2605155a-aee3-4155-8d0f-d96b0f0d55c9))
    (pad "1" smd roundrect (at -1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 732218da-55d4-48aa-87c2-64486fe43097))
    (pad "1" smd roundrect (at -1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp acd7b930-6bb1-46aa-899e-7c5d14148154))
    (pad "1" smd roundrect (at -1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c88650b2-eab3-49c7-a699-b13792378a80))
    (pad "1" smd roundrect (at -1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d336756a-bf27-45cc-8dfd-253023ebe7e0))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 045b12c8-2bb0-413b-a09e-81cf7a6bef33))
    (pad "2" smd roundrect (at 0 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5052b637-3ec4-419b-ac52-7e5c44dffe75))
    (pad "2" smd roundrect (at 0 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6177694a-8ecc-4765-9422-6eb6ee849b44))
    (pad "2" smd roundrect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d4e8ca61-7c3b-49f4-8d59-29a2b5ab7801))
    (pad "2" smd roundrect (at 0 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d9a207be-229d-4399-b189-a58312f3be68))
    (pad "3" smd roundrect (at 1.27 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f75e12a-4238-43ca-a5de-925aad9a95ec))
    (pad "3" smd roundrect (at 1.27 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3f00d0b3-c836-410a-8a68-c3bbbf7d3a02))
    (pad "3" smd roundrect (at 1.27 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9a27e27c-9cc4-42b7-a368-ae5d38f2a9ea))
    (pad "3" smd roundrect (at 1.27 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d114ae98-3161-40fd-96af-ed258fe57b20))
    (pad "3" smd roundrect (at 1.27 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f2a80413-1741-42ee-93eb-7cc3b1e87ca3))
    (pad "4" smd roundrect (at 2.54 1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4b4e460c-bcd1-4600-9a28-2ee60be32db5))
    (pad "4" smd roundrect (at 2.54 0 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 5af2cf1d-f2a9-4453-a4ca-fab37e5f28ec))
    (pad "4" smd roundrect (at 2.54 -1.27 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ad6c6d2e-2217-4ba9-b8a8-3008238e6777))
    (pad "4" smd roundrect (at 2.54 -2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d5465768-d607-419e-87a0-bde16c0e43ba))
    (pad "4" smd roundrect (at 2.54 2.54 180) (size 1 1) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp fa999884-ef6c-4c5f-b8db-aa94f41bace2))
  )

  (module "common_footprints:5x5_proto_array_2.54" (layer "B.Cu") (tedit 5F85D7D7) (tstamp feb9d3d9-6c99-43ab-a55c-8f717eab7a71)
    (at 132.22 11.1 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp f0da697a-880e-4e8b-8f45-72856734691d)
    )
    (fp_text value "5x5_proto_array_2.54" (at 0 -1 180 unlocked) (layer "B.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
      (tstamp 54d2c399-9c0f-414e-b565-a8fa07302b3c)
    )
    (pad "0" smd roundrect (at -5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2ac38a82-fc90-4868-a94c-8aebb45ad8e2))
    (pad "0" smd roundrect (at -5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52fc4ba9-77b0-4224-b653-0ac97ba8d2f6))
    (pad "0" smd roundrect (at -5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 886d5436-d631-4c8c-b4cf-640877025cbc))
    (pad "0" smd roundrect (at -5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cff8179f-5806-44ec-8cae-0df4768d400b))
    (pad "0" smd roundrect (at -5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f4125e7a-589b-4634-b047-0369ef27902b))
    (pad "1" smd roundrect (at -2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 004bafc6-171c-4379-bebb-59a3ded275dd))
    (pad "1" smd roundrect (at -2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 209ccb14-0585-40cd-9d9a-ab1448ddf2b2))
    (pad "1" smd roundrect (at -2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 29e79e78-b2fe-484a-8849-7161d2a74abe))
    (pad "1" smd roundrect (at -2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 405180e7-1e4c-482f-908a-096877628ad0))
    (pad "1" smd roundrect (at -2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a77f2ef7-bbfb-41e2-b865-f4f37cc79fcc))
    (pad "2" smd roundrect (at 0 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0984d164-68e6-47bd-90a8-67dbd4eafdc7))
    (pad "2" smd roundrect (at 0 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0bb968d0-a289-49da-b989-7ac5ab8ac4aa))
    (pad "2" smd roundrect (at 0 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 243f5a2e-99ac-4c9f-b8bf-b7d76a329b8d))
    (pad "2" smd roundrect (at 0 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4e27282b-f5e2-40fd-a5fd-0b0f703d22aa))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 75e04bd0-078e-4ad1-9842-9a97ea1ce56d))
    (pad "3" smd roundrect (at 2.54 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1cdc8c80-8636-439e-a8e7-4d48212d6ffc))
    (pad "3" smd roundrect (at 2.54 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 61dd3abe-4e08-4292-bd10-0808e756c6a8))
    (pad "3" smd roundrect (at 2.54 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 95b0280f-9a90-40f6-839f-6033596f11ab))
    (pad "3" smd roundrect (at 2.54 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp b93724fa-62e2-40b8-bd32-a1b9dad41dc0))
    (pad "3" smd roundrect (at 2.54 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp bd490049-7536-4604-ad38-6b1e766dd115))
    (pad "4" smd roundrect (at 5.08 0 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 310d45af-a6b8-4281-b4ab-1506d33397f1))
    (pad "4" smd roundrect (at 5.08 -5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 436af47c-7050-4d97-a693-1132145bb296))
    (pad "4" smd roundrect (at 5.08 2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 6c5dd62f-5bcb-4660-a6a8-03c280f456d4))
    (pad "4" smd roundrect (at 5.08 5.08 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 85911348-2964-4d3e-adcf-03bc9e3fa375))
    (pad "4" smd roundrect (at 5.08 -2.54 180) (size 2 2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp f8a306e2-a642-4f1f-8c39-925a15f14ee6))
  )

  (gr_line (start 159.727 83.4) (end 159.727 98.4) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 01afbce3-c0ef-4fd2-8a9b-faed85a298d5))
  (gr_line (start 121.727 83.4) (end 121.727 -1.6) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 03312bc8-89fe-471f-964e-90c5708e8310))
  (gr_line (start 159.727 -1.6) (end 177.727 -1.6) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 091e3232-f133-4b01-9e08-37c4a16e4aa5))
  (gr_line (start 159.727 -11.6) (end 159.727 -1.6) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 1bda6c77-bd3f-4212-990b-0710eed5cfef))
  (gr_circle (center 125.5 1.9) (end 124.15 1.9) (layer "Edge.Cuts") (width 0.16) (tstamp 29db33be-d616-4a84-89ed-7c42292849b8))
  (gr_line (start 177.727 83.4) (end 159.727 83.4) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 2c4e0714-4432-4a78-8a7e-58440d551c50))
  (gr_line (start 139.727 83.4) (end 121.727 83.4) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 3a175022-ffc8-42de-8fe3-64f5fbbe751e))
  (gr_line (start 159.727 98.4) (end 153.454 98.4) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 3f3a1c23-370c-4a48-aab1-711f7abf4519))
  (gr_line (start 153.454 98.4) (end 153.454 102) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 517c86e7-e61a-415e-a8de-dd68526cbb2a))
  (gr_line (start 146 98.4) (end 139.727 98.4) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 67f1cb96-74c7-483b-b176-f8d279f8ba7b))
  (gr_line (start 139.727 -11.6) (end 146 -11.6) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 7e7e86da-7fd7-429a-852f-28824946f58c))
  (gr_line (start 153.454 -15.2) (end 153.454 -11.6) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 80f2d637-9ed0-4aac-90ae-e01ff0b871ae))
  (gr_circle (center 174.5 59.9) (end 173.15 59.9) (layer "Edge.Cuts") (width 0.16) (tstamp 82e3f3c1-43b2-4488-9df2-4e9a47879eef))
  (gr_line (start 139.727 -1.6) (end 139.727 -11.6) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 856061d0-08c4-4ae2-9fe3-d80d10349d70))
  (gr_line (start 153.454 -11.6) (end 159.727 -11.6) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 8b104ef7-a8a0-43b3-9f72-21d580b73c3c))
  (gr_line (start 153.454 102) (end 146 102) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 8bc0949c-b4d4-4794-8252-72a3fecc16b0))
  (gr_line (start 146 102) (end 146 98.4) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp a7758fef-f54d-47e4-99fb-ffabc8a5aeec))
  (gr_line (start 139.727 98.4) (end 139.727 83.4) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp ad507930-7a2d-48ce-8a81-e88f23e9b235))
  (gr_circle (center 125.5 59.9) (end 124.15 59.9) (layer "Edge.Cuts") (width 0.16) (tstamp b0fbe9bb-831e-482f-bf2f-f757511b0300))
  (gr_line (start 146 -11.6) (end 146 -15.2) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp b8cd6b3f-9fe3-47af-9a91-4c34bffcee5c))
  (gr_circle (center 174.5 1.9) (end 173.15 1.9) (layer "Edge.Cuts") (width 0.16) (tstamp bdf96955-9d5d-4697-ac7a-8b6d057cbfb6))
  (gr_line (start 146 -15.2) (end 153.454 -15.2) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp c60bfc63-679c-4b54-ac54-b430c84415d4))
  (gr_line (start 121.727 -1.6) (end 139.727 -1.6) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp d57296c1-d4be-4ff5-a130-d6899e33ef6c))
  (gr_line (start 177.727 -1.6) (end 177.727 83.4) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp dc765672-fd43-468c-b7c2-9fcb68aa4455))

)
