(module "5x5_proto_array_1.27" (layer "F.Cu") (tedit 5F85D7CE)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 77ecf778-4831-4e22-9d9d-dfdb061a3696)
  )
  (fp_text value "5x5_proto_array_1.27" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f469d53f-eb34-426d-b276-e4e071bdde9d)
  )
  (pad "0" smd roundrect (at -2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 12d1bfbd-1eeb-4aef-8276-cccec516c28a))
  (pad "0" smd roundrect (at -2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 82a14ab9-b22d-4b76-aec4-19187967821d))
  (pad "0" smd roundrect (at -2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9770fcbf-05a4-476c-8520-fce2dd7ab8bc))
  (pad "0" smd roundrect (at -2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a9edd8f1-3520-4a1c-8bbb-d08fb8cb4fa9))
  (pad "0" smd roundrect (at -2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d5736c89-c7e3-4400-bcf9-07220bc683de))
  (pad "1" smd roundrect (at -1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 2e5d5e76-d9d0-4f86-aa28-1efa5d672760))
  (pad "1" smd roundrect (at -1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 46fdd886-71e9-4576-9c3d-cefc8cfdd540))
  (pad "1" smd roundrect (at -1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4f2f09c3-efc5-4760-9e79-b6f0d65ec9a6))
  (pad "1" smd roundrect (at -1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 755a8741-8553-4916-a4a8-4069ffceca58))
  (pad "1" smd roundrect (at -1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c28163b6-46ee-4d02-84ec-376624099881))
  (pad "2" smd roundrect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4325f110-3ce2-403e-9507-de9509dbdebb))
  (pad "2" smd roundrect (at 0 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 50d87612-11bd-4e26-9899-c2754ed96d53))
  (pad "2" smd roundrect (at 0 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 67e8d795-6d9f-411d-9b60-a959f9aaf125))
  (pad "2" smd roundrect (at 0 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 8d5b303b-82cc-434c-a91b-b60c326005d1))
  (pad "2" smd roundrect (at 0 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ee449797-7609-46ae-812a-8e59c162e0e9))
  (pad "3" smd roundrect (at 1.27 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0299b288-3e65-4368-834a-94768ab57145))
  (pad "3" smd roundrect (at 1.27 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 1ae8e461-c6c0-449c-9269-fed510ffeb3a))
  (pad "3" smd roundrect (at 1.27 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c910a252-8e74-4aa8-9130-7e1c1929ed25))
  (pad "3" smd roundrect (at 1.27 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dde301d8-5dfa-43fe-bffc-922d8d7442eb))
  (pad "3" smd roundrect (at 1.27 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ef0e6c05-6189-4a82-b47f-40eb9478a0a5))
  (pad "4" smd roundrect (at 2.54 1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0b5daff1-65fd-4b38-9301-83e0f2ea777d))
  (pad "4" smd roundrect (at 2.54 2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0f76b6c3-2efa-4142-af97-5166d593cdd2))
  (pad "4" smd roundrect (at 2.54 -2.54) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 195a3719-3772-454a-9c20-c4f6ce3f3a01))
  (pad "4" smd roundrect (at 2.54 0) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 981c7ad4-4105-45dd-b3e9-82b76e401b29))
  (pad "4" smd roundrect (at 2.54 -1.27) (size 1 1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp df3ca1e0-f761-4a93-b773-4aa1160a8441))
)
