(module "5x5_proto_array_2.54" (layer "F.Cu") (tedit 5F85D7D7)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 753141bb-5ae7-479e-9578-0feb0f4b8566)
  )
  (fp_text value "5x5_proto_array_2.54" (at 0 1 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 57220cf6-59cc-4c9f-8a94-dc3cfdefc7fe)
  )
  (pad "0" smd roundrect (at -5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 09f8c89b-90e1-4c04-bd1d-052979ec6196))
  (pad "0" smd roundrect (at -5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 9bc67f58-13cd-4e09-adec-de7898be0cc1))
  (pad "0" smd roundrect (at -5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a488b546-12f1-4fa1-8a78-4c056e2b42f5))
  (pad "0" smd roundrect (at -5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp dbe59d95-09fc-4024-9c9c-995d0ec2c487))
  (pad "0" smd roundrect (at -5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ef2af5be-3a9e-4b3c-97a3-b364b8e1a6b6))
  (pad "1" smd roundrect (at -2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4af2efce-5dbd-4413-80d8-6452e0a7786c))
  (pad "1" smd roundrect (at -2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp be227bf0-177e-4338-8ad0-f250c31a6ed2))
  (pad "1" smd roundrect (at -2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp d7872085-ccc6-4dde-9382-b10568a7b0b4))
  (pad "1" smd roundrect (at -2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp e3bbe957-26f3-467a-a4bc-c81067393e14))
  (pad "1" smd roundrect (at -2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp ef080744-0001-4e24-95f6-aa6cb5e586b1))
  (pad "2" smd roundrect (at 0 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3853e370-323c-4bc2-a8f8-275cabeb59a5))
  (pad "2" smd roundrect (at 0 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 46778bf2-44c4-49c1-bbe8-36cfc97cf151))
  (pad "2" smd roundrect (at 0 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 92b2b360-3d29-4fd7-aa1d-ef700d5e340a))
  (pad "2" smd roundrect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a28c387c-5ce7-4460-b77c-4917e8bd39dc))
  (pad "2" smd roundrect (at 0 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a9a4420d-7aed-4b91-a0dd-c8e7e0c0487f))
  (pad "3" smd roundrect (at 2.54 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 07edafdf-0fac-423e-bfd2-5369403bf9e7))
  (pad "3" smd roundrect (at 2.54 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 0da2c4e2-d9d7-4f4f-abd9-d49ff3795d7f))
  (pad "3" smd roundrect (at 2.54 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 3c619b85-bc84-47ea-8d38-0e07d0ec746f))
  (pad "3" smd roundrect (at 2.54 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 52230ff3-84d1-4fc7-b8c0-be33979df579))
  (pad "3" smd roundrect (at 2.54 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp c3edaf48-45d5-439e-8b1f-31a837ff0c3d))
  (pad "4" smd roundrect (at 5.08 0) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 38968eac-0ce3-4361-9fe0-1ac4b2a6396a))
  (pad "4" smd roundrect (at 5.08 2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 4bc31ef6-1c65-455f-9cde-b6afa6d28812))
  (pad "4" smd roundrect (at 5.08 -2.54) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp 982e7a13-e49e-4d15-b592-8a5d9ea65e45))
  (pad "4" smd roundrect (at 5.08 -5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp a85436e3-4587-498a-b92f-d7ad750cac3b))
  (pad "4" smd roundrect (at 5.08 5.08) (size 2 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.15) (chamfer top_left top_right bottom_left bottom_right) (tstamp cb7276a9-c774-4419-8e99-07fc9305df83))
)
