(kicad_pcb (version 20201002) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (grid_origin 150 150)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )


  (net 0 "")
  (net 1 "/tru_b1")
  (net 2 "/tru_b2")
  (net 3 "/tru_b3")
  (net 4 "/tru_b4")
  (net 5 "/tru_b5")
  (net 6 "/mesh_dn0r")
  (net 7 "/mesh_dn1r")
  (net 8 "Net-(J1-Pad13)")
  (net 9 "/mesh_dn1s")
  (net 10 "/mesh_dn0s")
  (net 11 "/tru_t1")
  (net 12 "/tru_t2")
  (net 13 "/tru_t3")
  (net 14 "/tru_t4")
  (net 15 "/tru_t5")
  (net 16 "/mesh_up0r")
  (net 17 "/mesh_up1r")
  (net 18 "Net-(J1-Pad3)")
  (net 19 "/mesh_up1s")
  (net 20 "/mesh_up0s")
  (net 21 "Net-(J2-Pad13)")
  (net 22 "Net-(J2-Pad12)")
  (net 23 "Net-(J2-Pad11)")
  (net 24 "Net-(J2-Pad5)")
  (net 25 "Net-(J2-Pad4)")
  (net 26 "Net-(J2-Pad3)")
  (net 27 "Net-(J2-Pad2)")
  (net 28 "Net-(J2-Pad1)")
  (net 29 "Net-(J3-Pad13)")
  (net 30 "Net-(J3-Pad12)")
  (net 31 "Net-(J3-Pad11)")
  (net 32 "Net-(J3-Pad5)")
  (net 33 "Net-(J3-Pad4)")
  (net 34 "Net-(J3-Pad3)")
  (net 35 "Net-(J3-Pad2)")
  (net 36 "Net-(J3-Pad1)")

  (module "common_footprints:8mm_plug" (layer "F.Cu") (tedit 5F85D873) (tstamp 1811a88f-07ba-47da-8eb6-fe2ae8cc9dcf)
    (at 150 182.9)
    (property "Sheet file" "/home/user/research/rotohsm/prototype/mech_pcbs/rotor_vstrut_pcb/rotor_vstrut_pcb.kicad_sch")
    (property "Sheet name" "")
    (path "/6a9bf823-0c9e-40ee-9e07-825e78b3c53a")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -4.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 46dbf47a-23a5-4157-9ede-c76fc4bce3e3)
    )
    (fp_text value "bottom" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ea4eb57f-8a9c-46e5-b930-5bd96e175751)
    )
    (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 64d931c2-62e6-4149-b14f-a13fe38d7c4a)
    )
    (fp_line (start 7.5 -0.8) (end -7.5 -0.8) (layer "Dwgs.User") (width 0.12) (tstamp 3fe23836-cc7b-46ec-a352-4dc0902b9924))
    (fp_line (start -4 0.8) (end 4 0.8) (layer "Dwgs.User") (width 0.12) (tstamp df02e2b3-3d66-4a63-aa56-835335d7ee4c))
    (fp_rect (start -4 0) (end 4 4) (layer "Dwgs.User") (width 0.1) (tstamp 409caab0-3c0f-49f0-a611-a043ee06f49e))
    (fp_rect (start -7.5 0) (end 7.5 -5.6) (layer "Dwgs.User") (width 0.1) (tstamp 7f6df47d-e42d-401e-b33b-939ee6b96513))
    (pad "1" smd rect (at -5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 28 "Net-(J2-Pad1)") (tstamp 752b16df-6e19-4e6d-9b52-0c4b5ace21d6))
    (pad "2" smd rect (at -2.5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 27 "Net-(J2-Pad2)") (tstamp 4c9a1e30-c59d-4454-a9d1-244ffd0b931d))
    (pad "3" smd rect (at 0 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 26 "Net-(J2-Pad3)") (tstamp aec0543d-15ae-408e-bf68-3198c828b7e2))
    (pad "4" smd rect (at 2.5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 25 "Net-(J2-Pad4)") (tstamp 4e3d050d-ad8b-4a44-9735-7998098fc3e5))
    (pad "5" smd rect (at 5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 24 "Net-(J2-Pad5)") (tstamp 95439f48-970b-4202-8f38-7d1900c60922))
    (pad "6" smd rect (at 5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 5 "/tru_b5") (tstamp 73203094-da20-4d39-9d9b-f07f93fa8311))
    (pad "7" smd rect (at 2.5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 4 "/tru_b4") (tstamp af2c8835-9c0c-4999-a175-84b72736e04a))
    (pad "8" smd rect (at 0 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 3 "/tru_b3") (tstamp 60a98580-72eb-48cd-b8ff-37c7f2f9ca68))
    (pad "9" smd rect (at -2.5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 2 "/tru_b2") (tstamp 3eef296a-f77d-43ff-80d0-5f75c1aaeba1))
    (pad "10" smd rect (at -5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 1 "/tru_b1") (tstamp ed2d1120-07ed-4b29-b009-a3a81d490829))
    (pad "11" smd rect (at -2.5 2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 23 "Net-(J2-Pad11)") (tstamp ad8b0f3c-caa9-4026-ad43-7322f36bd248))
    (pad "12" smd rect (at 0 2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 22 "Net-(J2-Pad12)") (tstamp a00f0f04-3b34-48ec-b1a4-9f63a5591201))
    (pad "13" smd rect (at 2.5 2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 21 "Net-(J2-Pad13)") (tstamp d553e627-9e3e-4559-b66c-2318d354e975))
    (pad "14" smd rect (at 2.5 2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 4 "/tru_b4") (tstamp 341e6d94-7f2a-4f65-a527-00b83ce4fc49))
    (pad "15" smd rect (at 0 2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 3 "/tru_b3") (tstamp df6d20d5-c0de-4b5f-ab1a-b9141591f583))
    (pad "16" smd rect (at -2.5 2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 2 "/tru_b2") (tstamp a2b6cfa4-3683-4006-8715-2e85fa846011))
  )

  (module "common_footprints:15mm_plug" (layer "F.Cu") (tedit 5F85D886) (tstamp 578b0775-c05a-42d7-9223-0db1f2d9868f)
    (at 150 173.35)
    (property "Sheet file" "/home/user/research/rotohsm/prototype/mech_pcbs/rotor_vstrut_pcb/rotor_vstrut_pcb.kicad_sch")
    (property "Sheet name" "")
    (path "/92226583-c767-4448-ada0-e9e18d9afd62")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -4.65 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 903aa136-9f96-48ea-b46d-43288f095503)
    )
    (fp_text value "base" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e9df4db4-d970-4d88-a289-758e65dbc1ba)
    )
    (fp_line (start 7.5 0.816678) (end -7.5 0.816678) (layer "Dwgs.User") (width 0.12) (tstamp 6e6ff282-9821-4559-8d56-5b4ae0dead3a))
    (fp_line (start 7.5 -0.8) (end -7.5 -0.8) (layer "Dwgs.User") (width 0.12) (tstamp d22d001a-a6d5-42fa-9589-cea048e05d9a))
    (fp_rect (start -7.5 3.8) (end 7.5 -3.8) (layer "Dwgs.User") (width 0.1) (tstamp 93af1ee5-e77c-4544-993d-b447b61de170))
    (pad "1" smd rect (at -5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 20 "/mesh_up0s") (tstamp a7704729-a3a8-4988-8291-3c1dd0e26c24))
    (pad "2" smd rect (at -2.5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 19 "/mesh_up1s") (tstamp e3c7e4d5-060b-49c7-8d20-37193f05fc49))
    (pad "3" smd rect (at 0 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 18 "Net-(J1-Pad3)") (tstamp 56482b1a-6918-4003-a17f-55c3c850703e))
    (pad "4" smd rect (at 2.5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 17 "/mesh_up1r") (tstamp 8dbe3ec6-6d86-4210-9433-6e355dca12fe))
    (pad "5" smd rect (at 5 -2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 16 "/mesh_up0r") (tstamp b01114a6-9b1a-4ca8-93b4-506c1357de33))
    (pad "6" smd rect (at 5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 15 "/tru_t5") (tstamp b034e8ab-7d64-4096-972e-31e795220787))
    (pad "7" smd rect (at 2.5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 14 "/tru_t4") (tstamp 6e53320f-97ff-4796-a8be-65fb54cd7188))
    (pad "8" smd rect (at 0 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 13 "/tru_t3") (tstamp 34d7bb8d-3199-4e47-b240-be1918685ef4))
    (pad "9" smd rect (at -2.5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 12 "/tru_t2") (tstamp 9c44e131-7612-4518-bde6-55c1df78ad8e))
    (pad "10" smd rect (at -5 -2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 11 "/tru_t1") (tstamp 7545b562-4b6b-4611-8a6e-51bda42bfd96))
    (pad "11" smd rect (at -5 2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 10 "/mesh_dn0s") (tstamp f31beca3-bfa2-41b4-bd35-5c20926400fc))
    (pad "12" smd rect (at -2.5 2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 9 "/mesh_dn1s") (tstamp eda422f4-0823-4de0-9523-5853d09d87fe))
    (pad "13" smd rect (at 0 2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(J1-Pad13)") (tstamp 0af6e3e5-4a9c-40be-8404-5ab7598193c0))
    (pad "14" smd rect (at 2.5 2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 7 "/mesh_dn1r") (tstamp 81b76107-00c2-44ec-9927-f500703db5c1))
    (pad "15" smd rect (at 5 2) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 6 "/mesh_dn0r") (tstamp 4a9d08af-241d-426b-a69a-10294d5f35cf))
    (pad "16" smd rect (at 5 2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 5 "/tru_b5") (tstamp 5a43305b-661a-4617-8c75-643d08135550))
    (pad "17" smd rect (at 2.5 2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 4 "/tru_b4") (tstamp e3e2c137-1910-41a4-8367-824a23a182fb))
    (pad "18" smd rect (at 0 2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 3 "/tru_b3") (tstamp fcb42c8b-49f6-4a06-90b5-f7488d08babc))
    (pad "19" smd rect (at -2.5 2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 2 "/tru_b2") (tstamp 97b9a8e3-9c01-4312-86f1-f75c8080097e))
    (pad "20" smd rect (at -5 2) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 1 "/tru_b1") (tstamp 46db2c9f-94bf-4f20-bdbc-1d09337d06ad))
  )

  (module "common_footprints:8mm_plug" (layer "F.Cu") (tedit 5F85D873) (tstamp bc6c26a6-39e2-4b53-8e0c-279085b5aea5)
    (at 150 21.3 180)
    (property "Sheet file" "/home/user/research/rotohsm/prototype/mech_pcbs/rotor_vstrut_pcb/rotor_vstrut_pcb.kicad_sch")
    (property "Sheet name" "")
    (path "/e4993730-1dee-4842-857c-75d225e7ee51")
    (attr through_hole)
    (fp_text reference "J3" (at -6.2 -4.4 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bf3ab76f-6389-4254-9743-0040ae964c02)
    )
    (fp_text value "top" (at 0 1 180 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6aa0c56d-34fb-48a8-930d-358c8aa92445)
    )
    (fp_text user "${REF}" (at 0 2.5 180 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ae6b8039-3aa4-4076-be0b-ae884caf0069)
    )
    (fp_line (start 7.5 -0.8) (end -7.5 -0.8) (layer "Dwgs.User") (width 0.12) (tstamp d0b249db-9c9a-4b83-8e83-c32805bd8e3f))
    (fp_line (start -4 0.8) (end 4 0.8) (layer "Dwgs.User") (width 0.12) (tstamp d1088dfc-85e5-46d5-8c95-9a63dff10d65))
    (fp_rect (start -4 0) (end 4 4) (layer "Dwgs.User") (width 0.1) (tstamp 4000607d-3161-426e-93ae-cc5fbc992d5c))
    (fp_rect (start -7.5 0) (end 7.5 -5.6) (layer "Dwgs.User") (width 0.1) (tstamp 7dd3eafe-e381-4501-a0ad-7c18673bb740))
    (pad "1" smd rect (at -5 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 36 "Net-(J3-Pad1)") (tstamp 584adde3-d30b-4bfa-abbd-c1bed6e4a1ef))
    (pad "2" smd rect (at -2.5 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 35 "Net-(J3-Pad2)") (tstamp a2966944-5310-427d-94b8-a6fca23a4bf1))
    (pad "3" smd rect (at 0 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 34 "Net-(J3-Pad3)") (tstamp f9df9bad-6a49-49da-8ea7-1645ce98e495))
    (pad "4" smd rect (at 2.5 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 33 "Net-(J3-Pad4)") (tstamp 73299d82-22c3-4105-852d-1ac6cb25d43b))
    (pad "5" smd rect (at 5 -2 180) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 32 "Net-(J3-Pad5)") (tstamp 15714ea4-f85d-430a-834f-c6ccf6b7ec09))
    (pad "6" smd rect (at 5 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 11 "/tru_t1") (tstamp 51445257-c677-45f9-8be4-6030e791e86e))
    (pad "7" smd rect (at 2.5 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 12 "/tru_t2") (tstamp 65ee9957-49a9-47cb-b061-7cdcaf76fc04))
    (pad "8" smd rect (at 0 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 13 "/tru_t3") (tstamp bc0e02d3-9feb-4c51-847f-30a20a00c725))
    (pad "9" smd rect (at -2.5 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 14 "/tru_t4") (tstamp 94ebb14a-ab14-472c-a4c3-9a4cce7cdfb2))
    (pad "10" smd rect (at -5 -2 180) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 15 "/tru_t5") (tstamp e8682703-d907-4439-a521-f838f741e6d2))
    (pad "11" smd rect (at -2.5 2 180) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 31 "Net-(J3-Pad11)") (tstamp ba74fedf-8085-4fb4-ab01-17c59d3b3b51))
    (pad "12" smd rect (at 0 2 180) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 30 "Net-(J3-Pad12)") (tstamp f97e43f3-5c3b-4e54-9af6-3efcfcfae08a))
    (pad "13" smd rect (at 2.5 2 180) (size 1.8 3) (layers "F.Cu" "F.Mask")
      (net 29 "Net-(J3-Pad13)") (tstamp 2f5dccf2-441f-4a1c-af5c-a44a087d7d82))
    (pad "14" smd rect (at 2.5 2 180) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 12 "/tru_t2") (tstamp 37a7184d-d263-40cf-8c3f-6f8bea62ccf1))
    (pad "15" smd rect (at 0 2 180) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 13 "/tru_t3") (tstamp bbb7c5e3-b8c3-46ca-9827-259ffe689f25))
    (pad "16" smd rect (at -2.5 2 180) (size 1.8 3) (layers "B.Cu" "B.Mask")
      (net 14 "/tru_t4") (tstamp 76c9020b-9126-4304-86c1-c334aac74811))
  )

  (gr_poly (pts
 (xy 160 172.5)
    (xy 140 172.5)
    (xy 140 25)
    (xy 160 25)) (layer "Eco1.User") (width 0.1) (tstamp 724fb27a-5098-4877-ae90-10c30d528453))
  (gr_line (start 146 18.5) (end 154 18.5) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 21d71c90-1663-47f2-805a-3a10bb7166bc))
  (gr_line (start 142.5 182.1) (end 146 182.1) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 34598794-23ad-45c5-a437-a984c0ab605a))
  (gr_line (start 154 18.5) (end 154 22.1) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 3547d435-8af2-4e43-ac75-cfb0f21102eb))
  (gr_line (start 154 185.7) (end 154 182.1) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 46859f9b-c0d1-474a-81ee-c6cb0f0e6b07))
  (gr_line (start 154 22.1) (end 157.5 22.1) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 4afe9ac1-c888-479e-9d7c-4bd9ef77e5bc))
  (gr_line (start 142.5 22.1) (end 146 22.1) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 64700040-2cea-446b-bc85-56fef465dfc5))
  (gr_line (start 146 22.1) (end 146 18.5) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp 9d86c8d0-736f-4f12-b5ef-91d43c55d32d))
  (gr_line (start 157.5 22.1) (end 157.5 182.1) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp a09a27f2-0a64-40fc-9420-70679a00fdd7))
  (gr_line (start 142.5 182.1) (end 142.5 22.1) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp b7857ac5-fbd7-4184-9f11-5164268584b6))
  (gr_line (start 146 182.1) (end 146 185.7) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp c26f97c8-3016-4d2d-91c4-ddb9d3097177))
  (gr_line (start 146 185.7) (end 154 185.7) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp c97639af-a612-4ca5-b67b-dad9ca826124))
  (gr_line (start 154 182.1) (end 157.5 182.1) (angle 90) (layer "Edge.Cuts") (width 0.16) (tstamp fce75ced-948f-43b6-8181-f62b28ee81f7))
  (gr_text "Top End" (at 150 26.5) (layer "F.SilkS") (tstamp 80ac6bc5-2e8f-42de-871c-2dd9a2b3af69)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "This\nside\nfaces\noutside" (at 150 44) (layer "F.SilkS") (tstamp ed777d03-f811-4342-8095-4262cac0c291)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 9c6a1bb5-60ff-46ca-a879-30e77db23bc5)
    (pts (xy 157.365012 173.3) (xy 157.365012 181.3))
    (height -3.284988)
    (gr_text "8.0 mm" (at 161.8 177.3 270) (layer "Dwgs.User") (tstamp 9c6a1bb5-60ff-46ca-a879-30e77db23bc5)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 2) (units_format 1) (precision 1))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 145 180.1) (end 145 175.35) (width 1.2) (layer "B.Cu") (net 1) (tstamp 4ae7b818-bae2-4561-84c0-d7b4a6e0e2aa))
  (segment (start 147.5 175.35) (end 147.5 180.1) (width 1.2) (layer "B.Cu") (net 2) (tstamp 25757950-e323-4496-adef-afbb36bf9bf5))
  (segment (start 147.5 180.1) (end 147.5 184.1) (width 1.2) (layer "B.Cu") (net 2) (tstamp 8fc0ba2a-35ad-446e-82c1-ba1a3f2dcd8d))
  (segment (start 150 175.35) (end 150 175) (width 1.2) (layer "B.Cu") (net 3) (tstamp 3896094f-f341-41b1-bd92-493de9eb1922))
  (segment (start 150 180.1) (end 150 175.35) (width 1.2) (layer "B.Cu") (net 3) (tstamp 8e3f5549-b1f3-412d-93ac-9074ab43fc44))
  (segment (start 150 180.1) (end 150 184.1) (width 1.2) (layer "B.Cu") (net 3) (tstamp c417a5be-ee66-43d8-a7c3-cf02813cb449))
  (segment (start 152.5 184.1) (end 152.5 180.1) (width 1.2) (layer "B.Cu") (net 4) (tstamp 6fc9b570-aa2c-4e01-a266-8af95346bb3c))
  (segment (start 152.5 175.35) (end 152.5 180.1) (width 1.2) (layer "B.Cu") (net 4) (tstamp f8425aef-9dc3-471c-93f6-d9f59bb5837c))
  (segment (start 155 175.35) (end 155 180.1) (width 1.2) (layer "B.Cu") (net 5) (tstamp 44c391d7-0d35-46e6-94e4-9367dde0aca9))
  (segment (start 145 24.1) (end 145 171.35) (width 1.2) (layer "B.Cu") (net 11) (tstamp 9e73ea58-6be9-47f9-a377-e2a291bb84db))
  (segment (start 147.5 20.1) (end 147.5 24.1) (width 1.2) (layer "B.Cu") (net 12) (tstamp 41980f15-737f-4886-83a3-e7484f93dfd2))
  (segment (start 147.5 171.35) (end 147.5 24.1) (width 1.2) (layer "B.Cu") (net 12) (tstamp 75d0f23c-dde4-42d1-9e04-2f634eba3124))
  (segment (start 150 24.1) (end 150 171.35) (width 1.2) (layer "B.Cu") (net 13) (tstamp 0daaf576-fd6e-44a2-bfcc-2f9a922165f5))
  (segment (start 150 20.1) (end 150 24.1) (width 1.2) (layer "B.Cu") (net 13) (tstamp dd92033e-b9bb-414f-b484-42691ad5fcc8))
  (segment (start 152.5 171.35) (end 152.5 24.1) (width 1.2) (layer "B.Cu") (net 14) (tstamp 6633d749-02a7-4188-aca3-9ccd0af54fd5))
  (segment (start 152.5 20.1) (end 152.5 24.1) (width 1.2) (layer "B.Cu") (net 14) (tstamp cb30446d-82f6-471a-ac35-70af7efbf489))
  (segment (start 155 24.1) (end 155 171.35) (width 1.2) (layer "B.Cu") (net 15) (tstamp 98f58298-4fe8-4a38-8351-8c2e74b14a80))

)
