EESchema-DOCLIB  Version 2.0
#
$CMP Rotary_Encoder_Switch_with_gnd
D Rotary encoder, dual channel, incremental quadrate outputs, with switch
K rotary switch encoder switch push button
F ~
$ENDCMP
#
#End Doc Library
