(module Würth_WR-WST_debug_490107671212_2x06_P2.54mm_Vertical (layer F.Cu) (tedit 64A6A11B)
  (descr "Würth WR-WST series direct-to-board connector footprint, debug application tolerances, MPN 490107671212 https://www.we-online.com/components/products/datasheet/490107671212.pdf Generated with kicad-footprint-generator.")
  (tags "connector Würth WR-WST_debug vertical")
  (attr exclude_from_bom)
  (fp_text reference REF** (at 0 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Würth_WR-WST_debug_490107671212_2x06_P2.54mm_Vertical (at 0 4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -11.415 -2.8) (end -11.415 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -11.415 2.8) (end 11.415 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start 11.415 2.8) (end 11.415 -2.8) (layer F.Fab) (width 0.1))
  (fp_line (start 11.415 -2.8) (end -11.415 -2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -7.735 2.8) (end -6.985 1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -6.985 1.3) (end -6.235 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -11.415 -2.8) (end -11.415 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.415 2.8) (end 11.415 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.415 2.8) (end 11.415 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.415 -2.8) (end -11.415 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.335 2.8) (end -9.585 1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.585 1.3) (end -8.835 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.335 -2.8) (end -10.335 -2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.335 -2.4) (end -8.835 -2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -8.835 -2.4) (end -8.835 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.435 2.8) (end 8.435 2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.435 2.4) (end 9.935 2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.935 2.4) (end 9.935 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.915 -3.3) (end -11.915 3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -11.915 3.3) (end 11.915 3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.915 3.3) (end 11.915 -3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.915 -3.3) (end -11.915 -3.3) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at -6.985 1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -5.715 -1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -4.445 1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -3.175 -1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -1.905 1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -0.635 -1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0.635 1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 1.905 -1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 3.175 1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 4.445 -1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 5.715 1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 6.985 -1.27) (size 1.85 1.85) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -8.215 -1.27) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 8.215 1.27) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  (fp_text user ${REFERENCE} (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
)
