(footprint "MTSM1346SMF1-100" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "REF**" (at 0 -3.5 0 unlocked) (layer "F.SilkS") (tstamp 94844c15-568c-4fa3-a607-69040e661d97)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "MTSM1346SMF1-100" (at 0 1 0 unlocked) (layer "F.Fab") (tstamp 6f1aa1c0-3c66-4205-b8f1-1964440b2a97)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp ecc39ab9-7bd3-435c-9592-2ed9167c0029)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 03e564f4-0f2c-4b49-b752-e767cfcf778d)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 1f41df07-2728-4aae-9b94-3e28ebeaefd7)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_line (start -0.25 0.6) (end -0.25 1.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 6600c07a-dc8f-4f4f-b698-4b36f01b7898))
  (fp_line (start 0 0.6) (end -0.25 0.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 4acbf4c6-6d04-4e48-9b42-e9363a7f99e3))
  (fp_line (start 1.45 0.6) (end 0 0.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 9b89d808-0216-4d0e-8369-486f19e4828a))
  (fp_rect (start -1.5 -1.5) (end 1.5 1.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 8b2f86fb-d332-4688-a68e-d12000493540))
  (fp_rect (start -1.7 -1.7) (end 1.7 1.7)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 9780c955-5324-4f3a-a757-bafd450ff138))
  (fp_text user "${REFERENCE}" (at 0 2.5 0 unlocked) (layer "F.Fab") (tstamp 76ae142d-c1dd-4fd1-8324-8892d6724e8e)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd roundrect (at 1.25 1.15 180) (size 2.5 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4285714286)
    (thermal_bridge_angle 45)
    (tstamp 5314e829-2a31-47d2-8c38-725917263cbc)
  )
  (pad "2" smd rect (at 1.575 0 180) (size 1.85 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 1c32838c-a5f9-4403-9438-b3afde00faf9)
  )
  (pad "3" smd rect (at 1.575 -1.15 180) (size 1.85 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp f247bdbc-b440-4a5e-a621-e4c358d98147)
  )
  (pad "4" smd rect (at -1.575 -1.15 180) (size 1.85 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 522d816f-4c10-4df4-86fb-7a69840d426c)
  )
  (pad "5" smd rect (at -1.575 0 180) (size 1.85 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp d971adf6-52b5-4d64-a89a-8e23528e6ba5)
  )
  (pad "6" smd rect (at -1.575 1.15 180) (size 1.85 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 68ce1124-7c10-40b9-b5ba-823548e5189c)
  )
)
