(module Würth_WR-WST_permanent_490107670412_2x02_P2.54mm_Vertical (layer F.Cu) (tedit 64A6A11B)
  (descr "Würth WR-WST series direct-to-board connector footprint, permanent application tolerances, MPN 490107670412 https://www.we-online.com/components/products/datasheet/490107670412.pdf Generated with kicad-footprint-generator.")
  (tags "connector Würth WR-WST_permanent vertical")
  (attr exclude_from_bom)
  (fp_text reference REF** (at 0 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Würth_WR-WST_permanent_490107670412_2x02_P2.54mm_Vertical (at 0 4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6.335 -2.8) (end -6.335 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -6.335 2.8) (end 6.335 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start 6.335 2.8) (end 6.335 -2.8) (layer F.Fab) (width 0.1))
  (fp_line (start 6.335 -2.8) (end -6.335 -2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -2.655 2.8) (end -1.905 1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -1.905 1.3) (end -1.155 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -6.335 -2.8) (end -6.335 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.335 2.8) (end 6.335 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.335 2.8) (end 6.335 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.335 -2.8) (end -6.335 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.155 2.8) (end -4.405 1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.405 1.3) (end -3.655 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.155 -2.8) (end -5.155 -2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.155 -2.4) (end -3.655 -2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.655 -2.4) (end -3.655 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.255 2.8) (end 3.255 2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.255 2.4) (end 4.755 2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.755 2.4) (end 4.755 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.835 -3.3) (end -6.835 3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.835 3.3) (end 6.835 3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.835 3.3) (end 6.835 -3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.835 -3.3) (end -6.835 -3.3) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at -1.905 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -0.635 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0.635 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 1.905 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -3.235 -1.27) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 3.235 1.27) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  (fp_text user ${REFERENCE} (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
)
