(footprint "bal-10x10mm" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "REF**" (at 0 -0.5 0 unlocked) (layer "F.SilkS") (tstamp de0f3d4f-0548-4afe-b757-b007f83a9e35)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "bal-10x10mm" (at 0 1 0 unlocked) (layer "F.Fab") (tstamp 94288aec-ce17-4e59-976e-5bed69e3739d)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 18e72dd5-2a40-41d0-80e6-e822e387c67d)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 81b3448f-0b7a-44d9-bd6d-a2750652caea)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 52617972-8d1c-497f-9a3d-12806d7165c1)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_rect (start -5 -5) (end 5 5)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 80d6ffe1-35d8-42e6-a99c-61c162456205))
  (fp_text user "${REFERENCE}" (at 0 2.5 0 unlocked) (layer "F.Fab") (tstamp 1dd43b51-1b85-4dbe-a3d5-14a2b02cedd6)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd circle (at 0 0) (size 10 10) (layers "F.Cu")
    (tstamp fd751de0-95ad-4daa-b946-9bc8a04d145a)
  )
  (pad "1" smd circle (at 0 0) (size 10 10) (layers "B.Cu")
    (tstamp 3c838a9d-3381-4b97-808d-b167edae1cfd)
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 0a2147b6-82c0-4257-a804-2263f1f662b4) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -5.25 -5.25)
        (xy 5.25 -5.25)
        (xy 5.25 5.25)
        (xy -5.25 5.25)
      )
    )
  )
)
