(footprint "mesh_conn" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (tags "net tie")
  (property "Reference" "REF**" (at 0 -2.25 0 unlocked) (layer "F.SilkS") hide (tstamp ad4f86a6-c40a-45de-9755-536816782561)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "mesh_conn" (at 0 1 0 unlocked) (layer "F.Fab") (tstamp e87da325-b358-40c2-9a7c-2bf2cb54bc3f)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 1a4151b5-9c45-483f-b7de-b3c48b0e0373)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 3a2afd89-4c34-4a0b-a3cc-24800fe97f31)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 5f1f1696-4799-4134-b64d-57be44267fde)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (net_tie_pad_groups "1, 4" "2, 3")
  (fp_poly
    (pts
      (xy -0.3 -0.525)
      (xy 0 -0.525)
      (xy 0 -0.375)
      (xy -0.3 -0.375)
    )
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 4df75b5b-7d40-4fbf-948b-f4bab6464fa9))
  (fp_poly
    (pts
      (xy -0.3 -0.225)
      (xy 0 -0.225)
      (xy 0 -0.075)
      (xy -0.3 -0.075)
    )
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 3377e9c2-d160-46a6-a717-63303eedeab7))
  (fp_poly
    (pts
      (xy -0.3 0.075)
      (xy 0 0.075)
      (xy 0 0.225)
      (xy -0.3 0.225)
    )
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 1b67dc42-1568-4a22-9736-0633ba3f1bd2))
  (fp_poly
    (pts
      (xy -0.3 0.375)
      (xy 0 0.375)
      (xy 0 0.525)
      (xy -0.3 0.525)
    )
    (stroke (width 0) (type solid)) (fill solid) (layer "F.Cu") (tstamp 66677be7-ab6c-42a1-a282-6cba00f68bff))
  (fp_text user "${REFERENCE}" (at 0 2.5 0 unlocked) (layer "F.Fab") (tstamp f741b3b8-fc10-442d-8f89-4dd2860f992f)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd circle (at -0.3 -0.45) (size 0.15 0.15) (layers "F.Cu")
    (tstamp fd3bbd8d-91d1-4664-b510-7ed188beee18)
  )
  (pad "2" smd circle (at -0.3 -0.15) (size 0.15 0.15) (layers "F.Cu")
    (tstamp 5171ea77-1c63-4ab6-8d5f-14c6eab087a8)
  )
  (pad "3" smd circle (at -0.3 0.15) (size 0.15 0.15) (layers "F.Cu")
    (tstamp 80b9cf1e-76d6-499a-8d4a-c27e4b29a23a)
  )
  (pad "4" smd circle (at -0.3 0.45) (size 0.15 0.15) (layers "F.Cu")
    (tstamp 6911242a-667c-4407-8e79-6ac9c5f4704c)
  )
  (pad "5" smd circle (at 0 -0.45) (size 0.15 0.15) (layers "F.Cu")
    (tstamp e65c026b-a582-481d-aa0f-83da4e05e52b)
  )
  (pad "5" smd circle (at 0 0.45 180) (size 0.15 0.15) (layers "F.Cu")
    (tstamp 9f47f11e-8f4c-46ef-a9fd-7e92635a649c)
  )
  (pad "6" smd circle (at 0 -0.15) (size 0.15 0.15) (layers "F.Cu")
    (tstamp 4adac25c-6de4-4cdf-b81d-79aadd631463)
  )
  (pad "6" smd circle (at 0 0.15 180) (size 0.15 0.15) (layers "F.Cu")
    (tstamp e67e9afa-18ce-4ca6-b663-6d33c75027af)
  )
)
