(module Würth_WR-WST_permanent_490107671612_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 64A6A11B)
  (descr "Würth WR-WST series direct-to-board connector footprint, permanent application tolerances, MPN 490107671612 https://www.we-online.com/components/products/datasheet/490107671612.pdf Generated with kicad-footprint-generator.")
  (tags "connector Würth WR-WST_permanent vertical")
  (attr exclude_from_bom)
  (fp_text reference REF** (at 0 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Würth_WR-WST_permanent_490107671612_2x08_P2.54mm_Vertical (at 0 4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -13.955 -2.8) (end -13.955 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -13.955 2.8) (end 13.955 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start 13.955 2.8) (end 13.955 -2.8) (layer F.Fab) (width 0.1))
  (fp_line (start 13.955 -2.8) (end -13.955 -2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -10.275 2.8) (end -9.525 1.3) (layer F.Fab) (width 0.1))
  (fp_line (start -9.525 1.3) (end -8.775 2.8) (layer F.Fab) (width 0.1))
  (fp_line (start -13.955 -2.8) (end -13.955 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -13.955 2.8) (end 13.955 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.955 2.8) (end 13.955 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 13.955 -2.8) (end -13.955 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -12.775 2.8) (end -12.025 1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -12.025 1.3) (end -11.275 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -12.775 -2.8) (end -12.775 -2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -12.775 -2.4) (end -11.275 -2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.275 -2.4) (end -11.275 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.875 2.8) (end 10.875 2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.875 2.4) (end 12.375 2.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.375 2.4) (end 12.375 2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -14.455 -3.3) (end -14.455 3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -14.455 3.3) (end 14.455 3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.455 3.3) (end 14.455 -3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.455 -3.3) (end -14.455 -3.3) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole circle (at -9.525 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -8.255 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -6.985 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -5.715 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -4.445 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -3.175 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -1.905 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -0.635 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 0.635 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 1.905 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 3.175 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 4.445 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 5.715 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 6.985 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 8.255 1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 9.525 -1.27) (size 1.75 1.75) (drill 1.4) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -10.855 -1.27) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 10.855 1.27) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  (fp_text user ${REFERENCE} (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
)
