(footprint "Bosch_BMI088_LGA" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "REF**" (at 0 14.5 0 unlocked) (layer "F.SilkS") (tstamp f97a3efe-8e1f-4684-abec-f09b41d0273a)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "Bosch_BMI088_LGA" (at 0 16 0 unlocked) (layer "F.Fab") (tstamp 507ecc84-52fd-413f-bbd7-488e6a6774d5)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 15 0 unlocked) (layer "F.Fab") hide (tstamp 86a561ab-f459-4896-a3fb-deffc38169af)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 15 0 unlocked) (layer "F.Fab") hide (tstamp 47e3ecba-bfc7-4cb8-aee6-a0c58e0d8f6c)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 15 0 unlocked) (layer "F.Fab") hide (tstamp 61b1f77d-fee5-4715-aefa-934b7eb8bf2d)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_rect (start -1.5 -2.25) (end 1.5 2.25)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp d4da083c-48cd-45d8-85d2-7ba5414f92c2))
  (fp_rect (start -1.75 -2.5) (end 1.75 2.5)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp d9afc9e9-a34c-49a9-a1ee-a81aa2657292))
  (fp_text user "${REFERENCE}" (at 0 17.5 0 unlocked) (layer "F.Fab") (tstamp 05e60479-6332-49f4-8e05-9851167efb3f)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd rect (at 1.2625 -1.5) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 33e4075d-571a-440f-beb1-39b5fc17748f)
  )
  (pad "2" smd rect (at 1.2625 -1) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 445ee1e7-5125-4727-854a-238f96f6239c)
  )
  (pad "3" smd rect (at 1.2625 -0.5) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 2d4aee6a-bfa1-47b5-931c-d1e9a1e75a32)
  )
  (pad "4" smd rect (at 1.2625 0) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 095909e0-1173-47ef-8f60-91851bef766c)
  )
  (pad "5" smd rect (at 1.2625 0.5) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp c889a00c-1efd-42a7-9620-07b6e1ad38ad)
  )
  (pad "6" smd rect (at 1.2625 1) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp fd785a6e-a6e4-479e-a743-9436638169b2)
  )
  (pad "7" smd rect (at 1.2625 1.5) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 98826b32-2175-45f7-a2e9-f123abbc8058)
  )
  (pad "8" smd rect (at 0 2.0125 90) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 649df130-2925-4aa0-9c17-b33575023cb7)
  )
  (pad "9" smd rect (at -1.2625 1.5) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp a3b62a16-22dc-4c87-a4b5-a7392f718405)
  )
  (pad "10" smd rect (at -1.2625 1) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 5a8497c5-7b36-4416-969b-523e2ad81294)
  )
  (pad "11" smd rect (at -1.2625 0.5) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 8976fc4d-827c-4ce9-ba98-c3392b3fded9)
  )
  (pad "12" smd rect (at -1.2625 0) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp b589d726-1f22-4583-b98c-ead3ecd8bf5f)
  )
  (pad "13" smd rect (at -1.2625 -0.5) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp ee32064b-3874-4d43-abf6-1ad170bfec82)
  )
  (pad "14" smd rect (at -1.2625 -1) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp dd51ecf0-f3c8-4742-8fb4-d2754cab1b14)
  )
  (pad "15" smd rect (at -1.2625 -1.5) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 98c84001-0cd6-4ab7-83e0-c351f3810a71)
  )
  (pad "16" smd rect (at 0 -2.0125 90) (size 0.675 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 1560c8a5-30bb-4783-b4a2-a69f1b22772d)
  )
)
