(footprint "USB-C 16Pin" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "J1" (at 0 1.5 180) (layer "F.SilkS") hide (tstamp eb2ebd2d-6a4e-46e3-ac8d-113c7e659e6f)
    (effects (font (size 0.45 0.45) (thickness 0.1125)))
  )
  (property "Value" "USB-c" (at 0 8.5 180) (layer "F.Fab") (tstamp ce2771fe-fbe3-4145-9ee0-e5ed9062e8b5)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp dfecbaa1-0d91-4435-b69b-6f4569e14f57)
    (effects (font (size 1.27 1.27)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp ff8bcdaf-da28-494f-97a9-2c66a8ae8d73)
    (effects (font (size 1.27 1.27)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 9a44db41-1e76-46aa-af17-509ea5b901a2)
    (effects (font (size 1.27 1.27)))
  )
  (attr through_hole)
  (fp_line (start -4.5 -0.5) (end -4 -0.5)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 81616b7e-c958-40a9-bab7-2c4407dc57bd))
  (fp_line (start -4.5 2) (end -4.5 4)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 1fb284a3-69c6-4c77-9727-61d4c95f4bf6))
  (fp_line (start -4.5 7.695) (end -4.5 6)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp e1b3a79a-9126-4f6e-a926-46486ce5c76d))
  (fp_line (start 4 -0.5) (end 4.5 -0.5)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 36601b65-ac65-4081-8a78-b712a8f227a6))
  (fp_line (start 4.5 4) (end 4.5 2)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 6d87da2f-0c03-4453-9608-d312078b4229))
  (fp_line (start 4.5 6) (end 4.5 7.695)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 4509a6e6-6429-446d-b86f-19c38a7fd203))
  (fp_line (start 4.5 7.695) (end -4.5 7.695)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 961e1aab-b3d8-4fb1-a635-9511c747b96c))
  (pad "" np_thru_hole circle (at -2.89 1.445) (size 0.65 0.65) (drill 0.65) (layers "*.Cu" "*.Mask")
    (tstamp e11ee38c-a7a7-4d1d-ad35-813467bc4fc7)
  )
  (pad "" np_thru_hole circle (at 2.89 1.445) (size 0.65 0.65) (drill 0.65) (layers "*.Cu" "*.Mask")
    (tstamp 30590349-81ff-40cf-bc51-e8f231481f3b)
  )
  (pad "A1" smd rect (at -3.2 0) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp 3efaa601-d1f7-438c-8238-f2ec20b4a02b)
  )
  (pad "A4" smd rect (at -2.4 0) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp c9c39476-0750-46c7-b6d3-d53473a0ef57)
  )
  (pad "A5" smd rect (at -1.25 0) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp 2cd75207-e911-4108-a715-6c23640b8c5a)
  )
  (pad "A6" smd rect (at -0.25 0) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp f852be3a-bf5e-4e7f-88f7-cae46347915a)
  )
  (pad "A7" smd rect (at 0.25 0) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp 109c7206-2743-4a6a-b2e1-e86b968fb143)
  )
  (pad "A8" smd rect (at 1.25 0) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp be05e9a3-e48d-4db4-8bb4-e68c4416fdab)
  )
  (pad "B1" smd rect (at 3.2 0) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp 87fad174-e2e2-4f1b-bea4-4231861cab62)
  )
  (pad "B4" smd rect (at 2.4 0) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp 4cb84203-3512-476c-90f1-4ce88e70492a)
  )
  (pad "B5" smd rect (at 1.75 0) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp 16a38fff-033c-4c29-82ee-d40bde9505fd)
  )
  (pad "B6" smd rect (at 0.75 0) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp 3b3d027c-23cf-40fb-b1ba-88d797619795)
  )
  (pad "B7" smd rect (at -0.75 0) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp acc5c908-c2ed-4e15-9882-f6a26b1fe29c)
  )
  (pad "B8" smd rect (at -1.75 0) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
    (tstamp 303243d5-fa42-46ae-b8a3-c004b1a76cbb)
  )
  (pad "S1" thru_hole oval (at -4.32 0.915) (size 1 2.1) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask")
    (tstamp 8f3654bc-4a83-49d9-8dc1-86d69a7a0638)
  )
  (pad "S1" thru_hole oval (at -4.32 5.095) (size 1 1.8) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
    (tstamp 641945ce-6818-498f-a758-da78b8299096)
  )
  (pad "S1" thru_hole oval (at 4.32 0.915) (size 1 2.1) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask")
    (tstamp 034e8501-2614-40d0-976a-9aaa881a6bda)
  )
  (pad "S1" thru_hole oval (at 4.32 5.095) (size 1 1.8) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
    (tstamp d3d4a3a3-7726-4f02-9b98-ad15dc4207e2)
  )
)
