(footprint "VBPW34SR" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "REF**" (at -1.6 -3 0 unlocked) (layer "F.SilkS") hide (tstamp a34d9215-775d-49f5-bf54-a8f43cd11775)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "VBPW34SR" (at 0 1 0 unlocked) (layer "F.Fab") (tstamp df6d4281-95bc-4ab8-a5da-a094a9921443)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp cde3aafd-9017-41d4-a0e8-0ebb4e11c23c)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 8bd66a9e-602b-4ca1-b4f6-2287088b5576)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 05ad87a2-2727-4cf9-8632-0a7c9280069f)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_line (start -1.6 -1.95) (end -1.6 1.95)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 4d6db9fa-ea01-45b1-badf-e89665394484))
  (fp_rect (start -2.2 -1.95) (end 2.2 1.95)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 9ea9edc8-5a95-4141-a023-865ddb73ecde))
  (fp_rect (start -1.68 -1.5) (end 1.32 1.5)
    (stroke (width 0.1) (type dot)) (fill none) (layer "F.SilkS") (tstamp 7833047e-6f3c-42c0-a2f2-09ac045669eb))
  (fp_rect (start -1.98 -1.8) (end 1.62 1.8)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp b4065235-60ce-44d5-86a8-bee6d6cc2972))
  (fp_rect (start -3.4 -2.2) (end 3.4 2.2)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 63ca6ccd-594f-442a-9477-3ba2bb12a625))
  (fp_text user "${REFERENCE}" (at 0 2.5 0 unlocked) (layer "F.Fab") (tstamp dd2b9e0d-6b5a-41aa-a5c4-160756cdc99f)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd rect (at -3.575 0 90) (size 1.75 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp cf045b39-6595-45d3-872b-24b8a472f1a1)
  )
  (pad "2" smd rect (at 3.575 0 90) (size 1.75 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 5f01b4f6-87fe-4d51-9b5e-70d6b6bcbd75)
  )
)
