(module solder_jumper_2pin (layer F.Cu) (tedit 5B38A791)
  (fp_text reference REF** (at 0 1.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value solder_jumper_2pin (at 0 -0.5) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -0.9) (end 0 0.9) (layer F.Mask) (width 0.5))
  (pad 1 smd trapezoid (at -0.7 0 90) (size 1.5 1) (rect_delta 0 0.6 ) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd trapezoid (at 0.7 0 270) (size 1.5 1) (rect_delta 0 0.6 ) (layers F.Cu F.Paste F.Mask))
)
