(footprint "Sinhoo_SMDSO30XX_SMD_Nut_M3" (version 20230913) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "REF**" (at 0 -4.6 0 unlocked) (layer "F.SilkS") hide (tstamp 2c5f6fe3-1b4b-4bc3-93bc-e1fb7760bab4)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "Sinhoo_SMDSO30XX_SMD_Nut_M3" (at 0 1 0 unlocked) (layer "F.Fab") (tstamp 57189eb9-9001-4fa9-b702-2fa66b4e4620)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 6968169e-ed18-4adb-b4f1-3f90bc093712)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp ac79ecda-1dbf-47ba-9f13-f8010c4e0e39)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 82bcafb6-8fe9-4c71-84ed-e007b98ce46f)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_text user "${REFERENCE}" (at 0 2.5 0 unlocked) (layer "F.Fab") (tstamp 4f68887e-84de-4f95-978b-4114f1210ce0)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" thru_hole circle (at 0 0) (size 7.5 7.5) (drill 4.22) (layers "*.Cu" "F.Paste" "F.Mask")
    (tstamp 21b433bb-2b1e-41ae-b5f0-097d7d1375f4)
  )
)
