(export (version D)
  (design
    (source /home/user/toys/led_tape_display/driver/driver.sch)
    (date "Thu Jan 31 10:32:29 2019")
    (tool "Eeschema (5.0.1)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source driver.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R28)
      (value "5mR 1W 2512")
      (footprint Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3D5DD5))
    (comp (ref R29)
      (value "5mR 1W")
      (footprint Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3D5E81))
    (comp (ref R30)
      (value "5mR 1W")
      (footprint Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3D5FC2))
    (comp (ref R31)
      (value "5mR 1W")
      (footprint Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3D600E))
    (comp (ref R32)
      (value "5mR 1W")
      (footprint Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3D603D))
    (comp (ref U7)
      (value INA226)
      (footprint Package_SO:MSOP-10_3x3mm_P0.5mm)
      (datasheet http://www.ti.com/lit/ds/symlink/ina226.pdf)
      (libsource (lib Analog_ADC) (part INA226) (description "High-Side or Low-Side Measurement, Bi-Directional Current and Power Monitor (0-36V) with I2C Compatible Interface, MSOP-10"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3D6130))
    (comp (ref Q3)
      (value TPHR6503PL)
      (footprint "footprints:Toshiba SOP Advance")
      (datasheet https://www.infineon.com/dgdl/Infineon-IRF7480M-DS-v01_02-EN.pdf?fileId=5546d462533600a4015355ff8fa41c30)
      (libsource (lib Transistor_FET) (part IRF7480M) (description "330A Id, 40V Vds, 1.2mOhm Rds, N-Channel MOSFET, DirectFET ME"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3D9DBF))
    (comp (ref Q1)
      (value TPHR6503PL)
      (footprint "footprints:Toshiba SOP Advance")
      (datasheet https://www.infineon.com/dgdl/Infineon-IRF7480M-DS-v01_02-EN.pdf?fileId=5546d462533600a4015355ff8fa41c30)
      (libsource (lib Transistor_FET) (part IRF7480M) (description "330A Id, 40V Vds, 1.2mOhm Rds, N-Channel MOSFET, DirectFET ME"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3DA5D0))
    (comp (ref Q2)
      (value TPHR6503PL)
      (footprint "footprints:Toshiba SOP Advance")
      (datasheet https://www.infineon.com/dgdl/Infineon-IRF7480M-DS-v01_02-EN.pdf?fileId=5546d462533600a4015355ff8fa41c30)
      (libsource (lib Transistor_FET) (part IRF7480M) (description "330A Id, 40V Vds, 1.2mOhm Rds, N-Channel MOSFET, DirectFET ME"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3DAAC4))
    (comp (ref Q4)
      (value TPHR6503PL)
      (footprint "footprints:Toshiba SOP Advance")
      (datasheet https://www.infineon.com/dgdl/Infineon-IRF7480M-DS-v01_02-EN.pdf?fileId=5546d462533600a4015355ff8fa41c30)
      (libsource (lib Transistor_FET) (part IRF7480M) (description "330A Id, 40V Vds, 1.2mOhm Rds, N-Channel MOSFET, DirectFET ME"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3DB5E6))
    (comp (ref R19)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3DB9A3))
    (comp (ref R21)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C405205))
    (comp (ref U4)
      (value TC4427)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib components) (part TC4427) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C406E47))
    (comp (ref C25)
      (value 0)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C40F6B4))
    (comp (ref C27)
      (value 0)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C40F928))
    (comp (ref R20)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C41E378))
    (comp (ref R22)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C41E39D))
    (comp (ref U5)
      (value TC4427)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (libsource (lib components) (part TC4427) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C41E3A6))
    (comp (ref C26)
      (value 0)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C41E3B0))
    (comp (ref C28)
      (value 0)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C41E3B6))
    (comp (ref U3)
      (value AMS1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.advanced-monolithic.com/pdf/ds1117.pdf)
      (libsource (lib Regulator_Linear) (part AMS1117-3.3) (description "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C45B743))
    (comp (ref C17)
      (value 1u)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C460459))
    (comp (ref C16)
      (value 1u)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C46605E))
    (comp (ref C15)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C46BEDF))
    (comp (ref R7)
      (value "10R .5W")
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C47C915))
    (comp (ref C19)
      (value 470u)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48FE5D))
    (comp (ref C18)
      (value 10u)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C49E930))
    (comp (ref U1)
      (value MT3608)
      (footprint Package_TO_SOT_SMD:SOT-23-6_Handsoldering)
      (libsource (lib components) (part MT3608) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3DB03B))
    (comp (ref L1)
      (value 10u)
      (footprint Inductor_SMD:L_Taiyo-Yuden_NR-50xx_HandSoldering)
      (libsource (lib components) (part L_EU_small) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3E1491))
    (comp (ref D1)
      (value "2A schottky")
      (footprint Diode_SMD:D_SMB_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky_Small_ALT) (description "Schottky diode, small symbol, filled shape"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3F3E87))
    (comp (ref C1)
      (value 10u)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3F99AD))
    (comp (ref C2)
      (value 470u)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3FB1E5))
    (comp (ref R2)
      (value 100k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C40F95F))
    (comp (ref R4)
      (value 3k3)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C417AAA))
    (comp (ref R3)
      (value 47k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C45B966))
    (comp (ref R5)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C45D762))
    (comp (ref C5)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48B1CF))
    (comp (ref R8)
      (value 47k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4AAEC7))
    (comp (ref R9)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4AAECD))
    (comp (ref C21)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4AAEDB))
    (comp (ref C3)
      (value 470u)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4E826F))
    (comp (ref C4)
      (value 10u)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4E8B95))
    (comp (ref R1)
      (value "10R .5W")
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C503EA9))
    (comp (ref C11)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5BBF20))
    (comp (ref C12)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5BD76D))
    (comp (ref C13)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5C8D7A))
    (comp (ref C14)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5C9980))
    (comp (ref C29)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5F270F))
    (comp (ref C24)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C60D685))
    (comp (ref C23)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C61DEFC))
    (comp (ref Y1)
      (value 8MHz)
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part Crystal_GND24) (description "Four pin crystal, GND on pins 2 and 4"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C62F3E9))
    (comp (ref C22)
      (value 12p)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6343C3))
    (comp (ref C20)
      (value 12p)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C645E08))
    (comp (ref R10)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6C27C5))
    (comp (ref U10)
      (value PC817)
      (footprint Package_DIP:DIP-4_W7.62mm)
      (datasheet http://www.soselectronic.cz/a_info/resource/d/pc817.pdf)
      (libsource (lib Isolator) (part PC817) (description "DC Optocoupler, Vce 35V, CTR 50-300%, DIP4"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C90990C))
    (comp (ref R39)
      (value 680)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C90D04A))
    (comp (ref U9)
      (value PC817)
      (footprint Package_DIP:DIP-4_W7.62mm)
      (datasheet http://www.soselectronic.cz/a_info/resource/d/pc817.pdf)
      (libsource (lib Isolator) (part PC817) (description "DC Optocoupler, Vce 35V, CTR 50-300%, DIP4"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C912594))
    (comp (ref R36)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C991BA6))
    (comp (ref R33)
      (value 390)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9F015A))
    (comp (ref R35)
      (value 390)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA7557C))
    (comp (ref R34)
      (value 720)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA78FA9))
    (comp (ref J6)
      (value "1602 I2C LCD")
      (footprint Connectors_Molex:Molex_KK-6410-04_04x2.54mm_Straight)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDBF041))
    (comp (ref R26)
      (value 1k5)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE0D5AA))
    (comp (ref R27)
      (value 1k5)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE10E6A))
    (comp (ref D4)
      (value cyan)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part LED_Small_ALT) (description "Light emitting diode, small symbol, filled shape"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D120495))
    (comp (ref D5)
      (value cyan)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part LED_Small_ALT) (description "Light emitting diode, small symbol, filled shape"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D120F6F))
    (comp (ref D6)
      (value pink)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part LED_Small_ALT) (description "Light emitting diode, small symbol, filled shape"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D12221B))
    (comp (ref D7)
      (value pink)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part LED_Small_ALT) (description "Light emitting diode, small symbol, filled shape"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D12562A))
    (comp (ref R13)
      (value 150)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D18F534))
    (comp (ref R14)
      (value 150)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D18F810))
    (comp (ref R15)
      (value 150)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D190038))
    (comp (ref R16)
      (value 150)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D1904ED))
    (comp (ref U8)
      (value MCP9804_MSOP)
      (footprint Package_SO:MSOP-8_3x3mm_P0.65mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/22203b.pdf)
      (libsource (lib Sensor_Temperature) (part MCP9804_MSOP) (description "Microchip Technology Digital Temperature Sensor MSOP"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D7751AD))
    (comp (ref J7)
      (value IN_VCC)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-3-5.08_1x03_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x03) (description "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C557B2A))
    (comp (ref J8)
      (value IN_GND)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-3-5.08_1x03_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x03) (description "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C558772))
    (comp (ref J2)
      (value OUT_B)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-3-5.08_1x03_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x03) (description "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D9205))
    (comp (ref J1)
      (value OUT_A)
      (footprint TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-3-5.08_1x03_P5.08mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x03) (description "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5DA183))
    (comp (ref H1)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68E1B2))
    (comp (ref H2)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C68F0B2))
    (comp (ref H3)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6913F3))
    (comp (ref H4)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6916D1))
    (comp (ref J9)
      (value SWD)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA7AF20))
    (comp (ref J10)
      (value FAN)
      (footprint Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C533914))
    (comp (ref U13)
      (value MAX485E)
      (footprint Package_SO:SO-8_5.3x6.2mm_P1.27mm)
      (datasheet https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf)
      (libsource (lib Interface_UART) (part MAX485E) (description "Half duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate, no low-power shutdown, with receiver/driver enable, 32 receiver drive kapacitity, DIP-8 and SOIC-8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C607F28))
    (comp (ref J5)
      (value RJ45_LED_Shielded)
      (footprint Connector_RJ:RJ45_Amphenol_RJHSE538X)
      (datasheet ~)
      (libsource (lib Connector) (part RJ45_LED_Shielded) (description "RJ connector, 8P8C (8 positions 8 connected), two LEDs, Shielded"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63EC4A))
    (comp (ref U11)
      (value AMS1117-5.0)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.advanced-monolithic.com/pdf/ds1117.pdf)
      (libsource (lib Regulator_Linear) (part AMS1117-3.3) (description "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8A447A))
    (comp (ref C8)
      (value 22u)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.00mm)
      (datasheet ~)
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8A4489))
    (comp (ref C7)
      (value 10u)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8A4492))
    (comp (ref C6)
      (value 100n)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA4A962))
    (comp (ref U12)
      (value PC817)
      (footprint Package_DIP:DIP-4_W7.62mm)
      (datasheet http://www.soselectronic.cz/a_info/resource/d/pc817.pdf)
      (libsource (lib Isolator) (part PC817) (description "DC Optocoupler, Vce 35V, CTR 50-300%, DIP4"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB95EB7))
    (comp (ref R18)
      (value 390)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC27782))
    (comp (ref R23)
      (value 720)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC2B8EF))
    (comp (ref U6)
      (value STM32F030F4Px)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (datasheet http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00088500.pdf)
      (libsource (lib MCU_ST_STM32F0) (part STM32F030F4Px) (description "ARM Cortex-M0 MCU, 16KB flash, 4KB RAM, 48MHz, 2.4-3.6V, 15 GPIO, TSSOP-20"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D52BF88))
    (comp (ref U2)
      (value 74HC595)
      (footprint Package_SO:SOIC-16_3.9x9.9mm_P1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/sn74hc595.pdf)
      (libsource (lib 74xx) (part 74HC595) (description "8-bit serial in/out Shift Register 3-State Outputs"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D86E00F))
    (comp (ref R6)
      (value 150)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBC4555))
    (comp (ref R12)
      (value 150)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBC4A74))
    (comp (ref J4)
      (value RJ45_LED_Shielded)
      (footprint Connector_RJ:RJ45_Amphenol_RJHSE538X)
      (datasheet ~)
      (libsource (lib Connector) (part RJ45_LED_Shielded) (description "RJ connector, 8P8C (8 positions 8 connected), two LEDs, Shielded"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC186F5))
    (comp (ref R17)
      (value 150)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E16DB9D))
    (comp (ref R11)
      (value 150)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E16F5AD))
    (comp (ref H5)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C580F0A))
    (comp (ref H6)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C580F10))
    (comp (ref H7)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C580F16))
    (comp (ref H8)
      (value MountingHole)
      (footprint MountingHole:MountingHole_3.2mm_M3)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C580F1C)))
  (libparts
    (libpart (lib 74xx) (part 74HC595)
      (aliases
        (alias 74LS595)
        (alias 74HCT595))
      (description "8-bit serial in/out Shift Register 3-State Outputs")
      (docs http://www.ti.com/lit/ds/symlink/sn74hc595.pdf)
      (footprints
        (fp DIP*W7.62mm*)
        (fp SOIC*3.9x9.9mm*P1.27mm*)
        (fp TSSOP*4.4x5mm*P0.65mm*)
        (fp SOIC*5.3x10.2mm*P1.27mm*)
        (fp SOIC*7.5x10.3mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74HC595))
      (pins
        (pin (num 1) (name QB) (type 3state))
        (pin (num 2) (name QC) (type 3state))
        (pin (num 3) (name QD) (type 3state))
        (pin (num 4) (name QE) (type 3state))
        (pin (num 5) (name QF) (type 3state))
        (pin (num 6) (name QG) (type 3state))
        (pin (num 7) (name QH) (type 3state))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name QH') (type output))
        (pin (num 10) (name ~SRCLR) (type input))
        (pin (num 11) (name SRCLK) (type input))
        (pin (num 12) (name RCLK) (type input))
        (pin (num 13) (name ~OE) (type input))
        (pin (num 14) (name SER) (type input))
        (pin (num 15) (name QA) (type 3state))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib Analog_ADC) (part INA226)
      (description "High-Side or Low-Side Measurement, Bi-Directional Current and Power Monitor (0-36V) with I2C Compatible Interface, MSOP-10")
      (docs http://www.ti.com/lit/ds/symlink/ina226.pdf)
      (footprints
        (fp MSOP*3x3mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) INA226)
        (field (name Footprint) Package_SO:MSOP-10_3x3mm_P0.5mm))
      (pins
        (pin (num 1) (name A1) (type passive))
        (pin (num 2) (name A0) (type passive))
        (pin (num 3) (name ~Alert~) (type openCol))
        (pin (num 4) (name SDA) (type BiDi))
        (pin (num 5) (name SCL) (type input))
        (pin (num 6) (name Vs) (type power_in))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name Vbus) (type input))
        (pin (num 9) (name Vin-) (type input))
        (pin (num 10) (name Vin+) (type input))))
    (libpart (lib Connector) (part 8P8C_LED_Shielded)
      (aliases
        (alias RJ45_LED_Shielded))
      (description "RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45, Shielded")
      (docs ~)
      (footprints
        (fp 8P8C*)
        (fp RJ45*))
      (fields
        (field (name Reference) J)
        (field (name Value) 8P8C_LED_Shielded))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))
        (pin (num 11) (name ~) (type passive))
        (pin (num 12) (name ~) (type passive))
        (pin (num SH) (name ~) (type passive))))
    (libpart (lib Connector) (part Screw_Terminal_01x03)
      (description "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp TerminalBlock*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Device) (part CP_Small)
      (description "Polarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal_GND24)
      (description "Four pin crystal, GND on pins 2 and 4")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND24))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib Device) (part D_Schottky_Small_ALT)
      (description "Schottky diode, small symbol, filled shape")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_Small_ALT))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part LED_Small_ALT)
      (description "Light emitting diode, small symbol, filled shape")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_Small_ALT))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R_Small)
      (description "Resistor, small symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Interface_UART) (part MAX481E)
      (aliases
        (alias MAX483E)
        (alias MAX485E)
        (alias MAX487E)
        (alias MAX1487E)
        (alias MAX3485)
        (alias MAX3483)
        (alias MAX3486))
      (description "Half duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate, with low-power shutdown, with receiver/driver enable, 32 receiver drive kapacitity, DIP-8 and SOIC-8")
      (docs https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf)
      (footprints
        (fp DIP*W7.62mm*)
        (fp SOIC*3.9x4.9mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MAX481E))
      (pins
        (pin (num 1) (name RO) (type output))
        (pin (num 2) (name ~RE) (type input))
        (pin (num 3) (name DE) (type input))
        (pin (num 4) (name DI) (type input))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name A) (type BiDi))
        (pin (num 7) (name B) (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Isolator) (part PC817)
      (description "DC Optocoupler, Vce 35V, CTR 50-300%, DIP4")
      (docs http://www.soselectronic.cz/a_info/resource/d/pc817.pdf)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) PC817)
        (field (name Footprint) Package_DIP:DIP-4_W7.62mm))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))))
    (libpart (lib MCU_ST_STM32F0) (part STM32F030F4Px)
      (description "ARM Cortex-M0 MCU, 16KB flash, 4KB RAM, 48MHz, 2.4-3.6V, 15 GPIO, TSSOP-20")
      (docs http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00088500.pdf)
      (footprints
        (fp TSSOP*4.4x6.5mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030F4Px)
        (field (name Footprint) Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm))
      (pins
        (pin (num 1) (name BOOT0) (type input))
        (pin (num 2) (name PF0) (type input))
        (pin (num 3) (name PF1) (type input))
        (pin (num 4) (name NRST) (type input))
        (pin (num 5) (name VDDA) (type power_in))
        (pin (num 6) (name PA0) (type BiDi))
        (pin (num 7) (name PA1) (type BiDi))
        (pin (num 8) (name PA2) (type BiDi))
        (pin (num 9) (name PA3) (type BiDi))
        (pin (num 10) (name PA4) (type BiDi))
        (pin (num 11) (name PA5) (type BiDi))
        (pin (num 12) (name PA6) (type BiDi))
        (pin (num 13) (name PA7) (type BiDi))
        (pin (num 14) (name PB1) (type BiDi))
        (pin (num 15) (name VSS) (type power_in))
        (pin (num 16) (name VDD) (type power_in))
        (pin (num 17) (name PA9) (type BiDi))
        (pin (num 18) (name PA10) (type BiDi))
        (pin (num 19) (name PA13) (type BiDi))
        (pin (num 20) (name PA14) (type BiDi))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole)))
    (libpart (lib Regulator_Linear) (part AP1117-15)
      (aliases
        (alias AP1117-18)
        (alias AP1117-25)
        (alias AP1117-33)
        (alias AP1117-50)
        (alias LD1117S33TR_SOT223)
        (alias LD1117S12TR_SOT223)
        (alias LD1117S18TR_SOT223)
        (alias LD1117S25TR_SOT223)
        (alias LD1117S50TR_SOT223)
        (alias NCP1117-12_SOT223)
        (alias NCP1117-1.5_SOT223)
        (alias NCP1117-1.8_SOT223)
        (alias NCP1117-2.0_SOT223)
        (alias NCP1117-2.5_SOT223)
        (alias NCP1117-2.85_SOT223)
        (alias NCP1117-3.3_SOT223)
        (alias NCP1117-5.0_SOT223)
        (alias AMS1117-1.5)
        (alias AMS1117-1.8)
        (alias AMS1117-2.5)
        (alias AMS1117-2.85)
        (alias AMS1117-3.3)
        (alias AMS1117-5.0))
      (description "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223")
      (docs http://www.diodes.com/datasheets/AP1117.pdf)
      (footprints
        (fp SOT?223*TabPin2*))
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117-15)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-223-3_TabPin2))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Sensor_Temperature) (part MCP9804_MSOP)
      (description "Microchip Technology Digital Temperature Sensor MSOP")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/22203b.pdf)
      (footprints
        (fp MSOP*3x3mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP9804_MSOP)
        (field (name Footprint) Package_SO:MSOP-8_3x3mm_P0.65mm))
      (pins
        (pin (num 1) (name SDA) (type BiDi))
        (pin (num 2) (name SCL) (type input))
        (pin (num 3) (name Alert) (type output))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name A2) (type input))
        (pin (num 6) (name A1) (type input))
        (pin (num 7) (name A0) (type input))
        (pin (num 8) (name VDD) (type power_in))))
    (libpart (lib Transistor_FET) (part IRF60DM206)
      (aliases
        (alias IRF7480M)
        (alias IRF7486M)
        (alias IRF7580M)
        (alias IRF7780M))
      (description "130A Id, 60V Vds, 2.9mOhm Rds, N-Channel MOSFET, DirectFET ME")
      (docs https://www.infineon.com/dgdl/irf60dm206.pdf?fileId=5546d462533600a4015355e433aa19ca)
      (footprints
        (fp DirectFET*ME*))
      (fields
        (field (name Reference) Q)
        (field (name Value) IRF60DM206)
        (field (name Footprint) Package_DirectFET:DirectFET_ME))
      (pins
        (pin (num 1) (name D) (type passive))
        (pin (num 2) (name G) (type input))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib components) (part L_EU_small)
      (fields
        (field (name Reference) L)
        (field (name Value) L_EU_small))
      (pins
        (pin (num 1) (name 1) (type unspc))
        (pin (num 2) (name 2) (type unspc))))
    (libpart (lib components) (part MT3608)
      (fields
        (field (name Reference) U)
        (field (name Value) MT3608))
      (pins
        (pin (num 1) (name SW) (type output))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name FB) (type input))
        (pin (num 4) (name EN) (type input))
        (pin (num 5) (name IN) (type power_in))))
    (libpart (lib components) (part TC4427)
      (fields
        (field (name Reference) U)
        (field (name Value) TC4427))
      (pins
        (pin (num 2) (name IN_A) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name IN_B) (type input))
        (pin (num 5) (name OUT_B) (type output))
        (pin (num 6) (name VDD) (type power_in))
        (pin (num 7) (name OUT_A) (type output)))))
  (libraries
    (library (logical 74xx)
      (uri /home/user/ref/kicad-symbols/74xx.lib))
    (library (logical Analog_ADC)
      (uri /home/user/ref/kicad-symbols/Analog_ADC.lib))
    (library (logical Connector)
      (uri /home/user/ref/kicad-symbols/Connector.lib))
    (library (logical Connector_Generic)
      (uri /home/user/ref/kicad-symbols/Connector_Generic.lib))
    (library (logical Device)
      (uri /home/user/ref/kicad-symbols/Device.lib))
    (library (logical Interface_UART)
      (uri /home/user/ref/kicad-symbols/Interface_UART.lib))
    (library (logical Isolator)
      (uri /home/user/ref/kicad-symbols/Isolator.lib))
    (library (logical MCU_ST_STM32F0)
      (uri /home/user/ref/kicad-symbols/MCU_ST_STM32F0.lib))
    (library (logical Mechanical)
      (uri /home/user/ref/kicad-symbols/Mechanical.lib))
    (library (logical Regulator_Linear)
      (uri /home/user/ref/kicad-symbols/Regulator_Linear.lib))
    (library (logical Sensor_Temperature)
      (uri /home/user/ref/kicad-symbols/Sensor_Temperature.lib))
    (library (logical Transistor_FET)
      (uri /home/user/ref/kicad-symbols/Transistor_FET.lib))
    (library (logical components)
      (uri /home/user/toys/led_tape_display/driver/components.lib)))
  (nets
    (net (code 1) (name /DRV1F)
      (node (ref C25) (pin 1))
      (node (ref Q4) (pin 2))
      (node (ref R19) (pin 1)))
    (net (code 2) (name GND)
      (node (ref C18) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref U7) (pin 7))
      (node (ref U7) (pin 9))
      (node (ref U7) (pin 2))
      (node (ref U7) (pin 1))
      (node (ref R32) (pin 2))
      (node (ref R31) (pin 2))
      (node (ref R30) (pin 2))
      (node (ref R29) (pin 2))
      (node (ref R28) (pin 2))
      (node (ref U2) (pin 13))
      (node (ref U6) (pin 15))
      (node (ref U2) (pin 8))
      (node (ref U6) (pin 1))
      (node (ref J4) (pin 9))
      (node (ref J4) (pin 11))
      (node (ref J8) (pin 3))
      (node (ref J8) (pin 2))
      (node (ref J8) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref C26) (pin 2))
      (node (ref U5) (pin 3))
      (node (ref C16) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref R5) (pin 1))
      (node (ref R39) (pin 1))
      (node (ref C21) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref Y1) (pin 4))
      (node (ref Y1) (pin 2))
      (node (ref C20) (pin 1))
      (node (ref C22) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C27) (pin 1))
      (node (ref C25) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref C29) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref J10) (pin 2))
      (node (ref J6) (pin 4))
      (node (ref J9) (pin 3))
      (node (ref J5) (pin 9))
      (node (ref J5) (pin 11)))
    (net (code 3) (name /ISO_DE)
      (node (ref R23) (pin 1))
      (node (ref U12) (pin 3))
      (node (ref U13) (pin 2))
      (node (ref U13) (pin 3)))
    (net (code 4) (name /DRV4F)
      (node (ref Q1) (pin 2))
      (node (ref R22) (pin 1))
      (node (ref C28) (pin 2)))
    (net (code 5) (name "Net-(J5-Pad7)")
      (node (ref J5) (pin 7)))
    (net (code 6) (name "Net-(J5-Pad8)")
      (node (ref J5) (pin 8)))
    (net (code 7) (name /SWCLK)
      (node (ref U6) (pin 20))
      (node (ref J9) (pin 2)))
    (net (code 8) (name /SWDIO)
      (node (ref U6) (pin 19))
      (node (ref J9) (pin 4)))
    (net (code 9) (name /ISO_5V)
      (node (ref U13) (pin 8))
      (node (ref C8) (pin 1))
      (node (ref U11) (pin 2))
      (node (ref U9) (pin 4))
      (node (ref C6) (pin 1))
      (node (ref U12) (pin 4))
      (node (ref C7) (pin 1)))
    (net (code 10) (name "Net-(R18-Pad2)")
      (node (ref R18) (pin 2))
      (node (ref U12) (pin 2)))
    (net (code 11) (name "Net-(D7-Pad1)")
      (node (ref D7) (pin 1))
      (node (ref R13) (pin 2)))
    (net (code 12) (name "Net-(D5-Pad1)")
      (node (ref R14) (pin 2))
      (node (ref D5) (pin 1)))
    (net (code 13) (name "Net-(D6-Pad1)")
      (node (ref R15) (pin 2))
      (node (ref D6) (pin 1)))
    (net (code 14) (name "Net-(D4-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref R16) (pin 2)))
    (net (code 15) (name "Net-(U8-Pad3)")
      (node (ref U8) (pin 3)))
    (net (code 16) (name /GND_MEAS)
      (node (ref U8) (pin 7))
      (node (ref U8) (pin 6))
      (node (ref U8) (pin 5))
      (node (ref U8) (pin 4))
      (node (ref R28) (pin 1))
      (node (ref Q4) (pin 3))
      (node (ref Q3) (pin 3))
      (node (ref R29) (pin 1))
      (node (ref R30) (pin 1))
      (node (ref R31) (pin 1))
      (node (ref R32) (pin 1))
      (node (ref U7) (pin 10)))
    (net (code 17) (name +3V3)
      (node (ref C12) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref C17) (pin 1))
      (node (ref U6) (pin 16))
      (node (ref U9) (pin 1))
      (node (ref U6) (pin 5))
      (node (ref U2) (pin 10))
      (node (ref D4) (pin 2))
      (node (ref C18) (pin 1))
      (node (ref D5) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref U12) (pin 1))
      (node (ref D7) (pin 2))
      (node (ref D6) (pin 2))
      (node (ref U7) (pin 6))
      (node (ref J6) (pin 3))
      (node (ref R27) (pin 1))
      (node (ref R26) (pin 1))
      (node (ref J10) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref U8) (pin 8))
      (node (ref C19) (pin 1))
      (node (ref J9) (pin 1))
      (node (ref U2) (pin 16))
      (node (ref U10) (pin 4))
      (node (ref C13) (pin 1)))
    (net (code 18) (name /SCL)
      (node (ref U8) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref U6) (pin 17))
      (node (ref R27) (pin 2))
      (node (ref U7) (pin 5)))
    (net (code 19) (name /DRV3F)
      (node (ref Q3) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref R21) (pin 1)))
    (net (code 20) (name /DRV2F)
      (node (ref R20) (pin 1))
      (node (ref Q2) (pin 2))
      (node (ref C26) (pin 1)))
    (net (code 21) (name "Net-(J4-Pad8)")
      (node (ref J4) (pin 8)))
    (net (code 22) (name "Net-(R12-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref U2) (pin 4)))
    (net (code 23) (name "Net-(R6-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref U2) (pin 5)))
    (net (code 24) (name /CLED1)
      (node (ref J4) (pin 12))
      (node (ref R11) (pin 2)))
    (net (code 25) (name "Net-(J4-Pad7)")
      (node (ref J4) (pin 7)))
    (net (code 26) (name /CLED2)
      (node (ref R17) (pin 2))
      (node (ref J4) (pin 10)))
    (net (code 27) (name /CLED3)
      (node (ref J5) (pin 12))
      (node (ref R6) (pin 2)))
    (net (code 28) (name /CLED4)
      (node (ref J5) (pin 10))
      (node (ref R12) (pin 2)))
    (net (code 29) (name /VIN_MON)
      (node (ref R8) (pin 2))
      (node (ref C21) (pin 1))
      (node (ref R9) (pin 2))
      (node (ref U2) (pin 12))
      (node (ref U6) (pin 10)))
    (net (code 30) (name "Net-(R17-Pad1)")
      (node (ref R17) (pin 1))
      (node (ref U2) (pin 6)))
    (net (code 31) (name "Net-(R11-Pad1)")
      (node (ref R11) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 32) (name "Net-(U2-Pad9)")
      (node (ref U2) (pin 9)))
    (net (code 33) (name /MOSI)
      (node (ref U6) (pin 13))
      (node (ref U2) (pin 14)))
    (net (code 34) (name /SCK)
      (node (ref U6) (pin 11))
      (node (ref U2) (pin 11)))
    (net (code 35) (name /RX485_A)
      (node (ref U13) (pin 6))
      (node (ref J5) (pin 5))
      (node (ref J4) (pin 5)))
    (net (code 36) (name /RS485_B)
      (node (ref J5) (pin 4))
      (node (ref U13) (pin 7))
      (node (ref J4) (pin 4)))
    (net (code 37) (name /BUS_VCC)
      (node (ref J5) (pin 2))
      (node (ref U11) (pin 3))
      (node (ref J5) (pin 1))
      (node (ref J4) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 38) (name /TX)
      (node (ref R33) (pin 1))
      (node (ref U6) (pin 8)))
    (net (code 39) (name /RX)
      (node (ref R36) (pin 1))
      (node (ref U6) (pin 9)))
    (net (code 40) (name /DE)
      (node (ref U6) (pin 7))
      (node (ref R18) (pin 1)))
    (net (code 41) (name /ISO_DI)
      (node (ref U9) (pin 3))
      (node (ref U13) (pin 4))
      (node (ref R34) (pin 1)))
    (net (code 42) (name /VBOOT_MON)
      (node (ref R3) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref U6) (pin 6)))
    (net (code 43) (name "Net-(R35-Pad2)")
      (node (ref U10) (pin 1))
      (node (ref R35) (pin 2)))
    (net (code 44) (name /ISO_RO)
      (node (ref R35) (pin 1))
      (node (ref U13) (pin 1)))
    (net (code 45) (name "Net-(R33-Pad2)")
      (node (ref U9) (pin 2))
      (node (ref R33) (pin 2)))
    (net (code 46) (name /SLED4)
      (node (ref U2) (pin 15))
      (node (ref R16) (pin 1)))
    (net (code 47) (name /SLED1)
      (node (ref U2) (pin 3))
      (node (ref R13) (pin 1)))
    (net (code 48) (name /SLED2)
      (node (ref U2) (pin 2))
      (node (ref R14) (pin 1)))
    (net (code 49) (name /SLED3)
      (node (ref U2) (pin 1))
      (node (ref R15) (pin 1)))
    (net (code 50) (name /SDA)
      (node (ref U6) (pin 18))
      (node (ref J6) (pin 2))
      (node (ref R26) (pin 2))
      (node (ref U8) (pin 1))
      (node (ref U7) (pin 4)))
    (net (code 51) (name /CTRL_A)
      (node (ref U4) (pin 2))
      (node (ref U6) (pin 12))
      (node (ref U5) (pin 4)))
    (net (code 52) (name /DRV2)
      (node (ref U5) (pin 7))
      (node (ref R20) (pin 2)))
    (net (code 53) (name /DRV4)
      (node (ref R22) (pin 2))
      (node (ref U5) (pin 5)))
    (net (code 54) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 3)))
    (net (code 55) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref L1) (pin 2)))
    (net (code 56) (name "Net-(C15-Pad1)")
      (node (ref U3) (pin 3))
      (node (ref C16) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 57) (name /OUT_A)
      (node (ref Q1) (pin 3))
      (node (ref Q3) (pin 1))
      (node (ref J1) (pin 3))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 1)))
    (net (code 58) (name "Net-(U7-Pad3)")
      (node (ref U7) (pin 3)))
    (net (code 59) (name /DRV3)
      (node (ref U4) (pin 5))
      (node (ref R21) (pin 2)))
    (net (code 60) (name /OUT_B)
      (node (ref J2) (pin 3))
      (node (ref Q4) (pin 1))
      (node (ref Q2) (pin 3))
      (node (ref J2) (pin 2))
      (node (ref J2) (pin 1)))
    (net (code 61) (name /DRV1)
      (node (ref R19) (pin 2))
      (node (ref U4) (pin 7)))
    (net (code 62) (name /XT1)
      (node (ref C20) (pin 2))
      (node (ref U6) (pin 3))
      (node (ref Y1) (pin 3)))
    (net (code 63) (name /XT2)
      (node (ref U6) (pin 2))
      (node (ref C22) (pin 1))
      (node (ref Y1) (pin 1)))
    (net (code 64) (name /RST)
      (node (ref U6) (pin 4))
      (node (ref R10) (pin 1)))
    (net (code 65) (name +VSW)
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref U4) (pin 6))
      (node (ref C23) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U5) (pin 6)))
    (net (code 66) (name /ISO_GND)
      (node (ref U11) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref J4) (pin 6))
      (node (ref J5) (pin 6))
      (node (ref J4) (pin SH))
      (node (ref U13) (pin 5))
      (node (ref J4) (pin 3))
      (node (ref R34) (pin 2))
      (node (ref U10) (pin 2))
      (node (ref J5) (pin 3))
      (node (ref J5) (pin SH))
      (node (ref C6) (pin 2))
      (node (ref R23) (pin 2)))
    (net (code 67) (name /CTRL_B)
      (node (ref U6) (pin 14))
      (node (ref U4) (pin 4))
      (node (ref U5) (pin 2)))
    (net (code 68) (name "Net-(R36-Pad2)")
      (node (ref R36) (pin 2))
      (node (ref R39) (pin 2))
      (node (ref U10) (pin 3)))
    (net (code 69) (name /VIN)
      (node (ref U7) (pin 8))
      (node (ref R1) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref Q2) (pin 1))
      (node (ref J7) (pin 3))
      (node (ref J7) (pin 2))
      (node (ref J7) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 70) (name "Net-(C3-Pad1)")
      (node (ref U1) (pin 4))
      (node (ref C4) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref L1) (pin 1)))))