                ************************
                *****  DRILL LIST  *****
                ************************

 Date                 : Sat Feb 05 23:42:05 2022
 Host                 : Windows_Hostname
 User                 : Windows_User
 Output Data          : C:/TEMP/Not_Actual_Path/DF_Drill_thru_plt.fdr
 Output List          : C:/TEMP/Not_Actual_Path/DF_Drill_thru_plt.fdl

 Target File          : C:/TEMP/Not_Actual_Path/routed.dsgn
 From-To              : Only through
 Object               : Round hole
                      : Slot hole
                      : Rectangular hole
                      : Hole in padstack (Round hole)
                      : Hole in padstack (Slot hole)
                      : Hole in padstack (Rectangular hole)
 Slot Hole            : Alternately from both ends(Migration rate: 0.50000/Odd number: Off)
 Rectangular Hole     : Alternately from both ends(Migration rate: 0.50000/Odd number: Off)
 Diameter/Hole Type   : All
 Plating Attribute    : Plated
 Embedded Comp. Via   : Do not output

 Reference Point      : 0.00000, 0.00000 [mm]
 Mirror               : Off
 Rotate               : 0-degree (No rotation)
 Scale                : 1.00000
 Offset               : 0.00000, 0.00000 [mm]

 Toolpath Sorting     : N sort
 Test Coupon          : Timing: 0 / Number of outputs: 1


 NCF File             : C:/Project_Path/settings/ncf/Excellon2.ncf
 NCF Comment          : EXCELLON2 FORMAT
 Data Type            : Excellon2 Type
 Character Code       : ASCII
 EOB Code             : LF
 EOR Code             : SPACE

 Unit                 : inch
 Coordinate Format    : 4V4
 Round Unit           : 0.00010
 Inc. / Abs.          : Absolute
 Zero Suppress        : Trailing Zero Suppress
 Omitting Coordinates : Omit
 Zero Return          : During Tool Changing: Do not make


 Assign Code          : Auto
 Distinguish Tools    : Hole type: Off
                      : Round hole and slot hole(rectangular hole): On
                      : Plating attribute: Off
                      : Embedded component via attribute: On

 Tool Table           : 
============================================================================================
| No. | Hole  | Code | Tool  | Diameter |        | Corner | Angle  |   Hole    |  Plating  |
|     | Shape |      | Shape |  Width   | Height | Radius |        |   Type    | Attribute |
|-----+-------+------+-------+----------+--------+--------+--------+-----------+-----------|
|   1 | Round | T01  | Round |   0.1000 | ------ | ------ | ------ | Undefined | Plated    |
============================================================================================

 Tool Count           : 
======================================================================
|  No.  | Code |     Hit     | Test Coupon | Inspection | Moved Dis. |
|-------+------+-------------+-------------+------------+------------|
|     1 | T01  |         100 |           0 |          0 | 1234.56789 |
|-------+------+-------------+-------------+------------+------------|
| Total        |         100 |           0 |          0 | 1234.56789 |
======================================================================

 Data Area            : min = ( 1.00000, 1.00000 ), max = ( 101.00000, 101.00000 )
