G04 Created with the python gerber_writer 0.4.2.19*
G04 #@! TF.CreationDate,2024-04-07T16:27:54.932609*
G04 #@! TF.FileFunction,Copper,L1,Top,Signal*
G04 #@! TF.FilePolarity,Positive*
G04 From https://gitlab.com/gerbolyze/gerbonara/-/issues/11 *
%MOMM*%
%FSLAX36Y36*%
G75*
%AMRoundedThermal*
0 Circular thermal with rounded corners*
0 $1 outer diameter*
0 $2 inner diameter*
0 $3 gap of straight thermal primitive*
0 $4 rotation angle*
0 $5 diameter rounding circles*
0 $6 x coordinate of q1 along h axis circle, rotated*
0 $7 y coordinate of q1 along h axis circle, rotated*
0 $8 x coordinate of q1 along v axis circle, rotated*
0 $9 y coordinate of q1 along v axis circle, rotated*
7,0,0,$1,$2,$3,$4*
1,1,$5,$6,$7*
1,1,$5,-$7,$6*
1,1,$5,-$6,-$7*
1,1,$5,$7,-$6*
1,1,$5,$8,$9*
1,1,$5,-$9,$8*
1,1,$5,-$8,-$9*
1,1,$5,$9,-$8*
1,0,$2,0,0*
%
G04 #@! TA.AperFunction,ThermalReliefPad*
G04 #@! TAShape,RoundedThermal,1,0.8,0.06,45*
%ADD10RoundedThermal,1X0.8X0.182911X45X0.103913X0.253521X0.369418X-0.253521X0.369418*%
G04 #@! TD*
%LPD*%
G04 #@! TA.AperFunction,Conductor*
G36*
X55000000Y50000000D02*
G01*
X60800000Y50000000D01*
G03*
X63000000Y52200000I0J2200000D01*
G01*
X63000000Y56000000D01*
X55000000Y56000000D01*
X55000000Y50000000D01*
G37*
G04 #@! TD*
%LPC*%
D10*
X60800000Y52200000D03*
M02*
