(footprint "L_Murata_3x3"
	(version 20241010)
	(generator "pcbnew")
	(generator_version "8.99")
	(layer "F.Cu")
	(descr "Inductor, Cenker, CKCS3012, 3.0x3.0x1.3mm, https://www.ckcoil.com/file/upload/spae532/2023-07/11/202307110955366446.pdf")
	(tags "Inductor ckcs")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
		(uuid "e4003573-c5bd-47bb-b85b-9655250e4007")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "L_Murata_3x3"
		(at 0 2.5 0)
		(layer "F.Fab")
		(uuid "2ce2f21a-73dd-43e5-90d1-4137244db6fd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b09e777b-eb16-4da9-83a9-88b153f8efce")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "32996a56-81ed-44e6-816c-093f4a901642")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "f3cd29c4-598e-4952-91d5-814bed07b3ce")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.76 -1.76)
		(end -1.76 -1.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "93126452-9b62-4d86-b52b-e4cfecc5c68b")
	)
	(fp_line
		(start -1.76 -1.76)
		(end 1.76 -1.76)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "48217306-d939-4835-8702-e1fd73efd63d")
	)
	(fp_line
		(start -1.76 1.76)
		(end -1.76 1.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fdec88b2-cfb1-40df-ae6e-d35557a28aa5")
	)
	(fp_line
		(start -1.76 1.76)
		(end 1.76 1.76)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "59c42cec-142d-4aa1-be1c-33dfc0e5ecda")
	)
	(fp_line
		(start 1.76 -1.76)
		(end 1.76 -1.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e19af70a-ff5c-4189-afbc-c95132febe8b")
	)
	(fp_line
		(start 1.76 1.76)
		(end 1.76 1.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "58dc5671-4542-435a-981e-06752ca9181e")
	)
	(fp_line
		(start -2 -1.75)
		(end -2 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2d6a0f09-d082-4450-8661-b44df62f6e75")
	)
	(fp_line
		(start -2 1.75)
		(end 2 1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f2aa8e76-d7e2-4535-ab44-615a18ffb34b")
	)
	(fp_line
		(start 2 -1.75)
		(end -2 -1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9034ce3e-82b1-4318-bd6f-049f82ddb9dc")
	)
	(fp_line
		(start 2 1.75)
		(end 2 -1.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "af2cffe6-3267-4f3a-a03d-d7a6ed50ad1d")
	)
	(fp_line
		(start -1.5 -1.5)
		(end -1.5 1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a40b3118-f9c6-4aee-8d23-684ca1b4ab1b")
	)
	(fp_line
		(start -1.5 1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "491da019-28e5-47ac-9be7-fd83af966714")
	)
	(fp_line
		(start 1.5 -1.5)
		(end -1.5 -1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f10032ea-e0b0-48ab-8898-38962eaf97f4")
	)
	(fp_line
		(start 1.5 1.5)
		(end 1.5 -1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5abfbf07-e55d-4cd3-9e15-a32012636a38")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "e19c8134-ae33-480c-92a2-56452886e098")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "1" smd rect
		(at -1.1 0)
		(size 0.8 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "6b0b7cf6-6872-40cb-ac61-3ccb41ea353e")
	)
	(pad "2" smd rect
		(at 1.1 0)
		(size 0.8 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "43acfdc4-6471-434e-bcec-bb3b2e23c4af")
	)
	(embedded_fonts no)
	(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Cenker_CKCS3012.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
