(footprint "sfp_edge_connector_male" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "J1" (at -0.005992 7.02904 180 unlocked) (layer "F.SilkS") (tstamp 012d590d-1d34-4ab9-9c12-278cd8ac6c3d)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Value" "dbg" (at 0.1 -6.5 0 unlocked) (layer "F.Fab") hide (tstamp c069a667-f2a9-4ace-8d69-35e48f4c7896)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp a033ea76-b26a-4fdb-b531-91c06c944a6e)
    (effects (font (size 1.27 1.27)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 841997db-42fa-429a-8646-bd6ac7cd58a2)
    (effects (font (size 1.27 1.27)))
  )
  (property "Description" "Generic connector, double row, 02x10, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 33b7f5aa-7145-4acb-ada4-149dc32da70e)
    (effects (font (size 1.27 1.27)))
  )
  (property "DNP" "DNP" (at 0 0 -90) (layer "F.Fab") hide (tstamp a28111ed-f4be-4d74-abe4-b619fdfe1193)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_line (start -4.5 6) (end 4.5 6)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a4428433-892e-49d8-9630-b9b6939fcb3a))
  (fp_rect (start -4.605992 -0.004438) (end 4.594008 3.495562)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "B.Mask") (tstamp 125f8e69-5c5c-412f-980c-4535d29e6fc6))
  (fp_rect (start -4.6 0) (end 4.6 3.5)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Mask") (tstamp 9c8640a4-e76d-45a2-877a-ccca68f283fb))
  (fp_line (start -4.6 -0.010223) (end -4.6 5.989777)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp 63431b8e-1c49-49f0-a3b4-280f56351412))
  (fp_line (start -4.6 -0.010223) (end 4.6 -0.010223)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp e3c79883-9ae6-4078-96ed-b6552d02fb83))
  (fp_line (start 4.6 -0.010223) (end 4.6 5.989777)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp fa1cc20d-1e41-43fc-92cb-c7766d86fc71))
  (fp_rect (start -4.6 0) (end 4.6 6)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp 8071876f-0d1c-4caa-93f7-174bff39c954))
  (fp_rect (start -4.6 0) (end 4.6 6)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 92d1b75e-a8ef-4d50-8d2f-826b565be2fb))
  (fp_text user "${REF}" (at -1 -4.8 0 unlocked) (layer "F.Fab") hide (tstamp 7231a561-3440-4183-9607-ac21d2b12553)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd rect (at -3.396501 1.998194) (size 0.6 3) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp e8d13b7b-c261-447f-8f51-b99202df59ad)
  )
  (pad "2" smd rect (at -2.596501 2.397342) (size 0.6 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp d95c6787-7462-4174-933a-7bdc74cbeb9a)
  )
  (pad "3" smd rect (at -1.796501 2.398194) (size 0.6 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp 6cfc4a0a-2cd0-4e35-b763-ddf49269f0b1)
  )
  (pad "4" smd rect (at -0.996501 1.99129) (size 0.6 3) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp 896a31aa-2061-4dda-92ef-2054ca0cb9d5)
  )
  (pad "5" smd rect (at -0.194057 2.196207) (size 0.6 2.6) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp 01f45944-5fb8-4067-898a-345041c44dd9)
  )
  (pad "6" smd rect (at 0.605943 2.198194) (size 0.6 2.6) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp e99b4ca2-672c-4f27-97ea-ebd9e9aba971)
  )
  (pad "7" smd rect (at 1.403499 1.994742) (size 0.6 3) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp a702671d-5f89-49d6-9f8d-a864969730b5)
  )
  (pad "8" smd rect (at 2.203499 2.397342) (size 0.6 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp 4f2e4d45-e229-4dd8-a945-94ee1e557776)
  )
  (pad "9" smd rect (at 3.003499 2.398194) (size 0.6 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp a507340a-814f-47ba-b8fc-019f1208389a)
  )
  (pad "10" smd rect (at 3.803499 1.998194) (size 0.6 3) (layers "B.Cu" "B.Paste" "B.Mask")
    (thermal_bridge_angle 45)
    (tstamp af86d971-7826-4037-8c7f-f4e32b6aec67)
  )
  (pad "11" smd rect (at 3.4 2) (size 0.6 3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 389eafea-f5a6-45a6-b630-d5635d15ca44)
  )
  (pad "12" smd rect (at 2.6 2.399148) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 268b6b11-2c7c-4781-8e97-6fb105d2e235)
  )
  (pad "13" smd rect (at 1.8 2.4) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 82a65a45-ec09-4019-8fa5-955d7f4029e7)
  )
  (pad "14" smd rect (at 1 1.993096) (size 0.6 3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 2bcac0a0-7548-4d49-9606-e52e7f497b30)
  )
  (pad "15" smd rect (at 0.197556 2.198013) (size 0.6 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 5abe30bb-27ec-4555-9cc2-98a56c11416e)
  )
  (pad "16" smd rect (at -0.602444 2.2) (size 0.6 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 48b0b452-1531-4f5f-86f2-08fbbf20a90a)
  )
  (pad "17" smd rect (at -1.4 1.996548) (size 0.6 3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp e83e36a3-9317-4bac-9981-714adc7e9487)
  )
  (pad "18" smd rect (at -2.2 2.399148) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 1242816d-aee8-4fc7-bf9d-5dce34cf16b4)
  )
  (pad "19" smd rect (at -3 2.4) (size 0.6 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 25679e05-b3ed-4dbf-a721-cdba2e2220fa)
  )
  (pad "20" smd rect (at -3.8 2) (size 0.6 3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 59014b12-3eee-4f14-9e57-3669d27bc6fe)
  )
)
