(footprint "SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.34x2.34mm"
	(version 20240225)
	(generator "pcbnew")
	(generator_version "8.99")
	(layer "F.Cu")
	(descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOIC SO")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
		(uuid "ffa0f657-cdb7-44c7-8e69-528e0a4a4129")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.34x2.34mm"
		(at 0 3.4 0)
		(layer "F.Fab")
		(uuid "1db929a3-e155-4c09-a67d-cc32c14c0d35")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.34x2.34mm"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0005ac6a-58c6-4ba1-969b-576176e03940")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "817a7b3a-a946-4a38-a062-945052602dba")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1c10de3b-4bb5-4e62-90e3-51eaa16ede93")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 0 -2.56)
		(end -1.95 -2.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c6ebe8a5-f662-411b-a552-118c43055729")
	)
	(fp_line
		(start 0 -2.56)
		(end 1.95 -2.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7209cbf4-37d0-421a-9c60-5ed823991615")
	)
	(fp_line
		(start 0 2.56)
		(end -1.95 2.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "10b668fc-01e7-4797-afb2-37f7b0d0bf21")
	)
	(fp_line
		(start 0 2.56)
		(end 1.95 2.56)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0096ed58-a946-4f80-97b6-21bcd821b04f")
	)
	(fp_poly
		(pts
			(xy -2.7 -2.465) (xy -2.94 -2.801) (xy -2.46 -2.801) (xy -2.7 -2.465)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "9ebf1eee-5627-4886-a237-e6aa69bf33a0")
	)
	(fp_line
		(start -3.7 -2.7)
		(end -3.7 2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a8f546d9-dcd7-4308-ae96-7073c52a8a23")
	)
	(fp_line
		(start -3.7 2.7)
		(end 3.7 2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "78d15d65-da85-4688-89ee-59ee2bb58374")
	)
	(fp_line
		(start 3.7 -2.7)
		(end -3.7 -2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dc47e6a0-d692-4b65-bc7b-57eb90ef3c8d")
	)
	(fp_line
		(start 3.7 2.7)
		(end 3.7 -2.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fd0efa4c-68b1-4078-9861-e91604e2d899")
	)
	(fp_line
		(start -1.95 -1.475)
		(end -0.975 -2.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f578ea70-b1a9-4a88-99de-a3eda8114b14")
	)
	(fp_line
		(start -1.95 2.45)
		(end -1.95 -1.475)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d219e643-df80-43eb-a340-d348271d62d6")
	)
	(fp_line
		(start -0.975 -2.45)
		(end 1.95 -2.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2e9abf18-8637-4a2f-b14d-6ae532d60fc3")
	)
	(fp_line
		(start 1.95 -2.45)
		(end 1.95 2.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "935badc9-c133-44b7-bb00-9fa61ccf8edc")
	)
	(fp_line
		(start 1.95 2.45)
		(end -1.95 2.45)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "19d90de9-5e02-4225-8499-1a7a40a8a4fb")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "bb12b04b-81ae-4d4b-8e63-96349ff7a8f5")
		(effects
			(font
				(size 0.98 0.98)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd roundrect
		(at -0.57 -0.75)
		(size 0.92 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "298f63ed-94e0-44f9-ad60-d478190a492a")
	)
	(pad "" smd roundrect
		(at -0.57 0.75)
		(size 0.92 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "692d1462-769e-4a5a-81b2-3b1cf42b9266")
	)
	(pad "" smd roundrect
		(at 0.57 -0.75)
		(size 0.92 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e035d9ee-6884-43f7-8169-a3c1453f4d03")
	)
	(pad "" smd roundrect
		(at 0.57 0.75)
		(size 0.92 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "a90902ae-09d3-4a36-a1a4-80cb5a0ffd31")
	)
	(pad "1" smd roundrect
		(at -2.475 -1.905)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "2b7ff269-b925-488b-b2cf-5191f0b98069")
	)
	(pad "2" smd roundrect
		(at -2.475 -0.635)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "5eda7472-a334-4b2c-ace7-6369f01dcc94")
	)
	(pad "3" smd roundrect
		(at -2.475 0.635)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "56bdde26-4217-4199-98c9-1e0448136b50")
	)
	(pad "4" smd roundrect
		(at -2.475 1.905)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "4e53fb06-ba99-4930-a5a0-71fef485dccb")
	)
	(pad "5" smd roundrect
		(at 2.475 1.905)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "9e376029-a231-4046-bad9-9d5fe6115857")
	)
	(pad "6" smd roundrect
		(at 2.475 0.635)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "667dd0ed-3c6f-464c-b26f-bfeef266ca9c")
	)
	(pad "7" smd roundrect
		(at 2.475 -0.635)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "2968d448-27bc-4159-99a0-ac2d89a862ac")
	)
	(pad "8" smd roundrect
		(at 2.475 -1.905)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "7904de0a-1726-4d58-bb2b-2a96b1447410")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 2.34 2.34)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(uuid "84aad9d6-bb7a-48e8-910e-e2bc1f35f0ff")
	)
	(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
