(footprint "HCTL_HC-SFP-20P_C2897291"
	(version 20240225)
	(generator "pcbnew")
	(generator_version "8.99")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f2268bbc-4799-48b6-afcb-cabec8db21db")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "HCTL_HC-SFP-20P_C2897291"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b2aeb030-9e3c-4594-9f3a-a078e4cfd06b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "HCTL_HC-SFP-20P_C2897291"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8f73dfc6-3183-4b34-bcc6-a7927a61bb4d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c5489c33-898c-44be-b349-a8fc928a2ed0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "14dc4e9b-5b3b-4140-a1e3-2a69ba3f982a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start 4.8 0)
		(end 4.8 -4.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "946c4fdc-b13f-4895-b222-40e30af2216a")
	)
	(fp_line
		(start 4.8 0)
		(end 4.8 4.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "dc6ebd00-038b-4254-8087-ec7928d68279")
	)
	(fp_rect
		(start -5.7 -5.3)
		(end 5.7 5.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "1f3373b0-78d5-4e85-a51f-1b76362654f5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c19dbbbf-4635-4379-8228-f26e5588cee6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(uuid "b6c571b9-d8ff-4fd3-b33b-0dae1ffd4a7c")
		(pts
			(xy 4.8 -4.1) (xy 3.4 -4.1)
		)
		(height 2.75)
		(gr_text "1.4000 mm"
			(at 4.1 -8 0)
			(layer "Cmts.User")
			(uuid "b6c571b9-d8ff-4fd3-b33b-0dae1ffd4a7c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(uuid "e1f09bdb-c82e-4865-8cb9-4554ba471532")
		(pts
			(xy 4.8 4.1) (xy 3.8 4.1)
		)
		(height -2.3)
		(gr_text "1.0000 mm"
			(at 4.3 5.25 0)
			(layer "Cmts.User")
			(uuid "e1f09bdb-c82e-4865-8cb9-4554ba471532")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(pad "" np_thru_hole circle
		(at -4.8 0)
		(size 1.55 1.55)
		(drill 1.55)
		(layers "F&B.Cu" "*.Mask")
		(uuid "0df63985-970c-4086-824d-de5d180edfd3")
	)
	(pad "" np_thru_hole circle
		(at 4.8 0)
		(size 1.55 1.55)
		(drill 1.55)
		(layers "F&B.Cu" "*.Mask")
		(uuid "795cb72c-604e-478c-8e3c-6b008a205776")
	)
	(pad "1" smd rect
		(at -3.4 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "86791b1a-08a9-45ed-a558-f8faa770a32e")
	)
	(pad "2" smd rect
		(at -2.6 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "7931f0ad-9527-4db4-82e5-c7dca341e3f7")
	)
	(pad "3" smd rect
		(at -1.8 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "f0b8879e-1801-44de-a2b0-d7dbc5603089")
	)
	(pad "4" smd rect
		(at -1 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "4aad4c21-1713-4947-90da-e62eeb0c8dd7")
	)
	(pad "5" smd rect
		(at -0.2 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "c3ec7063-6887-46b0-af6c-2dd67e1825e4")
	)
	(pad "6" smd rect
		(at 0.6 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0954b82b-a011-485d-8961-51cdd97968d6")
	)
	(pad "7" smd rect
		(at 1.4 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "3b414af5-921a-4ecd-ad3e-b0b864f9d709")
	)
	(pad "8" smd rect
		(at 2.2 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "6773a7a1-f433-4ae8-b5ca-e0458c9548eb")
	)
	(pad "9" smd rect
		(at 3 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "854c7aa8-8864-417b-b681-3c905e9e505a")
	)
	(pad "10" smd rect
		(at 3.8 4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "bbaf04f7-9e1a-4f4d-8be3-d522d2070d9a")
	)
	(pad "11" smd rect
		(at 3.4 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "856d180a-a4b8-437f-90ce-a160397df6ca")
	)
	(pad "12" smd rect
		(at 2.6 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "3c41e8a4-c3b8-475b-ae60-2ac351d26c50")
	)
	(pad "13" smd rect
		(at 1.8 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "094c6818-f572-4af5-b683-44965ebe0c84")
	)
	(pad "14" smd rect
		(at 1 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "202fcbe9-2edc-451a-b157-eda6f50ecb31")
	)
	(pad "15" smd rect
		(at 0.2 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "d013f8cd-76b3-4e78-b2aa-1d93665357ab")
	)
	(pad "16" smd rect
		(at -0.6 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "514405ac-674e-4000-8b73-a268b9ddb532")
	)
	(pad "17" smd rect
		(at -1.4 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "76deb6a0-766d-4ff4-b655-000d8955be59")
	)
	(pad "18" smd rect
		(at -2.2 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "bfb97462-f907-442b-9f66-666dca93c65b")
	)
	(pad "19" smd rect
		(at -3 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "5c4daac7-633c-488f-9b0a-82af2da29cbb")
	)
	(pad "20" smd rect
		(at -3.8 -4.1)
		(size 0.5 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "35303279-43ce-4239-bef0-7f09bc14c02d")
	)
)
