(export (version D)
  (design
    (source /home/user/research/secureHID/pcb/securehid.sch)
    (date "Thu Nov 29 09:36:23 2018")
    (tool "Eeschema (5.0.1)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source securehid.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U2)
      (value STM32F103C8T6)
      (footprint Package_QFP:LQFP-48_7x7mm_P0.5mm)
      (libsource (lib MCU_ST_STM32F1) (part STM32F103C8Tx) (description "ARM Cortex-M3 MCU, 64KB flash, 20KB RAM, 72MHz, 2-3.6V, 37 GPIO, LQFP-48"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEAD06))
    (comp (ref J1)
      (value USB_B_Micro)
      (footprint footprints:microusb_ali_dovetail)
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEADC1))
    (comp (ref J6)
      (value USB_A)
      (footprint footprints:USB_A_FEMALE_THT)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32849715796.html))
      (libsource (lib conn) (part USB_A) (description "USB Type A connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEAE66))
    (comp (ref U1)
      (value AP1117-33)
      (footprint TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2)
      (datasheet http://www.diodes.com/datasheets/AP1117.pdf)
      (libsource (lib regul) (part AP1117-33) (description "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF631A))
    (comp (ref C10)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF660D))
    (comp (ref C9)
      (value 220u)
      (footprint Capacitor_SMD:C_Elec_10x10.2)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32556865449.html))
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF69F7))
    (comp (ref C12)
      (value 47u)
      (footprint Capacitor_SMD:C_Elec_6.3x5.8)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32846711940.html))
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF6DE0))
    (comp (ref C11)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEF7098))
    (comp (ref R9)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF05F40))
    (comp (ref R7)
      (value 22)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF06DFB))
    (comp (ref R6)
      (value 1k5)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF07F6E))
    (comp (ref Y2)
      (value 8MHz)
      (footprint Crystal:Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm_HandSoldering)
      (libsource (lib device) (part Crystal_GND24_Small) (description "Two pin crystal, two ground/package pins (pin2 and 4) small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF102A6))
    (comp (ref C17)
      (value 12p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF11861))
    (comp (ref C18)
      (value 12p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF125C0))
    (comp (ref R8)
      (value 1M)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF1348D))
    (comp (ref C14)
      (value 10u)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF1E83A))
    (comp (ref C15)
      (value 10u)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF1FBEB))
    (comp (ref R1)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF2746F))
    (comp (ref C7)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF38053))
    (comp (ref C8)
      (value 10u)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF395B5))
    (comp (ref U3)
      (value STM32F407VET6)
      (footprint Package_QFP:LQFP-100_14x14mm_P0.5mm)
      (libsource (lib MCU_ST_STM32F4) (part STM32F407VETx) (description "ARM Cortex-M4 MCU, 512KB flash, 128KB RAM, 168MHz, 1.8-3.6V, 82 GPIO, LQFP-100"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEEABF3))
    (comp (ref R5)
      (value 0)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF5BB39))
    (comp (ref C1)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF62211))
    (comp (ref C2)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF6342B))
    (comp (ref C4)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF6483B))
    (comp (ref C5)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF65555))
    (comp (ref C6)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF65AAF))
    (comp (ref BT1)
      (value CR2032)
      (footprint Battery:BatteryHolder_Keystone_1060_1x2032)
      (libsource (lib device) (part Battery_Cell) (description "single battery cell"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF6C982))
    (comp (ref J2)
      (value SWD_HOST)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF8388D))
    (comp (ref J3)
      (value UART_HOST)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFBEF9F))
    (comp (ref J5)
      (value UART_DEVICE)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFCCF0F))
    (comp (ref U4)
      (value FE1.1s)
      (footprint Package_SO:SSOP-28_3.9x9.9mm_P0.635mm)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32787809220.html))
      (libsource (lib components) (part FE1.1s) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFFC98A))
    (comp (ref J8)
      (value USB_A)
      (footprint footprints:USB_A_FEMALE_THT)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32849715796.html))
      (libsource (lib conn) (part USB_A) (description "USB Type A connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C01D6A6))
    (comp (ref C24)
      (value 10u)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C047824))
    (comp (ref C23)
      (value 10u)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C048AFF))
    (comp (ref Y4)
      (value 12MHz)
      (footprint Crystal:Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm_HandSoldering)
      (libsource (lib device) (part Crystal_GND24_Small) (description "Two pin crystal, two ground/package pins (pin2 and 4) small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C073CEB))
    (comp (ref C21)
      (value 22p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C07723C))
    (comp (ref C20)
      (value 22p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C079071))
    (comp (ref R10)
      (value 2k7)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C095FA0))
    (comp (ref R11)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0F41D6))
    (comp (ref J7)
      (value USB_SPARE)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Odd_Even) (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C134723))
    (comp (ref LS1)
      (value "12mm passive piezo")
      (footprint Buzzer_Beeper:Buzzer_12x9.5RM7.6)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32503620431.html))
      (libsource (lib device) (part Speaker_Crystal) (description "crystal speaker/transducer"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C238571))
    (comp (ref Q1)
      (value AO3400)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N7002.pdf)
      (libsource (lib transistors) (part 2N7002) (description "60V Vds, 0.115A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C23FA3A))
    (comp (ref D4)
      (value "Ice blue")
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/store/product//1758868_32693684017.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C249B1C))
    (comp (ref R12)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C25E0F0))
    (comp (ref R13)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C25EB0C))
    (comp (ref R14)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C25EC8A))
    (comp (ref R15)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C25F0FB))
    (comp (ref R16)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C25F439))
    (comp (ref R17)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C26016A))
    (comp (ref Q2)
      (value AO3400)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N7002.pdf)
      (libsource (lib transistors) (part 2N7002) (description "60V Vds, 0.115A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E1C85))
    (comp (ref D10)
      (value pink)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32376752790.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E1C8C))
    (comp (ref R18)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E1CB6))
    (comp (ref R19)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E1CBD))
    (comp (ref R20)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E1CC4))
    (comp (ref R21)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E1CCB))
    (comp (ref R22)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E1CD2))
    (comp (ref R23)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E1CD9))
    (comp (ref Q3)
      (value AO3400)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N7002.pdf)
      (libsource (lib transistors) (part 2N7002) (description "60V Vds, 0.115A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C35C82C))
    (comp (ref C29)
      (value 100p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C36E3E6))
    (comp (ref R24)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C39507D))
    (comp (ref R25)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3BA02E))
    (comp (ref C25)
      (value 47u)
      (footprint Capacitor_SMD:C_Elec_6.3x5.8)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32846711940.html))
      (libsource (lib device) (part CP_Small) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51704D))
    (comp (ref C26)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51BE00))
    (comp (ref C27)
      (value 47u)
      (footprint Capacitor_SMD:C_Elec_6.3x5.8)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32846711940.html))
      (libsource (lib device) (part CP_Small) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C56285D))
    (comp (ref C28)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C562864))
    (comp (ref D1)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5B8E64))
    (comp (ref D2)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5C2170))
    (comp (ref D3)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5C4C69))
    (comp (ref D16)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5C8AAB))
    (comp (ref D17)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5CCC8D))
    (comp (ref D18)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5CF123))
    (comp (ref D19)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5CFFD0))
    (comp (ref D20)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D158A))
    (comp (ref D21)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D3F1F))
    (comp (ref D22)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D4845))
    (comp (ref D23)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5D5CC9))
    (comp (ref RN1)
      (value 4*620)
      (footprint Resistor_SMD:R_Array_Convex_4x0603)
      (fields
        (field (name marutsu) https://www.marutsu.co.jp/pc/i/14222/))
      (libsource (lib device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5DE49D))
    (comp (ref RN2)
      (value 4*620)
      (footprint Resistor_SMD:R_Array_Convex_4x0603)
      (fields
        (field (name marutsu) https://www.marutsu.co.jp/pc/i/14222/))
      (libsource (lib device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63187D))
    (comp (ref RN3)
      (value 4*620)
      (footprint Resistor_SMD:R_Array_Convex_4x0603)
      (fields
        (field (name marutsu) https://www.marutsu.co.jp/pc/i/14222/))
      (libsource (lib device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C63296F))
    (comp (ref D24)
      (value red)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part LED_Small) (description "LED, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C6C0DF6))
    (comp (ref SW1)
      (value SW_Push)
      (footprint Button_Switch_SMD:SW_SPST_EVPBF)
      (libsource (lib switches) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA5E99A))
    (comp (ref Y1)
      (value 8MHz)
      (footprint Crystal:Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm_HandSoldering)
      (libsource (lib device) (part Crystal_GND24_Small) (description "Two pin crystal, two ground/package pins (pin2 and 4) small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFB4F88))
    (comp (ref C13)
      (value 12p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFB4F8F))
    (comp (ref C16)
      (value 12p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFB4F96))
    (comp (ref R4)
      (value 1M)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFB4F9D))
    (comp (ref C19)
      (value 12p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1E173E))
    (comp (ref C22)
      (value 12p)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1E1745))
    (comp (ref R2)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2E339B))
    (comp (ref R3)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C330F23))
    (comp (ref J4)
      (value SWD_DEVICE)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C397A42))
    (comp (ref TP8)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C47DFE5))
    (comp (ref TP10)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C485760))
    (comp (ref TP12)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C485D2E))
    (comp (ref TP13)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4860F8))
    (comp (ref TP15)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C486A3A))
    (comp (ref TP17)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C486BFA))
    (comp (ref TP21)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48822E))
    (comp (ref TP25)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48868A))
    (comp (ref TP29)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48940B))
    (comp (ref TP32)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C489AAB))
    (comp (ref TP34)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48A6A6))
    (comp (ref TP36)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48B64C))
    (comp (ref TP38)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48C6FB))
    (comp (ref TP40)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48CF33))
    (comp (ref TP42)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48D18C))
    (comp (ref TP44)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C48DB4A))
    (comp (ref TP7)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4901EF))
    (comp (ref TP6)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C493CA7))
    (comp (ref TP4)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C49510A))
    (comp (ref TP9)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C496BCA))
    (comp (ref TP11)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C49F6C2))
    (comp (ref TP16)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A055A))
    (comp (ref TP18)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A139B))
    (comp (ref TP22)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A15A3))
    (comp (ref TP26)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A17AF))
    (comp (ref TP30)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A19BF))
    (comp (ref TP45)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C4A7F68))
    (comp (ref TP20)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C936D5A))
    (comp (ref TP24)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9684E2))
    (comp (ref TP28)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C969C2A))
    (comp (ref TP31)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C96A276))
    (comp (ref TP33)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C96A49E))
    (comp (ref TP35)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C96B372))
    (comp (ref TP37)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C96BD12))
    (comp (ref TP39)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C96BF46))
    (comp (ref TP41)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C96CA1E))
    (comp (ref TP43)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C96DB03))
    (comp (ref TP14)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB50D04))
    (comp (ref TP5)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB84290))
    (comp (ref TP3)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBBAA24))
    (comp (ref TP1)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBEFE72))
    (comp (ref TP2)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF3D8C))
    (comp (ref TP46)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC59D09))
    (comp (ref TP47)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC968FC))
    (comp (ref TP48)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC985C2))
    (comp (ref TP49)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC99F42))
    (comp (ref TP50)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC9AA61))
    (comp (ref TP52)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD6F295))
    (comp (ref TP54)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD6F29D))
    (comp (ref TP56)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD6F2A4))
    (comp (ref TP58)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD6F2AB))
    (comp (ref TP60)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD6F2B2))
    (comp (ref TP62)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDA3ACF))
    (comp (ref TP64)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDA3AD7))
    (comp (ref TP66)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDA3ADE))
    (comp (ref TP68)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDA3AE5))
    (comp (ref TP70)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDA3AEC))
    (comp (ref TP72)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE11B57))
    (comp (ref TP74)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE11B5F))
    (comp (ref TP76)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE11B66))
    (comp (ref TP78)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE11B6D))
    (comp (ref TP51)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE56744))
    (comp (ref TP53)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE5674C))
    (comp (ref TP55)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE56753))
    (comp (ref TP57)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE5675A))
    (comp (ref TP59)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE56761))
    (comp (ref TP61)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE5676C))
    (comp (ref TP63)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE56774))
    (comp (ref TP65)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE5677B))
    (comp (ref TP67)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE56782))
    (comp (ref TP69)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE56789))
    (comp (ref TP71)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE56794))
    (comp (ref TP73)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE5679C))
    (comp (ref TP75)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE567A3))
    (comp (ref TP77)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE567AA))
    (comp (ref TP79)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF09FE7))
    (comp (ref TP80)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF0B43E))
    (comp (ref TP19)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF877DC))
    (comp (ref TP23)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF8ADC6))
    (comp (ref TP27)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF8B936))
    (comp (ref D11)
      (value pink)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32376752790.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51A7AC))
    (comp (ref D12)
      (value pink)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32376752790.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51AF3E))
    (comp (ref D13)
      (value pink)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32376752790.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51B8E6))
    (comp (ref D14)
      (value pink)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32376752790.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51CDA8))
    (comp (ref D15)
      (value pink)
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32376752790.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51D76E))
    (comp (ref D5)
      (value "Ice blue")
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/store/product//1758868_32693684017.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51EE78))
    (comp (ref D6)
      (value "Ice blue")
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/store/product//1758868_32693684017.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C51FC8E))
    (comp (ref D7)
      (value "Ice blue")
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/store/product//1758868_32693684017.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C52067C))
    (comp (ref D8)
      (value "Ice blue")
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/store/product//1758868_32693684017.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C527E21))
    (comp (ref D9)
      (value "Ice blue")
      (footprint LED_SMD:LED_PLCC_2835_Handsoldering)
      (fields
        (field (name ali) https://www.aliexpress.com/store/product//1758868_32693684017.html))
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5294FF))
    (comp (ref C30)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8C6262))
    (comp (ref U5)
      (value AP1117-33)
      (footprint TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2)
      (datasheet http://www.diodes.com/datasheets/AP1117.pdf)
      (libsource (lib regul) (part AP1117-33) (description "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAC94A7))
    (comp (ref C32)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAC94AE))
    (comp (ref C34)
      (value 47u)
      (footprint Capacitor_SMD:C_Elec_6.3x5.8)
      (fields
        (field (name ali) https://www.aliexpress.com/item//32846711940.html))
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAC94BE))
    (comp (ref C33)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAC94C5))
    (comp (ref C31)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC31EB0))
    (comp (ref C35)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC31EB6))
    (comp (ref C36)
      (value 100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC31EBC))
    (comp (ref R26)
      (value NETTIE)
      (footprint NetTie:NetTie-2_SMD_Pad2.0mm)
      (libsource (lib device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CCA267C))
    (comp (ref TP81)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BFF0539))
    (comp (ref TP82)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C0015E1))
    (comp (ref TP83)
      (value TestPoint_Alt)
      (footprint TestPoint:TestPoint_Pad_1.0x1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Alt) (description "test point (alternative shape)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C13B94B))
    (comp (ref Y3)
      (value 32.768kHz)
      (footprint Crystal:Crystal_C26-LF_D2.1mm_L6.5mm_Horizontal_1EP_style1)
      (datasheet ~)
      (libsource (lib Device) (part Crystal_GND3) (description "Three pin crystal, GND on pin 3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C2565BB)))
  (libparts
    (libpart (lib Connector) (part TestPoint_Alt)
      (description "test point (alternative shape)")
      (docs ~)
      (footprints
        (fp Pin*)
        (fp Test*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TestPoint_Alt))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x05_Odd_Even)
      (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x05_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))))
    (libpart (lib Device) (part Crystal_GND3)
      (description "Three pin crystal, GND on pin 3")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND3))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib MCU_ST_STM32F1) (part STM32F103C8Tx)
      (aliases
        (alias STM32F103CBTx))
      (description "ARM Cortex-M3 MCU, 64KB flash, 20KB RAM, 72MHz, 2-3.6V, 37 GPIO, LQFP-48")
      (docs http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00161566.pdf)
      (footprints
        (fp LQFP*7x7mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F103C8Tx)
        (field (name Footprint) Package_QFP:LQFP-48_7x7mm_P0.5mm))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name PC13) (type BiDi))
        (pin (num 3) (name PC14) (type BiDi))
        (pin (num 4) (name PC15) (type BiDi))
        (pin (num 5) (name PD0) (type input))
        (pin (num 6) (name PD1) (type input))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name VSSA) (type power_in))
        (pin (num 9) (name VDDA) (type power_in))
        (pin (num 10) (name PA0) (type BiDi))
        (pin (num 11) (name PA1) (type BiDi))
        (pin (num 12) (name PA2) (type BiDi))
        (pin (num 13) (name PA3) (type BiDi))
        (pin (num 14) (name PA4) (type BiDi))
        (pin (num 15) (name PA5) (type BiDi))
        (pin (num 16) (name PA6) (type BiDi))
        (pin (num 17) (name PA7) (type BiDi))
        (pin (num 18) (name PB0) (type BiDi))
        (pin (num 19) (name PB1) (type BiDi))
        (pin (num 20) (name PB2) (type BiDi))
        (pin (num 21) (name PB10) (type BiDi))
        (pin (num 22) (name PB11) (type BiDi))
        (pin (num 23) (name VSS) (type power_in))
        (pin (num 24) (name VDD) (type power_in))
        (pin (num 25) (name PB12) (type BiDi))
        (pin (num 26) (name PB13) (type BiDi))
        (pin (num 27) (name PB14) (type BiDi))
        (pin (num 28) (name PB15) (type BiDi))
        (pin (num 29) (name PA8) (type BiDi))
        (pin (num 30) (name PA9) (type BiDi))
        (pin (num 31) (name PA10) (type BiDi))
        (pin (num 32) (name PA11) (type BiDi))
        (pin (num 33) (name PA12) (type BiDi))
        (pin (num 34) (name PA13) (type BiDi))
        (pin (num 35) (name VSS) (type power_in))
        (pin (num 36) (name VDD) (type power_in))
        (pin (num 37) (name PA14) (type BiDi))
        (pin (num 38) (name PA15) (type BiDi))
        (pin (num 39) (name PB3) (type BiDi))
        (pin (num 40) (name PB4) (type BiDi))
        (pin (num 41) (name PB5) (type BiDi))
        (pin (num 42) (name PB6) (type BiDi))
        (pin (num 43) (name PB7) (type BiDi))
        (pin (num 44) (name BOOT0) (type input))
        (pin (num 45) (name PB8) (type BiDi))
        (pin (num 46) (name PB9) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))))
    (libpart (lib MCU_ST_STM32F4) (part STM32F407VETx)
      (aliases
        (alias STM32F407VGTx))
      (description "ARM Cortex-M4 MCU, 512KB flash, 128KB RAM, 168MHz, 1.8-3.6V, 82 GPIO, LQFP-100")
      (docs http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00037051.pdf)
      (footprints
        (fp LQFP*14x14mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F407VETx)
        (field (name Footprint) Package_QFP:LQFP-100_14x14mm_P0.5mm))
      (pins
        (pin (num 1) (name PE2) (type BiDi))
        (pin (num 2) (name PE3) (type BiDi))
        (pin (num 3) (name PE4) (type BiDi))
        (pin (num 4) (name PE5) (type BiDi))
        (pin (num 5) (name PE6) (type BiDi))
        (pin (num 6) (name VBAT) (type power_in))
        (pin (num 7) (name PC13) (type BiDi))
        (pin (num 8) (name PC14) (type BiDi))
        (pin (num 9) (name PC15) (type BiDi))
        (pin (num 10) (name VSS) (type power_in))
        (pin (num 11) (name VDD) (type power_in))
        (pin (num 12) (name PH0) (type input))
        (pin (num 13) (name PH1) (type input))
        (pin (num 14) (name NRST) (type input))
        (pin (num 15) (name PC0) (type BiDi))
        (pin (num 16) (name PC1) (type BiDi))
        (pin (num 17) (name PC2) (type BiDi))
        (pin (num 18) (name PC3) (type BiDi))
        (pin (num 19) (name VDD) (type power_in))
        (pin (num 20) (name VSSA) (type power_in))
        (pin (num 21) (name VREF+) (type power_in))
        (pin (num 22) (name VDDA) (type power_in))
        (pin (num 23) (name PA0) (type BiDi))
        (pin (num 24) (name PA1) (type BiDi))
        (pin (num 25) (name PA2) (type BiDi))
        (pin (num 26) (name PA3) (type BiDi))
        (pin (num 27) (name VSS) (type power_in))
        (pin (num 28) (name VDD) (type power_in))
        (pin (num 29) (name PA4) (type BiDi))
        (pin (num 30) (name PA5) (type BiDi))
        (pin (num 31) (name PA6) (type BiDi))
        (pin (num 32) (name PA7) (type BiDi))
        (pin (num 33) (name PC4) (type BiDi))
        (pin (num 34) (name PC5) (type BiDi))
        (pin (num 35) (name PB0) (type BiDi))
        (pin (num 36) (name PB1) (type BiDi))
        (pin (num 37) (name PB2) (type BiDi))
        (pin (num 38) (name PE7) (type BiDi))
        (pin (num 39) (name PE8) (type BiDi))
        (pin (num 40) (name PE9) (type BiDi))
        (pin (num 41) (name PE10) (type BiDi))
        (pin (num 42) (name PE11) (type BiDi))
        (pin (num 43) (name PE12) (type BiDi))
        (pin (num 44) (name PE13) (type BiDi))
        (pin (num 45) (name PE14) (type BiDi))
        (pin (num 46) (name PE15) (type BiDi))
        (pin (num 47) (name PB10) (type BiDi))
        (pin (num 48) (name PB11) (type BiDi))
        (pin (num 49) (name VCAP_1) (type power_in))
        (pin (num 50) (name VDD) (type power_in))
        (pin (num 51) (name PB12) (type BiDi))
        (pin (num 52) (name PB13) (type BiDi))
        (pin (num 53) (name PB14) (type BiDi))
        (pin (num 54) (name PB15) (type BiDi))
        (pin (num 55) (name PD8) (type BiDi))
        (pin (num 56) (name PD9) (type BiDi))
        (pin (num 57) (name PD10) (type BiDi))
        (pin (num 58) (name PD11) (type BiDi))
        (pin (num 59) (name PD12) (type BiDi))
        (pin (num 60) (name PD13) (type BiDi))
        (pin (num 61) (name PD14) (type BiDi))
        (pin (num 62) (name PD15) (type BiDi))
        (pin (num 63) (name PC6) (type BiDi))
        (pin (num 64) (name PC7) (type BiDi))
        (pin (num 65) (name PC8) (type BiDi))
        (pin (num 66) (name PC9) (type BiDi))
        (pin (num 67) (name PA8) (type BiDi))
        (pin (num 68) (name PA9) (type BiDi))
        (pin (num 69) (name PA10) (type BiDi))
        (pin (num 70) (name PA11) (type BiDi))
        (pin (num 71) (name PA12) (type BiDi))
        (pin (num 72) (name PA13) (type BiDi))
        (pin (num 73) (name VCAP_2) (type power_in))
        (pin (num 74) (name VSS) (type power_in))
        (pin (num 75) (name VDD) (type power_in))
        (pin (num 76) (name PA14) (type BiDi))
        (pin (num 77) (name PA15) (type BiDi))
        (pin (num 78) (name PC10) (type BiDi))
        (pin (num 79) (name PC11) (type BiDi))
        (pin (num 80) (name PC12) (type BiDi))
        (pin (num 81) (name PD0) (type BiDi))
        (pin (num 82) (name PD1) (type BiDi))
        (pin (num 83) (name PD2) (type BiDi))
        (pin (num 84) (name PD3) (type BiDi))
        (pin (num 85) (name PD4) (type BiDi))
        (pin (num 86) (name PD5) (type BiDi))
        (pin (num 87) (name PD6) (type BiDi))
        (pin (num 88) (name PD7) (type BiDi))
        (pin (num 89) (name PB3) (type BiDi))
        (pin (num 90) (name PB4) (type BiDi))
        (pin (num 91) (name PB5) (type BiDi))
        (pin (num 92) (name PB6) (type BiDi))
        (pin (num 93) (name PB7) (type BiDi))
        (pin (num 94) (name BOOT0) (type input))
        (pin (num 95) (name PB8) (type BiDi))
        (pin (num 96) (name PB9) (type BiDi))
        (pin (num 97) (name PE0) (type BiDi))
        (pin (num 98) (name PE1) (type BiDi))
        (pin (num 99) (name VSS) (type power_in))
        (pin (num 100) (name VDD) (type power_in))))
    (libpart (lib components) (part FE1.1s)
      (fields
        (field (name Reference) U)
        (field (name Value) FE1.1s))
      (pins
        (pin (num 1) (name VSS) (type input))
        (pin (num 2) (name XOUT) (type input))
        (pin (num 3) (name XIN) (type input))
        (pin (num 4) (name DM4) (type input))
        (pin (num 5) (name DP4) (type input))
        (pin (num 6) (name DM3) (type input))
        (pin (num 7) (name DP3) (type input))
        (pin (num 8) (name DM2) (type input))
        (pin (num 9) (name DP2) (type input))
        (pin (num 10) (name DM1) (type input))
        (pin (num 11) (name DP1) (type input))
        (pin (num 12) (name VD18_O) (type input))
        (pin (num 13) (name VD33) (type input))
        (pin (num 14) (name REXT) (type input))
        (pin (num 15) (name DMU) (type input))
        (pin (num 16) (name DPU) (type input))
        (pin (num 17) (name XRSTJ) (type input))
        (pin (num 18) (name VBUSM) (type input))
        (pin (num 19) (name BUSJ) (type input))
        (pin (num 20) (name VDD5) (type input))
        (pin (num 21) (name VDD33_O) (type input))
        (pin (num 22) (name DRV) (type input))
        (pin (num 23) (name LED1) (type input))
        (pin (num 24) (name LED2) (type input))
        (pin (num 25) (name PWRJ) (type input))
        (pin (num 26) (name OVCJ) (type input))
        (pin (num 27) (name TESTJ) (type input))
        (pin (num 28) (name VD18) (type input))))
    (libpart (lib conn) (part USB_A)
      (description "USB Type A connector")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_A))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name Shield) (type passive))))
    (libpart (lib device) (part Battery_Cell)
      (description "single battery cell")
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP_Small)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal_GND24_Small)
      (description "Two pin crystal, two ground/package pins (pin2 and 4) small symbol")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND24_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (footprints
        (fp LED*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part LED_Small)
      (description "LED, small symbol")
      (footprints
        (fp LED-*)
        (fp LED_*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part R_Pack04)
      (description "4 Resistor network, parallel topology, DIP package")
      (footprints
        (fp DIP*)
        (fp SOIC*))
      (fields
        (field (name Reference) RN)
        (field (name Value) R_Pack04))
      (pins
        (pin (num 1) (name R1.1) (type passive))
        (pin (num 2) (name R2.1) (type passive))
        (pin (num 3) (name R3.1) (type passive))
        (pin (num 4) (name R4.1) (type passive))
        (pin (num 5) (name R4.2) (type passive))
        (pin (num 6) (name R3.2) (type passive))
        (pin (num 7) (name R2.2) (type passive))
        (pin (num 8) (name R1.2) (type passive))))
    (libpart (lib device) (part R_Small)
      (description "Resistor, small symbol")
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Speaker_Crystal)
      (aliases
        (alias Speaker_Ultrasound))
      (description "crystal speaker/transducer")
      (fields
        (field (name Reference) LS)
        (field (name Value) Speaker_Crystal))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))))
    (libpart (lib regul) (part AP1117-15)
      (aliases
        (alias AP1117-18)
        (alias AP1117-25)
        (alias AP1117-33)
        (alias AP1117-50)
        (alias LD1117S33TR_SOT223)
        (alias LD1117S12TR_SOT223)
        (alias LD1117S18TR_SOT223)
        (alias LD1117S25TR_SOT223)
        (alias LD1117S50TR_SOT223)
        (alias NCP1117-12_SOT223)
        (alias NCP1117-1.5_SOT223)
        (alias NCP1117-1.8_SOT223)
        (alias NCP1117-2.0_SOT223)
        (alias NCP1117-2.5_SOT223)
        (alias NCP1117-2.85_SOT223)
        (alias NCP1117-3.3_SOT223)
        (alias NCP1117-5.0_SOT223))
      (description "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223")
      (docs http://www.diodes.com/datasheets/AP1117.pdf)
      (footprints
        (fp SOT?223*TabPin2*))
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117-15)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type passive))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib switches) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib transistors) (part BSS138)
      (aliases
        (alias 2N7002)
        (alias MMBF170))
      (description "50V Vds, 0.22 A Id, N-channel MOSFET, SOT-23")
      (docs https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BSS138)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT-23))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /home/user/ref/kicad-symbols/Connector.lib))
    (library (logical Connector_Generic)
      (uri /home/user/ref/kicad-symbols/Connector_Generic.lib))
    (library (logical Device)
      (uri /home/user/ref/kicad-symbols/Device.lib))
    (library (logical MCU_ST_STM32F1)
      (uri /home/user/ref/kicad-symbols/MCU_ST_STM32F1.lib))
    (library (logical MCU_ST_STM32F4)
      (uri /home/user/ref/kicad-symbols/MCU_ST_STM32F4.lib))
    (library (logical components)
      (uri /home/user/research/secureHID/pcb/components.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical regul)
      (uri /usr/share/kicad/library/regul.lib))
    (library (logical switches)
      (uri /usr/share/kicad/library/switches.lib))
    (library (logical transistors)
      (uri /usr/share/kicad/library/transistors.lib)))
  (nets
    (net (code 1) (name +3.3VA)
      (node (ref U2) (pin 48))
      (node (ref U5) (pin 2))
      (node (ref U2) (pin 9))
      (node (ref C33) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref U2) (pin 36))
      (node (ref U2) (pin 24))
      (node (ref U2) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref C35) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 2) (name /USBD_DM)
      (node (ref U2) (pin 32))
      (node (ref R9) (pin 2)))
    (net (code 3) (name /USBD_DP)
      (node (ref U2) (pin 33))
      (node (ref R7) (pin 1)))
    (net (code 4) (name GNDA)
      (node (ref C34) (pin 2))
      (node (ref J4) (pin 3))
      (node (ref TP83) (pin 1))
      (node (ref C33) (pin 2))
      (node (ref R26) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref J2) (pin 3))
      (node (ref J3) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref U2) (pin 44))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 47))
      (node (ref U2) (pin 35))
      (node (ref U2) (pin 23))
      (node (ref C35) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref C16) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref Y1) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref Y1) (pin 4))
      (node (ref C13) (pin 1)))
    (net (code 5) (name GND)
      (node (ref Y4) (pin 4))
      (node (ref Y4) (pin 2))
      (node (ref C30) (pin 1))
      (node (ref C21) (pin 2))
      (node (ref C23) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref C20) (pin 2))
      (node (ref R26) (pin 1))
      (node (ref Y3) (pin 3))
      (node (ref U4) (pin 27))
      (node (ref U4) (pin 1))
      (node (ref J8) (pin 5))
      (node (ref J8) (pin 4))
      (node (ref U4) (pin 19))
      (node (ref C29) (pin 2))
      (node (ref Q3) (pin 2))
      (node (ref Q2) (pin 3))
      (node (ref Y2) (pin 2))
      (node (ref C17) (pin 1))
      (node (ref C18) (pin 1))
      (node (ref R10) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref J7) (pin 7))
      (node (ref J7) (pin 8))
      (node (ref C1) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref U3) (pin 94))
      (node (ref BT1) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref Y2) (pin 4))
      (node (ref C9) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref J1) (pin 6))
      (node (ref J6) (pin 4))
      (node (ref J6) (pin 5))
      (node (ref J1) (pin 5))
      (node (ref U3) (pin 10))
      (node (ref U3) (pin 27))
      (node (ref U3) (pin 74))
      (node (ref U3) (pin 99))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C19) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref C27) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref C25) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref C26) (pin 1)))
    (net (code 6) (name "Net-(SW1-Pad2)")
      (node (ref U3) (pin 2))
      (node (ref SW1) (pin 2)))
    (net (code 7) (name "Net-(C16-Pad2)")
      (node (ref U2) (pin 6))
      (node (ref Y1) (pin 3))
      (node (ref C16) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 8) (name /DBGD_TX)
      (node (ref J5) (pin 4))
      (node (ref U2) (pin 30)))
    (net (code 9) (name "Net-(C13-Pad2)")
      (node (ref U2) (pin 5))
      (node (ref R4) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref C13) (pin 2)))
    (net (code 10) (name +3V3)
      (node (ref J2) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref U3) (pin 19))
      (node (ref R2) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref U3) (pin 75))
      (node (ref C6) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U3) (pin 28))
      (node (ref U3) (pin 11))
      (node (ref U3) (pin 100))
      (node (ref C1) (pin 1))
      (node (ref U3) (pin 50))
      (node (ref C2) (pin 1)))
    (net (code 11) (name "Net-(TP15-Pad1)")
      (node (ref U2) (pin 40))
      (node (ref TP15) (pin 1)))
    (net (code 12) (name "Net-(TP13-Pad1)")
      (node (ref TP13) (pin 1))
      (node (ref U2) (pin 39)))
    (net (code 13) (name "Net-(TP12-Pad1)")
      (node (ref U2) (pin 20))
      (node (ref TP12) (pin 1)))
    (net (code 14) (name "Net-(TP10-Pad1)")
      (node (ref U2) (pin 19))
      (node (ref TP10) (pin 1)))
    (net (code 15) (name "Net-(TP8-Pad1)")
      (node (ref U2) (pin 18))
      (node (ref TP8) (pin 1)))
    (net (code 16) (name /SWCLKD)
      (node (ref U2) (pin 37))
      (node (ref J4) (pin 2)))
    (net (code 17) (name /SWDIOD)
      (node (ref U2) (pin 34))
      (node (ref J4) (pin 4)))
    (net (code 18) (name "Net-(TP17-Pad1)")
      (node (ref TP17) (pin 1))
      (node (ref U2) (pin 41)))
    (net (code 19) (name "Net-(TP44-Pad1)")
      (node (ref TP44) (pin 1))
      (node (ref U2) (pin 28)))
    (net (code 20) (name "Net-(TP30-Pad1)")
      (node (ref TP30) (pin 1))
      (node (ref U2) (pin 29)))
    (net (code 21) (name "Net-(TP26-Pad1)")
      (node (ref TP26) (pin 1))
      (node (ref U2) (pin 17)))
    (net (code 22) (name "Net-(TP22-Pad1)")
      (node (ref U2) (pin 16))
      (node (ref TP22) (pin 1)))
    (net (code 23) (name "Net-(TP18-Pad1)")
      (node (ref U2) (pin 15))
      (node (ref TP18) (pin 1)))
    (net (code 24) (name "Net-(TP16-Pad1)")
      (node (ref TP16) (pin 1))
      (node (ref U2) (pin 14)))
    (net (code 25) (name "Net-(TP11-Pad1)")
      (node (ref TP11) (pin 1))
      (node (ref U2) (pin 11)))
    (net (code 26) (name "Net-(TP9-Pad1)")
      (node (ref U2) (pin 10))
      (node (ref TP9) (pin 1)))
    (net (code 27) (name "Net-(TP4-Pad1)")
      (node (ref U2) (pin 2))
      (node (ref TP4) (pin 1)))
    (net (code 28) (name "Net-(TP6-Pad1)")
      (node (ref U2) (pin 3))
      (node (ref TP6) (pin 1)))
    (net (code 29) (name "Net-(TP7-Pad1)")
      (node (ref U2) (pin 4))
      (node (ref TP7) (pin 1)))
    (net (code 30) (name "Net-(TP42-Pad1)")
      (node (ref U2) (pin 27))
      (node (ref TP42) (pin 1)))
    (net (code 31) (name "Net-(TP40-Pad1)")
      (node (ref U2) (pin 26))
      (node (ref TP40) (pin 1)))
    (net (code 32) (name "Net-(TP38-Pad1)")
      (node (ref U2) (pin 25))
      (node (ref TP38) (pin 1)))
    (net (code 33) (name "Net-(TP36-Pad1)")
      (node (ref U2) (pin 22))
      (node (ref TP36) (pin 1)))
    (net (code 34) (name "Net-(TP34-Pad1)")
      (node (ref U2) (pin 21))
      (node (ref TP34) (pin 1)))
    (net (code 35) (name "Net-(TP32-Pad1)")
      (node (ref TP32) (pin 1))
      (node (ref U2) (pin 46)))
    (net (code 36) (name "Net-(TP29-Pad1)")
      (node (ref U2) (pin 45))
      (node (ref TP29) (pin 1)))
    (net (code 37) (name "Net-(TP25-Pad1)")
      (node (ref U2) (pin 43))
      (node (ref TP25) (pin 1)))
    (net (code 38) (name "Net-(TP21-Pad1)")
      (node (ref U2) (pin 42))
      (node (ref TP21) (pin 1)))
    (net (code 39) (name "Net-(C19-Pad2)")
      (node (ref U3) (pin 8))
      (node (ref Y3) (pin 1))
      (node (ref C19) (pin 2)))
    (net (code 40) (name /SECURE_IF_F4TX)
      (node (ref U2) (pin 13))
      (node (ref U3) (pin 25))
      (node (ref TP82) (pin 1)))
    (net (code 41) (name /SECURE_IF_F4RX)
      (node (ref U2) (pin 12))
      (node (ref TP81) (pin 1))
      (node (ref U3) (pin 26)))
    (net (code 42) (name /DBGD_RX)
      (node (ref J5) (pin 3))
      (node (ref U2) (pin 31)))
    (net (code 43) (name "Net-(R3-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref U2) (pin 7)))
    (net (code 44) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U3) (pin 14)))
    (net (code 45) (name "Net-(D18-Pad1)")
      (node (ref D18) (pin 1))
      (node (ref RN2) (pin 2)))
    (net (code 46) (name "Net-(D16-Pad1)")
      (node (ref RN1) (pin 4))
      (node (ref D16) (pin 1)))
    (net (code 47) (name "Net-(D3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref RN1) (pin 3)))
    (net (code 48) (name "Net-(D1-Pad1)")
      (node (ref RN1) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 49) (name "Net-(D2-Pad1)")
      (node (ref RN1) (pin 2))
      (node (ref D2) (pin 1)))
    (net (code 50) (name "Net-(D22-Pad1)")
      (node (ref RN3) (pin 2))
      (node (ref D22) (pin 1)))
    (net (code 51) (name "Net-(D20-Pad1)")
      (node (ref RN2) (pin 4))
      (node (ref D20) (pin 1)))
    (net (code 52) (name /PIEZO_OUT)
      (node (ref U3) (pin 47))
      (node (ref R25) (pin 1)))
    (net (code 53) (name "Net-(C29-Pad1)")
      (node (ref R25) (pin 2))
      (node (ref Q3) (pin 1))
      (node (ref C29) (pin 1)))
    (net (code 54) (name VBUS)
      (node (ref LS1) (pin 2))
      (node (ref J3) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref J6) (pin 1))
      (node (ref J7) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref J5) (pin 1))
      (node (ref D11) (pin 2))
      (node (ref D12) (pin 2))
      (node (ref D13) (pin 2))
      (node (ref U4) (pin 18))
      (node (ref D15) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref D6) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref D14) (pin 2))
      (node (ref D10) (pin 2))
      (node (ref J8) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref U5) (pin 3))
      (node (ref C32) (pin 1))
      (node (ref R24) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref D9) (pin 2))
      (node (ref U4) (pin 20))
      (node (ref D2) (pin 2))
      (node (ref J7) (pin 1))
      (node (ref D24) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref D23) (pin 2))
      (node (ref D21) (pin 2))
      (node (ref D18) (pin 2))
      (node (ref D20) (pin 2))
      (node (ref D19) (pin 2))
      (node (ref D17) (pin 2))
      (node (ref D22) (pin 2))
      (node (ref D16) (pin 2))
      (node (ref D3) (pin 2)))
    (net (code 55) (name /LED0)
      (node (ref RN1) (pin 8))
      (node (ref U3) (pin 3)))
    (net (code 56) (name /LED3)
      (node (ref U3) (pin 38))
      (node (ref RN1) (pin 5)))
    (net (code 57) (name /LED2)
      (node (ref RN1) (pin 6))
      (node (ref U3) (pin 5)))
    (net (code 58) (name /LED1)
      (node (ref RN1) (pin 7))
      (node (ref U3) (pin 4)))
    (net (code 59) (name /LED7)
      (node (ref RN2) (pin 5))
      (node (ref U3) (pin 42)))
    (net (code 60) (name /LED9)
      (node (ref RN3) (pin 7))
      (node (ref U3) (pin 44)))
    (net (code 61) (name /LED10)
      (node (ref RN3) (pin 6))
      (node (ref U3) (pin 45)))
    (net (code 62) (name /LED11)
      (node (ref U3) (pin 46))
      (node (ref RN3) (pin 5)))
    (net (code 63) (name "Net-(D24-Pad1)")
      (node (ref RN3) (pin 4))
      (node (ref D24) (pin 1)))
    (net (code 64) (name "Net-(D23-Pad1)")
      (node (ref D23) (pin 1))
      (node (ref RN3) (pin 3)))
    (net (code 65) (name "Net-(D21-Pad1)")
      (node (ref D21) (pin 1))
      (node (ref RN3) (pin 1)))
    (net (code 66) (name /LED4)
      (node (ref RN2) (pin 8))
      (node (ref U3) (pin 39)))
    (net (code 67) (name /LED5)
      (node (ref RN2) (pin 7))
      (node (ref U3) (pin 40)))
    (net (code 68) (name /LED6)
      (node (ref RN2) (pin 6))
      (node (ref U3) (pin 41)))
    (net (code 69) (name /LED8)
      (node (ref RN3) (pin 8))
      (node (ref U3) (pin 43)))
    (net (code 70) (name "Net-(D19-Pad1)")
      (node (ref D19) (pin 1))
      (node (ref RN2) (pin 3)))
    (net (code 71) (name "Net-(D17-Pad1)")
      (node (ref D17) (pin 1))
      (node (ref RN2) (pin 1)))
    (net (code 72) (name "Net-(TP45-Pad1)")
      (node (ref TP45) (pin 1))
      (node (ref U2) (pin 38)))
    (net (code 73) (name "Net-(Q2-Pad2)")
      (node (ref R22) (pin 2))
      (node (ref R23) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref R18) (pin 2))
      (node (ref Q2) (pin 2)))
    (net (code 74) (name "Net-(Q1-Pad3)")
      (node (ref R14) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref Q1) (pin 3))
      (node (ref R12) (pin 2))
      (node (ref R13) (pin 2)))
    (net (code 75) (name "Net-(D6-Pad1)")
      (node (ref D6) (pin 1))
      (node (ref R14) (pin 1)))
    (net (code 76) (name "Net-(D5-Pad1)")
      (node (ref D5) (pin 1))
      (node (ref R13) (pin 1)))
    (net (code 77) (name "Net-(D15-Pad1)")
      (node (ref D15) (pin 1))
      (node (ref R23) (pin 1)))
    (net (code 78) (name "Net-(D14-Pad1)")
      (node (ref D14) (pin 1))
      (node (ref R22) (pin 1)))
    (net (code 79) (name "Net-(D13-Pad1)")
      (node (ref R21) (pin 1))
      (node (ref D13) (pin 1)))
    (net (code 80) (name "Net-(D12-Pad1)")
      (node (ref R20) (pin 1))
      (node (ref D12) (pin 1)))
    (net (code 81) (name "Net-(D11-Pad1)")
      (node (ref D11) (pin 1))
      (node (ref R19) (pin 1)))
    (net (code 82) (name "Net-(C22-Pad2)")
      (node (ref U3) (pin 9))
      (node (ref Y3) (pin 2))
      (node (ref C22) (pin 2)))
    (net (code 83) (name "Net-(TP3-Pad1)")
      (node (ref U3) (pin 29))
      (node (ref TP3) (pin 1)))
    (net (code 84) (name "Net-(TP49-Pad1)")
      (node (ref U3) (pin 53))
      (node (ref TP49) (pin 1)))
    (net (code 85) (name "Net-(TP48-Pad1)")
      (node (ref TP48) (pin 1))
      (node (ref U3) (pin 52)))
    (net (code 86) (name "Net-(TP47-Pad1)")
      (node (ref TP47) (pin 1))
      (node (ref U3) (pin 51)))
    (net (code 87) (name "Net-(TP46-Pad1)")
      (node (ref U3) (pin 48))
      (node (ref TP46) (pin 1)))
    (net (code 88) (name "Net-(TP1-Pad1)")
      (node (ref TP1) (pin 1))
      (node (ref U3) (pin 23)))
    (net (code 89) (name "Net-(TP2-Pad1)")
      (node (ref U3) (pin 24))
      (node (ref TP2) (pin 1)))
    (net (code 90) (name "Net-(TP50-Pad1)")
      (node (ref TP50) (pin 1))
      (node (ref U3) (pin 54)))
    (net (code 91) (name "Net-(TP5-Pad1)")
      (node (ref U3) (pin 67))
      (node (ref TP5) (pin 1)))
    (net (code 92) (name "Net-(TP14-Pad1)")
      (node (ref TP14) (pin 1))
      (node (ref U3) (pin 77)))
    (net (code 93) (name "Net-(TP24-Pad1)")
      (node (ref TP24) (pin 1))
      (node (ref U3) (pin 36)))
    (net (code 94) (name "Net-(TP28-Pad1)")
      (node (ref TP28) (pin 1))
      (node (ref U3) (pin 37)))
    (net (code 95) (name "Net-(TP31-Pad1)")
      (node (ref U3) (pin 89))
      (node (ref TP31) (pin 1)))
    (net (code 96) (name "Net-(TP33-Pad1)")
      (node (ref TP33) (pin 1))
      (node (ref U3) (pin 90)))
    (net (code 97) (name "Net-(TP35-Pad1)")
      (node (ref U3) (pin 91))
      (node (ref TP35) (pin 1)))
    (net (code 98) (name "Net-(TP60-Pad1)")
      (node (ref U3) (pin 33))
      (node (ref TP60) (pin 1)))
    (net (code 99) (name "Net-(TP70-Pad1)")
      (node (ref TP70) (pin 1))
      (node (ref U3) (pin 66)))
    (net (code 100) (name "Net-(TP68-Pad1)")
      (node (ref TP68) (pin 1))
      (node (ref U3) (pin 65)))
    (net (code 101) (name "Net-(TP66-Pad1)")
      (node (ref U3) (pin 64))
      (node (ref TP66) (pin 1)))
    (net (code 102) (name "Net-(TP64-Pad1)")
      (node (ref U3) (pin 63))
      (node (ref TP64) (pin 1)))
    (net (code 103) (name "Net-(TP62-Pad1)")
      (node (ref TP62) (pin 1))
      (node (ref U3) (pin 34)))
    (net (code 104) (name "Net-(TP54-Pad1)")
      (node (ref TP54) (pin 1))
      (node (ref U3) (pin 16)))
    (net (code 105) (name "Net-(TP56-Pad1)")
      (node (ref TP56) (pin 1))
      (node (ref U3) (pin 17)))
    (net (code 106) (name "Net-(TP58-Pad1)")
      (node (ref TP58) (pin 1))
      (node (ref U3) (pin 18)))
    (net (code 107) (name "Net-(TP37-Pad1)")
      (node (ref U3) (pin 92))
      (node (ref TP37) (pin 1)))
    (net (code 108) (name "Net-(TP52-Pad1)")
      (node (ref TP52) (pin 1))
      (node (ref U3) (pin 15)))
    (net (code 109) (name "Net-(TP39-Pad1)")
      (node (ref U3) (pin 93))
      (node (ref TP39) (pin 1)))
    (net (code 110) (name "Net-(TP41-Pad1)")
      (node (ref TP41) (pin 1))
      (node (ref U3) (pin 95)))
    (net (code 111) (name "Net-(TP43-Pad1)")
      (node (ref U3) (pin 96))
      (node (ref TP43) (pin 1)))
    (net (code 112) (name "Net-(TP20-Pad1)")
      (node (ref TP20) (pin 1))
      (node (ref U3) (pin 35)))
    (net (code 113) (name "Net-(TP19-Pad1)")
      (node (ref TP19) (pin 1))
      (node (ref U3) (pin 97)))
    (net (code 114) (name "Net-(TP23-Pad1)")
      (node (ref TP23) (pin 1))
      (node (ref U3) (pin 98)))
    (net (code 115) (name "Net-(TP27-Pad1)")
      (node (ref TP27) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 116) (name "Net-(TP79-Pad1)")
      (node (ref TP79) (pin 1))
      (node (ref U3) (pin 61)))
    (net (code 117) (name "Net-(TP80-Pad1)")
      (node (ref TP80) (pin 1))
      (node (ref U3) (pin 62)))
    (net (code 118) (name "Net-(TP76-Pad1)")
      (node (ref TP76) (pin 1))
      (node (ref U3) (pin 80)))
    (net (code 119) (name "Net-(TP57-Pad1)")
      (node (ref TP57) (pin 1))
      (node (ref U3) (pin 84)))
    (net (code 120) (name "Net-(TP59-Pad1)")
      (node (ref TP59) (pin 1))
      (node (ref U3) (pin 85)))
    (net (code 121) (name "Net-(TP55-Pad1)")
      (node (ref TP55) (pin 1))
      (node (ref U3) (pin 83)))
    (net (code 122) (name "Net-(TP53-Pad1)")
      (node (ref TP53) (pin 1))
      (node (ref U3) (pin 82)))
    (net (code 123) (name "Net-(TP51-Pad1)")
      (node (ref TP51) (pin 1))
      (node (ref U3) (pin 81)))
    (net (code 124) (name "Net-(TP74-Pad1)")
      (node (ref U3) (pin 79))
      (node (ref TP74) (pin 1)))
    (net (code 125) (name "Net-(TP78-Pad1)")
      (node (ref U3) (pin 7))
      (node (ref TP78) (pin 1)))
    (net (code 126) (name "Net-(TP72-Pad1)")
      (node (ref TP72) (pin 1))
      (node (ref U3) (pin 78)))
    (net (code 127) (name "Net-(TP65-Pad1)")
      (node (ref U3) (pin 88))
      (node (ref TP65) (pin 1)))
    (net (code 128) (name "Net-(TP73-Pad1)")
      (node (ref U3) (pin 58))
      (node (ref TP73) (pin 1)))
    (net (code 129) (name "Net-(TP75-Pad1)")
      (node (ref U3) (pin 59))
      (node (ref TP75) (pin 1)))
    (net (code 130) (name "Net-(TP77-Pad1)")
      (node (ref TP77) (pin 1))
      (node (ref U3) (pin 60)))
    (net (code 131) (name "Net-(TP71-Pad1)")
      (node (ref TP71) (pin 1))
      (node (ref U3) (pin 57)))
    (net (code 132) (name "Net-(TP63-Pad1)")
      (node (ref TP63) (pin 1))
      (node (ref U3) (pin 87)))
    (net (code 133) (name "Net-(TP67-Pad1)")
      (node (ref U3) (pin 55))
      (node (ref TP67) (pin 1)))
    (net (code 134) (name "Net-(TP69-Pad1)")
      (node (ref TP69) (pin 1))
      (node (ref U3) (pin 56)))
    (net (code 135) (name "Net-(TP61-Pad1)")
      (node (ref U3) (pin 86))
      (node (ref TP61) (pin 1)))
    (net (code 136) (name /HUB_NRST)
      (node (ref C30) (pin 2))
      (node (ref U3) (pin 30))
      (node (ref R11) (pin 1))
      (node (ref U4) (pin 17)))
    (net (code 137) (name /DBGH_RX)
      (node (ref U3) (pin 69))
      (node (ref J3) (pin 3)))
    (net (code 138) (name "Net-(C15-Pad1)")
      (node (ref C15) (pin 1))
      (node (ref U3) (pin 73)))
    (net (code 139) (name "Net-(C14-Pad1)")
      (node (ref C14) (pin 1))
      (node (ref U3) (pin 49)))
    (net (code 140) (name VSSA)
      (node (ref C8) (pin 2))
      (node (ref U3) (pin 20))
      (node (ref C7) (pin 1)))
    (net (code 141) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref U3) (pin 21)))
    (net (code 142) (name VDDA)
      (node (ref R1) (pin 2))
      (node (ref U3) (pin 22))
      (node (ref C7) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref C8) (pin 1)))
    (net (code 143) (name "Net-(BT1-Pad1)")
      (node (ref U3) (pin 6))
      (node (ref BT1) (pin 1)))
    (net (code 144) (name "Net-(C18-Pad2)")
      (node (ref Y2) (pin 3))
      (node (ref R8) (pin 2))
      (node (ref U3) (pin 13))
      (node (ref C18) (pin 2)))
    (net (code 145) (name /DBGH_TX)
      (node (ref J3) (pin 4))
      (node (ref U3) (pin 68)))
    (net (code 146) (name "Net-(J6-Pad3)")
      (node (ref J6) (pin 3))
      (node (ref U4) (pin 11)))
    (net (code 147) (name "Net-(J6-Pad2)")
      (node (ref U4) (pin 10))
      (node (ref J6) (pin 2)))
    (net (code 148) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 149) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref R9) (pin 1)))
    (net (code 150) (name "Net-(C17-Pad2)")
      (node (ref U3) (pin 12))
      (node (ref Y2) (pin 1))
      (node (ref C17) (pin 2))
      (node (ref R8) (pin 1)))
    (net (code 151) (name "Net-(J1-Pad3)")
      (node (ref R7) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref J1) (pin 3)))
    (net (code 152) (name /USBH_DM)
      (node (ref U3) (pin 70))
      (node (ref U4) (pin 15)))
    (net (code 153) (name "Net-(J7-Pad10)")
      (node (ref J7) (pin 10)))
    (net (code 154) (name "Net-(J7-Pad9)")
      (node (ref J7) (pin 9)))
    (net (code 155) (name "Net-(J7-Pad6)")
      (node (ref U4) (pin 5))
      (node (ref J7) (pin 6)))
    (net (code 156) (name "Net-(J7-Pad5)")
      (node (ref J7) (pin 5))
      (node (ref U4) (pin 7)))
    (net (code 157) (name /ALARM_LED_BLUE)
      (node (ref Q1) (pin 1))
      (node (ref U3) (pin 31)))
    (net (code 158) (name "Net-(LS1-Pad1)")
      (node (ref Q3) (pin 3))
      (node (ref LS1) (pin 1))
      (node (ref R24) (pin 2)))
    (net (code 159) (name "Net-(J7-Pad4)")
      (node (ref J7) (pin 4))
      (node (ref U4) (pin 4)))
    (net (code 160) (name "Net-(J7-Pad3)")
      (node (ref J7) (pin 3))
      (node (ref U4) (pin 6)))
    (net (code 161) (name "Net-(C20-Pad1)")
      (node (ref U4) (pin 2))
      (node (ref Y4) (pin 1))
      (node (ref C20) (pin 1)))
    (net (code 162) (name "Net-(R10-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref U4) (pin 14)))
    (net (code 163) (name "Net-(C21-Pad1)")
      (node (ref Y4) (pin 3))
      (node (ref C21) (pin 1))
      (node (ref U4) (pin 3)))
    (net (code 164) (name /3V3_HUB)
      (node (ref C23) (pin 2))
      (node (ref U4) (pin 21))
      (node (ref R11) (pin 2))
      (node (ref U4) (pin 26))
      (node (ref U4) (pin 13)))
    (net (code 165) (name "Net-(U4-Pad25)")
      (node (ref U4) (pin 25)))
    (net (code 166) (name /ALARM_LED_PINK)
      (node (ref Q2) (pin 1))
      (node (ref U3) (pin 32)))
    (net (code 167) (name "Net-(D10-Pad1)")
      (node (ref R18) (pin 1))
      (node (ref D10) (pin 1)))
    (net (code 168) (name "Net-(D7-Pad1)")
      (node (ref R15) (pin 1))
      (node (ref D7) (pin 1)))
    (net (code 169) (name "Net-(D4-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 170) (name "Net-(D9-Pad1)")
      (node (ref R17) (pin 1))
      (node (ref D9) (pin 1)))
    (net (code 171) (name "Net-(D8-Pad1)")
      (node (ref D8) (pin 1))
      (node (ref R16) (pin 1)))
    (net (code 172) (name /SWDIOH)
      (node (ref J2) (pin 4))
      (node (ref U3) (pin 72)))
    (net (code 173) (name /SWCLKH)
      (node (ref J2) (pin 2))
      (node (ref U3) (pin 76)))
    (net (code 174) (name "Net-(C24-Pad2)")
      (node (ref U4) (pin 28))
      (node (ref C24) (pin 2))
      (node (ref U4) (pin 12)))
    (net (code 175) (name "Net-(J8-Pad2)")
      (node (ref J8) (pin 2))
      (node (ref U4) (pin 8)))
    (net (code 176) (name "Net-(J8-Pad3)")
      (node (ref J8) (pin 3))
      (node (ref U4) (pin 9)))
    (net (code 177) (name "Net-(U4-Pad24)")
      (node (ref U4) (pin 24)))
    (net (code 178) (name "Net-(U4-Pad23)")
      (node (ref U4) (pin 23)))
    (net (code 179) (name "Net-(U4-Pad22)")
      (node (ref U4) (pin 22)))
    (net (code 180) (name /USBH_DP)
      (node (ref U3) (pin 71))
      (node (ref U4) (pin 16)))))