(footprint "mesh_conn" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "REF**" (at 0 -2.25 0 unlocked) (layer "F.SilkS") hide (tstamp ad4f86a6-c40a-45de-9755-536816782561)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "mesh_conn" (at 0 1 0 unlocked) (layer "F.Fab") (tstamp e87da325-b358-40c2-9a7c-2bf2cb54bc3f)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 1a4151b5-9c45-483f-b7de-b3c48b0e0373)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 3a2afd89-4c34-4a0b-a3cc-24800fe97f31)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 5f1f1696-4799-4134-b64d-57be44267fde)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_text user "${REFERENCE}" (at 0 2.5 0 unlocked) (layer "F.Fab") (tstamp f741b3b8-fc10-442d-8f89-4dd2860f992f)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd circle (at 0 -0.45) (size 0.15 0.15) (layers "F.Cu")
    (tstamp e65c026b-a582-481d-aa0f-83da4e05e52b)
  )
  (pad "2" smd circle (at 0 -0.15) (size 0.15 0.15) (layers "F.Cu")
    (tstamp 4adac25c-6de4-4cdf-b81d-79aadd631463)
  )
  (pad "3" smd circle (at 0 0.15) (size 0.15 0.15) (layers "F.Cu")
    (tstamp 80b9cf1e-76d6-499a-8d4a-c27e4b29a23a)
  )
  (pad "4" smd circle (at 0 0.45) (size 0.15 0.15) (layers "F.Cu")
    (tstamp 6911242a-667c-4407-8e79-6ac9c5f4704c)
  )
)
