(footprint "P16612-011CA" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "REF**" (at 0 -2.55 0 unlocked) (layer "F.SilkS") (tstamp c2276d27-16d8-4ad4-8bde-592813a4d3a8)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "P16612-011CA" (at 0 1 0 unlocked) (layer "F.Fab") (tstamp c17f9354-4dcd-427f-a0cd-3651420b79cd)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 65b5b503-94ba-469f-ac07-825c708743d5)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp c4b71734-68fe-44c7-a657-275085e813a7)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 4907b044-9154-4565-bbc3-4d78188ae664)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_line (start 0.75 -1.75) (end 1.8 -1.75)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 5bc9e9b8-c81f-4e2f-aeda-6038318a1525))
  (fp_line (start 1.8 -1.75) (end 1.8 -0.8)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp ef59ca4e-da2f-41c0-8fee-f72ca0a547ee))
  (fp_rect (start -1.3 -1.3) (end 1.3 1.3)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp d519c4bb-87d6-401d-8dfe-10740fe38960))
  (fp_rect (start -1.5 -1.5) (end 1.5 1.5)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 9e7fce77-0bdc-4c75-b86e-4d88362275b0))
  (fp_text user "${REFERENCE}" (at 0 2.5 0 unlocked) (layer "F.Fab") (tstamp 76855fc3-1cfc-4e28-b002-8380fdafa654)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd rect (at 0.9 0 180) (size 1.3 3.1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 3198d885-b53d-4ffb-96b6-184c86fac519)
  )
  (pad "2" smd rect (at -0.9 0 180) (size 1.3 3.1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp 7295e3bf-5769-43de-a2ad-24d6cd74bcf1)
  )
)
