(footprint "VBPW34S" (version 20230620) (generator pcbnew)
  (layer "F.Cu")
  (property "Reference" "REF**" (at -1.6 -3 0 unlocked) (layer "F.SilkS") hide (tstamp 88390548-67d9-49ae-8e4c-db01d26978d2)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (property "Value" "VBPW34S" (at 0 1 0 unlocked) (layer "F.Fab") (tstamp 49bcfcc7-6ef0-4846-b5f7-960c636434bb)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp db2c230f-92ec-4075-9bd3-c08c516cad56)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp f9c53b5c-993a-4b69-8b9e-da34f17dd77b)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide (tstamp 4e42c3fd-b0f8-4932-8240-d6c55ea8e994)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (attr smd)
  (fp_line (start -1.6 -1.95) (end -1.6 1.95)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp a2f763ed-a004-441d-8244-eac6029b573e))
  (fp_rect (start -2.2 -1.95) (end 2.2 1.95)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 13d36aea-793c-41ad-904d-3542d7f1a2c4))
  (fp_rect (start -1 -1) (end 1 1)
    (stroke (width 0.1) (type dot)) (fill none) (layer "F.SilkS") (tstamp 93cc726b-eb93-4c74-875e-19bac486e589))
  (fp_rect (start -3.4 -2.2) (end 3.4 2.2)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 35a10b49-2333-4ae0-ad4f-be7c11e460a8))
  (fp_text user "${REFERENCE}" (at 0 2.5 0 unlocked) (layer "F.Fab") (tstamp 6da511a8-5272-4940-a236-8bdcca2bcba5)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd rect (at -3.575 0 90) (size 1.75 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp c26b90cf-eb56-4095-b993-a534163b7718)
  )
  (pad "2" smd rect (at 3.575 0 90) (size 1.75 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45)
    (tstamp e1b9bf11-3775-4900-ad1e-6eb4ef74afc1)
  )
)
